================================================================================
                               ama3bevb_pwm_example
================================================================================


Copyright (C) 2013-2019, Fujitsu Electronics Europe GmbH or a               
subsidiary of Fujitsu Electronics Europe GmbH.  All rights reserved.        
                                                                            
This software, including source code, documentation and related             
materials ("Software"), is owned by Fujitsu Electronics Europe GmbH or      
one of its subsidiaries ("Fujitsu").
                                                                            
If no EULA applies, Fujitsu hereby grants you a personal, non-exclusive,    
non-transferable license to copy, modify, and compile the                   
Software source code solely for use in connection with Fujitsu's            
integrated circuit products.  Any reproduction, modification, translation,  
compilation, or representation of this Software except as specified         
above is prohibited without the express written permission of Fujitsu.      
                                                                            
Disclaimer: THIS SOFTWARE IS PROVIDED AS-IS, WITH NO                        
WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING,                        
BUT NOT LIMITED TO, NONINFRINGEMENT, IMPLIED                                
WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A                             
PARTICULAR PURPOSE. Fujitsu reserves the right to make                      
changes to the Software without notice. Fujitsu does not assume any         
liability arising out of the application or use of the Software or any      
product or circuit described in the Software. Fujitsu does not              
authorize its products for use in any products where a malfunction or       
failure of the Fujitsu product may reasonably be expected to result in      
significant property damage, injury or death ("High Risk Product"). By      
including Fujitsu's product in a High Risk Product, the manufacturer        
of such system or application assumes all risk of such use and in doing     
so agrees to indemnify Fujitsu against all liability.                       


================================================================================
History
** Date        Ver       Initials          Description
**   - 2019-03-21  V1.0  LEh             First Version
**   - 2019-08-30  V1.1  MSc             Startup for IAR corrected

Supported toolchain versions


ARM        5.11
IAR        7.30
iSYSTEM    9.12.213
Segger     4.1
================================================================================

This is an example project for Ambiq Micro Apollo3Blue, demonstrating the use of the
Counter/Timer module with PWM and an interrupt service routine to update the duty
cycle. The Counter/Timer module is using GPIO30 for output which is the CT11 timer output 
(LED D8 on evaluation board).

The duty cycle will be changed in periodically resulting in a fading LED.

================================================================================

================================================================================ 
EOF (not truncated) 
================================================================================ 
 
