| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_ppg_int_sel Struct Reference
Base Timer (BT)

structure to select the PPG interrupt More...

`#include <bt.h>`

## Data Fields
boolean_t | bPpgTrigInt
| PPG trigger interrupt selection.
boolean_t | bPpgUnderflowInt
| PPG underflow interrupt selection.

## Detailed Description

structure to select the PPG interrupt

Definition at line 610 of file bt.h.

## Field Documentation

boolean_t bPpgTrigInt

PPG trigger interrupt selection.

Definition at line 612 of file bt.h.

Referenced by Bt_Ppg_DisableInt(), and Bt_Ppg_EnableInt().

boolean_t bPpgUnderflowInt

PPG underflow interrupt selection.

Definition at line 613 of file bt.h.

Referenced by Bt_Ppg_DisableInt(), and Bt_Ppg_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h