| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_pwm_int_cb Struct Reference
Base Timer (BT)

structure to set the PWM interrupt callback function More...

`#include <bt.h>`

## Data Fields
func_ptr_t | pfnPwmTrigIntCallback
| Pointer to trigger interrupt callback function.
func_ptr_t | pfnPwmDutyMatchIntCallback
| Pointer to duty match interrupt callback function.
func_ptr_t | pfnPwmUnderflowIntCallback
| Pointer to underflow interrupt callback function.

## Detailed Description

structure to set the PWM interrupt callback function

Definition at line 495 of file bt.h.

## Field Documentation

func_ptr_t pfnPwmDutyMatchIntCallback

Pointer to duty match interrupt callback function.

Definition at line 498 of file bt.h.

Referenced by Bt_Pwm_EnableInt().

func_ptr_t pfnPwmTrigIntCallback

Pointer to trigger interrupt callback function.

Definition at line 497 of file bt.h.

Referenced by Bt_Pwm_EnableInt().

func_ptr_t pfnPwmUnderflowIntCallback

Pointer to underflow interrupt callback function.

Definition at line 499 of file bt.h.

Referenced by Bt_Pwm_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h