| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_wfg_ctrl_bits Struct Reference
Waveform Generator (WFG)

`#include <mft_wfg.h>`

## Data Fields
en_gten_bits_t | enGtenBits
| select the output condition
en_psel_bits_t | enPselBits
| select the PPG timer unit
en_pgen_bits_t | enPgenBits
| how to reflect the CH_PPG signal
en_dmod_bit_t | enDmodBit
| polarity for RTO0 and RTO1 signal output

## Detailed Description

Definition at line 388 of file mft_wfg.h.

## Field Documentation

en_dmod_bit_t enDmodBit

polarity for RTO0 and RTO1 signal output

Definition at line 393 of file mft_wfg.h.

Referenced by Mft_Wfg_ConfigCtrlBits().

en_gten_bits_t enGtenBits

select the output condition

Definition at line 390 of file mft_wfg.h.

Referenced by Mft_Wfg_ConfigCtrlBits().

en_pgen_bits_t enPgenBits

how to reflect the CH_PPG signal

Definition at line 392 of file mft_wfg.h.

Referenced by Mft_Wfg_ConfigCtrlBits().

en_psel_bits_t enPselBits

select the PPG timer unit

Definition at line 391 of file mft_wfg.h.

Referenced by Mft_Wfg_ConfigCtrlBits().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mft/mft_wfg.h