| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_uart_int_sel Struct Reference
Multi Function Serial Interface (MFS)

UART interrupt selection. More...

`#include <mfs.h>`

## Data Fields
boolean_t | bTxInt
| UART TX interrupt.
boolean_t | bRxInt
| UART RX interrupt.
boolean_t | bTxIdle
| UART TX idle interrupt.
boolean_t | bTxFifoInt
| UART TX FIFO interrupt.

## Detailed Description

UART interrupt selection.

Definition at line 528 of file mfs.h.

## Field Documentation

boolean_t bRxInt

UART RX interrupt.

Definition at line 531 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), and Mfs_Uart_EnableInt().

boolean_t bTxFifoInt

UART TX FIFO interrupt.

Definition at line 533 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), and Mfs_Uart_EnableInt().

boolean_t bTxIdle

UART TX idle interrupt.

Definition at line 532 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), and Mfs_Uart_EnableInt().

boolean_t bTxInt

UART TX interrupt.

Definition at line 530 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), and Mfs_Uart_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h