| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_dma_int_sel Struct Reference
Direct Memory Access (DMA)

DMA interrupt selection. More...

`#include <dma.h>`

## Data Fields
boolean_t | bCompleteInt
| Select DMA transfer completion interrupt.
boolean_t | bErrorInt
| Select DMA transfer error interrupt.

## Detailed Description

DMA interrupt selection.

Definition at line 192 of file dma.h.

## Field Documentation

boolean_t bCompleteInt

Select DMA transfer completion interrupt.

Definition at line 194 of file dma.h.

Referenced by Dma_DisableInt(), and Dma_EnableInt().

boolean_t bErrorInt

Select DMA transfer error interrupt.

Definition at line 195 of file dma.h.

Referenced by Dma_DisableInt(), and Dma_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/dma/dma.h