| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_adc_int_sel Struct Reference
12-Bit Analog Digital Converter (ADC)

ADC interrupt selection. More...

`#include <adc.h>`

## Data Fields
boolean_t | bScanIrq
| TRUE: Enable Scan Conversion Interrupt.
boolean_t | bPrioIrq
| TRUE: Enable Priority Conversion Interrupt.
boolean_t | bFifoOverrunIrq
| TRUE: Enable FIFO Overrun Interrupt.
boolean_t | bComparisonIrq
| TRUE: Enable Conversion Comparison Interrupt.
boolean_t | bRangeComparisonIrq
| TRUE: Enable Range Comparison Interrupt.

## Detailed Description

ADC interrupt selection.

Definition at line 359 of file adc.h.

## Field Documentation

boolean_t bComparisonIrq

TRUE: Enable Conversion Comparison Interrupt.

Definition at line 364 of file adc.h.

Referenced by Adc_DisableInt(), and Adc_EnableInt().

boolean_t bFifoOverrunIrq

TRUE: Enable FIFO Overrun Interrupt.

Definition at line 363 of file adc.h.

Referenced by Adc_DisableInt(), and Adc_EnableInt().

boolean_t bPrioIrq

TRUE: Enable Priority Conversion Interrupt.

Definition at line 362 of file adc.h.

Referenced by Adc_DisableInt(), and Adc_EnableInt().

boolean_t bRangeComparisonIrq

TRUE: Enable Range Comparison Interrupt.

Definition at line 365 of file adc.h.

Referenced by Adc_DisableInt(), and Adc_EnableInt().

boolean_t bScanIrq

TRUE: Enable Scan Conversion Interrupt.

Definition at line 361 of file adc.h.

Referenced by Adc_DisableInt(), and Adc_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/adc/adc.h