<map id="G" name="G">
<area shape="rect" id="node2" href="$group___mfs_group.html#gae8cd82420bb720cad1f9e15865819e3a" title="Disable CSIO interrupts." alt="" coords="152,183,288,209"/>
<area shape="rect" id="node16" href="$group___mfs_group.html#ga20d458b20db5310def084c028b9b1e6a" title="Disable I2C interrupts." alt="" coords="155,360,285,387"/>
<area shape="rect" id="node27" href="$group___mfs_group.html#ga4f6a2543d12956a5752ff52580612d12" title="Disable LIN interrupts." alt="" coords="156,411,284,437"/>
<area shape="rect" id="node28" href="$group___mfs_group.html#ga4a9257468cace49c8bd1fcc3d1cf05c4" title="Disable UART interrupts." alt="" coords="152,461,288,488"/>
<area shape="rect" id="node3" href="$csio__int__s25fl127s_8c.html#a7de37c4b69fdf7bb88482c9ceff7622e" title="CSIO Master receive interrupt callback function." alt="" coords="337,132,498,159"/>
<area shape="rect" id="node12" href="$csio__int__s25fl127s_8c.html#ad1ec0debf452779ed03c63fb987cd1c9" title="CSIO master transfer interrupt callback function." alt="" coords="337,183,498,209"/>
<area shape="rect" id="node4" href="$csio__int__s25fl127s_8c.html#a8d96de1f8acdd5f446026cccd7ee8e0b" title="Read data from S25FL127S." alt="" coords="561,56,647,83"/>
<area shape="rect" id="node7" href="$csio__int__s25fl127s_8c.html#a1080b0f6949d30ea901a3f8225f9787f" title="Read register from S25FL127S." alt="" coords="563,157,645,184"/>
<area shape="rect" id="node5" href="$csio__int__s25fl127s_8h.html#a9526b5938866a0bd96b1eeb85d716d09" title="Read data from S25FL127S." alt="" coords="739,56,853,83"/>
<area shape="rect" id="node6" href="$csio__int__s25fl127s_8h.html#a0bb140b1ceab26292bb08d17fd9af89d" title="Read ID from S25FL127S." alt="" coords="733,5,859,32"/>
<area shape="rect" id="node8" href="$csio__int__s25fl127s_8h.html#a598e7ad72ae67fa2bc12a359480356d4" title="Sector erase 4KB sector." alt="" coords="713,208,879,235"/>
<area shape="rect" id="node9" href="$csio__int__s25fl127s_8h.html#a95bb1cc75d33448c83cb69e5b4b3886d" title="Chip erase the whole Flash memory." alt="" coords="726,157,866,184"/>
<area shape="rect" id="node10" href="$csio__int__s25fl127s_8h.html#a178746052ef9e5abf9821063ec29da2c" title="Page program S25FL127S." alt="" coords="715,107,877,133"/>
<area shape="rect" id="node11" href="$csio__int__s25fl127s_8h.html#a4f813c900d86faa134d52d4831f4234d" title="Sector erase 64kB or 256kB sector." alt="" coords="719,259,873,285"/>
<area shape="rect" id="node13" href="$csio__int__s25fl127s_8c.html#a42260569e48834e4d5bc3bb2a9c3f970" title="Write command only to S25FL127S." alt="" coords="561,208,647,235"/>
<area shape="rect" id="node14" href="$csio__int__s25fl127s_8c.html#aa2ae015adaa95e1c422a5fac316eb1e9" title="Write command and address only to S25FL127S." alt="" coords="547,259,661,285"/>
<area shape="rect" id="node15" href="$csio__int__s25fl127s_8c.html#a3da7a5d796ca9b4041b0f6d46b116b87" title="Write command, address, data to S25FL127S." alt="" coords="561,107,647,133"/>
<area shape="rect" id="node17" href="$i2c__int__at24cxx_8c.html#afdb5a5aa9b8e36eacc0c54c6ea27ba67" title="I2C TX callback function." alt="" coords="367,411,467,437"/>
<area shape="rect" id="node26" href="$i2c__int__at24cxx_8c.html#a9c449fed7e2de0cec7d466eb3e054ab7" title="I2C stop detection callback function." alt="" coords="343,360,491,387"/>
<area shape="rect" id="node18" href="$i2c__int__at24cxx_8c.html#acdc22353113e27336f95d90c71c1a547" title="Read I2C data." alt="" coords="565,360,643,387"/>
<area shape="rect" id="node21" href="$i2c__int__at24cxx_8c.html#aec4840a29d49b8335f98c801afebeaa5" title="Write I2C data." alt="" coords="565,411,643,437"/>
<area shape="rect" id="node24" href="$i2c__int__at24cxx_8c.html#a6f3d8082e6d0f2a24634e10883ebadfe" title="Perform a dummy write and read at the following." alt="" coords="557,461,651,488"/>
<area shape="rect" id="node19" href="$group___i2c_at24cxx_group.html#ga872adeb2f3933d08622518cc37ba6c28" title="Read the data of current data address of AT24CXX." alt="" coords="710,309,882,336"/>
<area shape="rect" id="node20" href="$group___i2c_at24cxx_group.html#gaf689ffe3a4e1bb250960398d88a882ba" title="Read data bytes following by random read or current address read." alt="" coords="715,360,877,387"/>
<area shape="rect" id="node22" href="$group___i2c_at24cxx_group.html#ga2b547e2af91d16a30b37d34f911f15c4" title="Write byte at a certain address of AT24CXX." alt="" coords="732,411,860,437"/>
<area shape="rect" id="node23" href="$group___i2c_at24cxx_group.html#ga6cd7eaff4e9287364feadd928305f15f" title="Write a page bytes at a page address of AT24CXX." alt="" coords="730,461,862,488"/>
<area shape="rect" id="node25" href="$group___i2c_at24cxx_group.html#ga18bfb67bb388fa8c996b6ac2b3dce006" title="Read a byte data of ramdon data address of AT24CXX." alt="" coords="721,512,871,539"/>
</map>
