| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_dt_intern_data Struct Reference
Dual Timer (DT)

Datatype for holding internal data needed for DT. More...

`#include <dt.h>`

## Data Fields
dt_cb_func_ptr_t | pfnIntCallbackIntern [DtMaxChannels]
| Callback for interrupts of DT channel 0.

## Detailed Description

Datatype for holding internal data needed for DT.

Definition at line 219 of file dt.h.

## Field Documentation

dt_cb_func_ptr_t pfnIntCallbackIntern[DtMaxChannels]

Callback for interrupts of DT channel 0.

Definition at line 222 of file dt.h.

Referenced by Dt_DeInit(), Dt_DisableInt(), Dt_EnableInt(), Dt_Init(), and DtIrqHandler().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/dt/dt.h