| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_csio_int_sel Struct Reference
Multi Function Serial Interface (MFS)

CSIO interrupt selection. More...

`#include <mfs.h>`

## Data Fields
boolean_t | bTxInt
| CSIO TX interrupt.
boolean_t | bRxInt
| CSIO RX interrupt.
boolean_t | bTxIdle
| CSIO TX idle interrupt.
boolean_t | bTxFifoInt
| CSIO TX FIFO interrupt.
boolean_t | bCsErrInt
| CSIO chip selection interrupt.
boolean_t | bSerialTimerInt
| CSIO serial timer interrupt.

## Detailed Description

CSIO interrupt selection.

Definition at line 764 of file mfs.h.

## Field Documentation

boolean_t bCsErrInt

CSIO chip selection interrupt.

Definition at line 770 of file mfs.h.

Referenced by Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

boolean_t bRxInt

CSIO RX interrupt.

Definition at line 767 of file mfs.h.

Referenced by CsioMasterRxIntCallback(), CsioRxData(), CsioRxReg(), Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

boolean_t bSerialTimerInt

CSIO serial timer interrupt.

Definition at line 771 of file mfs.h.

Referenced by Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

boolean_t bTxFifoInt

CSIO TX FIFO interrupt.

Definition at line 769 of file mfs.h.

Referenced by Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

boolean_t bTxIdle

CSIO TX idle interrupt.

Definition at line 768 of file mfs.h.

Referenced by Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

boolean_t bTxInt

CSIO TX interrupt.

Definition at line 766 of file mfs.h.

Referenced by CsioMasterTxIntCallback(), CsioRxData(), CsioRxReg(), CsioTxCmd(), CsioTxCmdAddr(), CsioTxData(), Mfs_Csio_DisableInt(), and Mfs_Csio_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h