| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_prio_fifo_info Struct Reference
12-Bit Analog Digital Converter (ADC)

Priority conversion FIFO information. More...

`#include <adc.h>`

## Data Fields
uint16_t | u16Data
| Priority conversion result data.
boolean_t | bInValid
| Priority conversion invalid or not, TRUE: data valid, FALSE: data invalid.
en_prio_start_cause_t | enStartCause
| Priority conversion start cause.
uint8_t | u8Ch
| Priority conversion channel which is sampled.

## Detailed Description

Priority conversion FIFO information.

Definition at line 409 of file adc.h.

## Field Documentation

boolean_t bInValid

Priority conversion invalid or not, TRUE: data valid, FALSE: data invalid.

Definition at line 412 of file adc.h.

Referenced by Adc_ExtractPrioFifo().

en_prio_start_cause_t enStartCause

Priority conversion start cause.

Definition at line 413 of file adc.h.

Referenced by Adc_ExtractPrioFifo().

uint16_t u16Data

Priority conversion result data.

Definition at line 411 of file adc.h.

Referenced by Adc_ExtractPrioFifo().

uint8_t u8Ch

Priority conversion channel which is sampled.

Definition at line 414 of file adc.h.

Referenced by Adc_ExtractPrioFifo().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/adc/adc.h