<map id="G" name="G">
<area shape="rect" id="node2" href="$i2c__polling__at24cxx_8c.html#abf0e0cf12ff99a33b2a03dafc4bed27f" title="Generate I2C restart signal and send device address." alt="" coords="232,19,312,45"/>
<area shape="rect" id="node4" href="$i2c__int__at24cxx_8c.html#afdb5a5aa9b8e36eacc0c54c6ea27ba67" title="I2C TX callback function." alt="" coords="222,95,322,121"/>
<area shape="rect" id="node3" href="$group___i2c_at24cxx_group.html#ga18bfb67bb388fa8c996b6ac2b3dce006" title="Read a byte data of ramdon data address of AT24CXX." alt="" coords="524,5,673,32"/>
<area shape="rect" id="node5" href="$i2c__int__at24cxx_8c.html#acdc22353113e27336f95d90c71c1a547" title="Read I2C data." alt="" coords="378,107,457,133"/>
<area shape="rect" id="node8" href="$i2c__int__at24cxx_8c.html#aec4840a29d49b8335f98c801afebeaa5" title="Write I2C data." alt="" coords="378,157,457,184"/>
<area shape="rect" id="node11" href="$i2c__int__at24cxx_8c.html#a6f3d8082e6d0f2a24634e10883ebadfe" title="Perform a dummy write and read at the following." alt="" coords="371,56,464,83"/>
<area shape="rect" id="node6" href="$group___i2c_at24cxx_group.html#ga872adeb2f3933d08622518cc37ba6c28" title="Read the data of current data address of AT24CXX." alt="" coords="513,56,685,83"/>
<area shape="rect" id="node7" href="$group___i2c_at24cxx_group.html#gaf689ffe3a4e1bb250960398d88a882ba" title="Read data bytes following by random read or current address read." alt="" coords="517,107,680,133"/>
<area shape="rect" id="node9" href="$group___i2c_at24cxx_group.html#ga2b547e2af91d16a30b37d34f911f15c4" title="Write byte at a certain address of AT24CXX." alt="" coords="535,157,663,184"/>
<area shape="rect" id="node10" href="$group___i2c_at24cxx_group.html#ga6cd7eaff4e9287364feadd928305f15f" title="Write a page bytes at a page address of AT24CXX." alt="" coords="533,208,665,235"/>
</map>
