| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_scan_fifo_info Struct Reference
12-Bit Analog Digital Converter (ADC)

Scan conversion FIFO information. More...

`#include <adc.h>`

## Data Fields
uint16_t | u16Data
| Scan converison result data.
boolean_t | bInValid
| Scan converison invalid or not, TRUE: data valid, FALSE: data invalid.
en_scan_start_cause_t | enStartCause
| Scan converison start cause.
uint8_t | u8Ch
| Scan converison channel which is sampled.

## Detailed Description

Scan conversion FIFO information.

Definition at line 384 of file adc.h.

## Field Documentation

boolean_t bInValid

Scan converison invalid or not, TRUE: data valid, FALSE: data invalid.

Definition at line 387 of file adc.h.

Referenced by Adc_ExtractScanFifo().

en_scan_start_cause_t enStartCause

Scan converison start cause.

Definition at line 388 of file adc.h.

Referenced by Adc_ExtractScanFifo().

uint16_t u16Data

Scan converison result data.

Definition at line 386 of file adc.h.

Referenced by Adc_ExtractScanFifo().

uint8_t u8Ch

Scan converison channel which is sampled.

Definition at line 389 of file adc.h.

Referenced by Adc_ExtractScanFifo().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/adc/adc.h