<map id="G" name="G">
<area shape="rect" id="node2" href="$i2c__polling__at24cxx_8c.html#a980779b9462a9ef16cb58d3b845dd256" title="Sene I2C data." alt="" coords="337,120,431,146"/>
<area shape="rect" id="node8" href="$i2c__polling__at24cxx_8c.html#a519a7e968f229a923f32be4cfd511109" title="Generate I2C start signal and send device address." alt="" coords="351,196,417,222"/>
<area shape="rect" id="node11" href="$i2c__polling__at24cxx_8c.html#a14eb8568c0d5aab6430574e4f66e684f" title="Generate I2C stop signal." alt="" coords="351,638,417,665"/>
<area shape="rect" id="node13" href="$i2c__int__at24cxx_8c.html#aec4840a29d49b8335f98c801afebeaa5" title="Write I2C data." alt="" coords="182,474,261,501"/>
<area shape="rect" id="node3" href="$i2c__polling__at24cxx_8c.html#a9a32d07c5fbbd6b40f354fbc0f124c74" title="Check the error status of I2C." alt="" coords="521,44,660,70"/>
<area shape="rect" id="node4" href="$group___mfs_group.html#ga943e82ab93be47ce1b297d7618bf3941" title="Get status of I2C according to status type." alt="" coords="737,348,865,374"/>
<area shape="rect" id="node5" href="$group___mfs_group.html#gadb0ad11f33b34c1385bf3757bc90b55b" title="Clear status of I2C according to status type." alt="" coords="528,550,653,577"/>
<area shape="rect" id="node6" href="$group___mfs_group.html#ga979470fb82aa36c39da087d1f8f7dbdb" title="Get the ACK signal from slave." alt="" coords="535,94,647,121"/>
<area shape="rect" id="node7" href="$group___mfs_group.html#gadabfb25f844c4a479af2b64b6f970d1e" title="Write I2C data buffer." alt="" coords="527,145,655,172"/>
<area shape="rect" id="node9" href="$group___mfs_group.html#ga2931d5dc017d46e6650a3dcaac570107" title="Configure ACK signal sent to master." alt="" coords="526,246,655,273"/>
<area shape="rect" id="node10" href="$group___mfs_group.html#ga32d7e527a3288abe8d06353766ca07cf" title="Generate start signal of I2C." alt="" coords="514,297,667,324"/>
<area shape="rect" id="node12" href="$group___mfs_group.html#ga20bc2b5286aab156d436881a9fcc46b2" title="Generate stop signal of I2C." alt="" coords="515,753,666,780"/>
<area shape="rect" id="node14" href="$i2c__int__at24cxx_8c.html#a6fefbcd496a9ffe3419fdd95dcddb9d4" title="I2C interrupt callback function." alt="" coords="333,373,435,400"/>
<area shape="rect" id="node16" href="$i2c__int__at24cxx_8c.html#a9c449fed7e2de0cec7d466eb3e054ab7" title="I2C stop detection callback function." alt="" coords="310,562,458,589"/>
<area shape="rect" id="node21" href="$i2c__int__at24cxx_8c.html#afdb5a5aa9b8e36eacc0c54c6ea27ba67" title="I2C TX callback function." alt="" coords="334,474,434,501"/>
<area shape="rect" id="node24" href="$group___mfs_group.html#ga0f86c7248bdc67e81d03ebc702043478" title="Enable I2C interrupts." alt="" coords="527,804,654,830"/>
<area shape="rect" id="node15" href="$i2c__int__at24cxx_8c.html#a9a32d07c5fbbd6b40f354fbc0f124c74" title="Check the error status of I2C." alt="" coords="521,398,660,425"/>
<area shape="rect" id="node17" href="$group___mfs_group.html#ga20d458b20db5310def084c028b9b1e6a" title="Disable I2C interrupts." alt="" coords="526,702,655,729"/>
<area shape="rect" id="node18" href="$group___mfs_group.html#ga5863a73df10f0912f7aebe6cf9fda9bc" title="Device dependent de&#45;initialization of interrupts according CMSIS." alt="" coords="752,677,851,704"/>
<area shape="rect" id="node19" href="$group___mfs_group.html#gadb8437de20f39d6a454facc105a27665" title="Return instance index for a certain I2C instance." alt="" coords="723,778,880,805"/>
<area shape="rect" id="node20" href="$group___mfs_group.html#ga9ac8e034a242e0c55216bc1fa8b763b7" title="Return the internal data for a certain I2C instance." alt="" coords="724,728,879,754"/>
<area shape="rect" id="node22" href="$i2c__int__at24cxx_8c.html#aa5c7c4d067fa7ce24af9e303979969fc" title="Delay function." alt="" coords="564,500,617,526"/>
<area shape="rect" id="node23" href="$group___mfs_group.html#gaf619aa836da6ac31f1f08b36cce9e113" title="Generate restart signal of I2C." alt="" coords="507,449,674,476"/>
<area shape="rect" id="node25" href="$group___mfs_group.html#ga040d9804b9de99276b574fad07166290" title="Device dependent initialization of transmit interrupts according CMSIS with level defined in pdl..." alt="" coords="760,829,843,856"/>
</map>
