| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_uart_int_cb Struct Reference
Multi Function Serial Interface (MFS)

UART interrupt callback function. More...

`#include <mfs.h>`

## Data Fields
func_ptr_t | pfnTxIntCb
| UART TX interrupt callback function pointer.
func_ptr_t | pfnRxIntCb
| UART RX interrupt callback function pointer.
func_ptr_t | pfnTxIdleCb
| UART TX idle interrupt callback function pointer.
func_ptr_t | pfnTxFifoIntCb
| UART TX FIFO interrupt callback function pointer.

## Detailed Description

UART interrupt callback function.

Definition at line 541 of file mfs.h.

## Field Documentation

func_ptr_t pfnRxIntCb

UART RX interrupt callback function pointer.

Definition at line 544 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), Mfs_Uart_EnableInt(), and MfsUartIrqHandlerRx().

func_ptr_t pfnTxFifoIntCb

UART TX FIFO interrupt callback function pointer.

Definition at line 546 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), Mfs_Uart_EnableInt(), and MfsUartIrqHandlerTx().

func_ptr_t pfnTxIdleCb

UART TX idle interrupt callback function pointer.

Definition at line 545 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), Mfs_Uart_EnableInt(), and MfsUartIrqHandlerTx().

func_ptr_t pfnTxIntCb

UART TX interrupt callback function pointer.

Definition at line 543 of file mfs.h.

Referenced by Mfs_Uart_DisableInt(), Mfs_Uart_EnableInt(), and MfsUartIrqHandlerTx().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h