| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_ppg_int_cb Struct Reference
Base Timer (BT)

structure to set the PPG interrupt callback function More...

`#include <bt.h>`

## Data Fields
func_ptr_t | pfnPpgTrigIntCallback
| Pointer to PPG trigger interrupt callback function.
func_ptr_t | pfnPpgUnderflowIntCallback
| Pointer to PPG underflow interrupt callback function.

## Detailed Description

structure to set the PPG interrupt callback function

Definition at line 621 of file bt.h.

## Field Documentation

func_ptr_t pfnPpgTrigIntCallback

Pointer to PPG trigger interrupt callback function.

Definition at line 623 of file bt.h.

Referenced by Bt_Ppg_EnableInt().

func_ptr_t pfnPpgUnderflowIntCallback

Pointer to PPG underflow interrupt callback function.

Definition at line 624 of file bt.h.

Referenced by Bt_Ppg_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h