| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_dt_channel_config Struct Reference
Dual Timer (DT)

Dt channel configuration. More...

`#include <dt.h>`

## Data Fields
uint8_t | u8Mode
| Mode, see description of en_dt_mode_t.
uint8_t | u8PrescalerDiv
| Prescaler, see description of en_dt_prescaler_t.
uint8_t | u8CounterSize
| Counter size, see description of en_dt_countersize_t.

## Detailed Description

Dt channel configuration.

The DT configuration is done on a per channel basis

Definition at line 182 of file dt.h.

## Field Documentation

uint8_t u8CounterSize

Counter size, see description of en_dt_countersize_t.

Definition at line 186 of file dt.h.

Referenced by Dt_Init().

uint8_t u8Mode

Mode, see description of en_dt_mode_t.

Definition at line 184 of file dt.h.

Referenced by Dt_Init().

uint8_t u8PrescalerDiv

Prescaler, see description of en_dt_prescaler_t.

Definition at line 185 of file dt.h.

Referenced by Dt_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/dt/dt.h