| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_frt_int_sel Struct Reference
Free-Run Timer (FRT)

Enumeration of FRT interrupt selection. More...

`#include <mft_frt.h>`

## Data Fields
boolean_t | bFrtZeroMatchInt
| zero match interrupt selection
boolean_t | bFrtPeakMatchInt
| peak match interrupt selection

## Detailed Description

Enumeration of FRT interrupt selection.

Definition at line 200 of file mft_frt.h.

## Field Documentation

boolean_t bFrtPeakMatchInt

peak match interrupt selection

Definition at line 203 of file mft_frt.h.

Referenced by Mft_Frt_DeInitIrq(), Mft_Frt_DisableInt(), Mft_Frt_EnableInt(), and Mft_Frt_InitIrq().

boolean_t bFrtZeroMatchInt

zero match interrupt selection

Definition at line 202 of file mft_frt.h.

Referenced by Mft_Frt_DeInitIrq(), Mft_Frt_DisableInt(), Mft_Frt_EnableInt(), and Mft_Frt_InitIrq().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mft/mft_frt.h