| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_rt_int_sel Struct Reference
Base Timer (BT)

structure to select the Reload timer interrupt More...

`#include <bt.h>`

## Data Fields
boolean_t | bRtTrigInt
| Trigger interrupt selection.
boolean_t | bRtUnderflowInt
| Underflow interrupt selection.

## Detailed Description

structure to select the Reload timer interrupt

Definition at line 725 of file bt.h.

## Field Documentation

boolean_t bRtTrigInt

Trigger interrupt selection.

Definition at line 727 of file bt.h.

Referenced by Bt_Rt_DisableInt(), and Bt_Rt_EnableInt().

boolean_t bRtUnderflowInt

Underflow interrupt selection.

Definition at line 728 of file bt.h.

Referenced by Bt_Rt_DisableInt(), and Bt_Rt_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h