| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_pwc_int_sel Struct Reference
Base Timer (BT)

structure to select the PWC timer interrupt More...

`#include <bt.h>`

## Data Fields
boolean_t | bPwcMeasCmpInt
| Trigger interrupt selection.
boolean_t | bPwcMeasOverflowInt
| Underflow interrupt selection.

## Detailed Description

structure to select the PWC timer interrupt

Definition at line 824 of file bt.h.

## Field Documentation

boolean_t bPwcMeasCmpInt

Trigger interrupt selection.

Definition at line 826 of file bt.h.

Referenced by Bt_Pwc_DisableInt(), and Bt_Pwc_EnableInt().

boolean_t bPwcMeasOverflowInt

Underflow interrupt selection.

Definition at line 827 of file bt.h.

Referenced by Bt_Pwc_DisableInt(), and Bt_Pwc_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h