| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_rtc_int_sel Struct Reference
Real Time Clock (RTC)

Interrupt configuration structure. More...

`#include <rtc.h>`

## Data Fields
uint8_t | HalfSecondInt: 1
uint8_t | OneSecondInt: 1
uint8_t | OneMinuteInt: 1
uint8_t | OneHourInt: 1
uint8_t | TimerInt: 1
uint8_t | AlarmInt: 1
uint8_t | TimeRewriteErrorInt: 1

## Detailed Description

Interrupt configuration structure.

Definition at line 302 of file rtc.h.

## Field Documentation

uint8_t AlarmInt

1: Alarm interrupt enabled 0: Alarm interrupt disabled

Definition at line 314 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t HalfSecondInt

1: 0.5-Second interrupt enabled 0: 0.5-Second interrupt disabled

Definition at line 304 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t OneHourInt

1: 1-Hour interrupt enabled 0: 1-Hour interrupt disabled

Definition at line 310 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t OneMinuteInt

1: 1-Minute interrupt enabled 0: 1-Minute interrupt disabled

Definition at line 308 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t OneSecondInt

1: 1-Second interrupt enabled 0: 1-Second interrupt disabled

Definition at line 306 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t TimeRewriteErrorInt

1: Time Rewrite Error interrupt enabled 0: Time Rewrite Error interrupt disabled

Definition at line 316 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

uint8_t TimerInt

1: Timer interrupt enabled 0: Timer interrupt disabled

Definition at line 312 of file rtc.h.

Referenced by Rtc_DisableInt(), and Rtc_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/rtc/rtc.h