<map id="G" name="G">
<area shape="rect" id="node2" href="$csio__int__s25fl127s_8c.html#ad1ec0debf452779ed03c63fb987cd1c9" title="CSIO master transfer interrupt callback function." alt="" coords="170,56,331,83"/>
<area shape="rect" id="node8" href="$group___mfs_group.html#gac27f4def5e621833c32f17f031ecc876" title="Disable CSIO functions." alt="" coords="177,157,325,184"/>
<area shape="rect" id="node9" href="$group___mfs_group.html#gaa41a2d1716fdaee70f79853aa391101d" title="Enable CSIO functions." alt="" coords="178,208,323,235"/>
<area shape="rect" id="node10" href="$group___mfs_group.html#ga19aa99d2c86e36d0ef7883339d792176" title="Enable CSIO interrupts." alt="" coords="409,107,543,133"/>
<area shape="rect" id="node12" href="$group___mfs_group.html#gade786cb8069c74536a43921cef89dea0" title="Get status of CSIO according to status type." alt="" coords="183,259,318,285"/>
<area shape="rect" id="node13" href="$group___mfs_group.html#ga1f94522e103aff747fcc0328a153bf12" title="Set the transfer byte count of a selected chip selection pin." alt="" coords="141,309,360,336"/>
<area shape="rect" id="node3" href="$group___mfs_group.html#gae8cd82420bb720cad1f9e15865819e3a" title="Disable CSIO interrupts." alt="" coords="408,56,544,83"/>
<area shape="rect" id="node7" href="$group___mfs_group.html#gafcf9263e7822db6b81922bd5fc9a574f" title="Write CSIO data buffer." alt="" coords="409,5,543,32"/>
<area shape="rect" id="node4" href="$group___mfs_group.html#ga7948d557cf9e92dfdef3f3cb952ed72b" title="Return the internal data for a certain CSIO instance." alt="" coords="594,56,755,83"/>
<area shape="rect" id="node5" href="$group___mfs_group.html#ga1f00b61f48c77b018a7bf286916e6d1c" title="Return instance index for a certain CSIO instance." alt="" coords="593,107,757,133"/>
<area shape="rect" id="node6" href="$group___mfs_group.html#ga5863a73df10f0912f7aebe6cf9fda9bc" title="Device dependent de&#45;initialization of interrupts according CMSIS." alt="" coords="625,5,724,32"/>
<area shape="rect" id="node11" href="$group___mfs_group.html#ga040d9804b9de99276b574fad07166290" title="Device dependent initialization of transmit interrupts according CMSIS with level defined in pdl..." alt="" coords="633,157,716,184"/>
</map>
