| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_adc_scan Struct Reference
12-Bit Analog Digital Converter (ADC)

Scan Conversion configuration. More...

`#include <adc.h>`

Collaboration diagram for stc_adc_scan:
[legend]

## Data Fields
en_adc_scan_mode_t | enScanMode
| Conversion Mode. See en_adc_scan_mode_t for details.
stc_ad_channel_list_t | u32ScanCannelSelect
| Selects scan channels for ADC (1 = active)
boolean_t | bScanTimerStartEnable
| TRUE: Triggers Scan Conversion by Timer.
en_adc_timer_select_t | enScanTimerTrigger
| See en_adc_timer_select_t for details.
uint8_t | u8ScanFifoDepth
| Depth of the Scan Conversion FIFO 0...15.

## Detailed Description

Scan Conversion configuration.

Definition at line 273 of file adc.h.

## Field Documentation

boolean_t bScanTimerStartEnable

TRUE: Triggers Scan Conversion by Timer.

Definition at line 277 of file adc.h.

Referenced by Adc_Init().

en_adc_scan_mode_t enScanMode

Conversion Mode. See en_adc_scan_mode_t for details.

Definition at line 275 of file adc.h.

Referenced by Adc_Init().

en_adc_timer_select_t enScanTimerTrigger

See en_adc_timer_select_t for details.

Definition at line 278 of file adc.h.

Referenced by Adc_Init().

stc_ad_channel_list_t u32ScanCannelSelect

Selects scan channels for ADC (1 = active)

Definition at line 276 of file adc.h.

Referenced by Adc_Init().

uint8_t u8ScanFifoDepth

Depth of the Scan Conversion FIFO 0...15.

Definition at line 279 of file adc.h.

Referenced by Adc_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/adc/adc.h