| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_pwm_int_sel Struct Reference
Base Timer (BT)

structure to select the PWM interrupt More...

`#include <bt.h>`

## Data Fields
boolean_t | bPwmTrigInt
| Trigger interrupt selection.
boolean_t | bPwmDutyMatchInt
| Duty match interrupt selection.
boolean_t | bPwmUnderflowInt
| Underflow interrupt selection.

## Detailed Description

structure to select the PWM interrupt

Definition at line 483 of file bt.h.

## Field Documentation

boolean_t bPwmDutyMatchInt

Duty match interrupt selection.

Definition at line 486 of file bt.h.

Referenced by Bt_Pwm_DisableInt(), and Bt_Pwm_EnableInt().

boolean_t bPwmTrigInt

Trigger interrupt selection.

Definition at line 485 of file bt.h.

Referenced by Bt_Pwm_DisableInt(), and Bt_Pwm_EnableInt().

boolean_t bPwmUnderflowInt

Underflow interrupt selection.

Definition at line 487 of file bt.h.

Referenced by Bt_Pwm_DisableInt(), and Bt_Pwm_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h