| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_lin_int_cb Struct Reference
Multi Function Serial Interface (MFS)

LIN interrupt callback function. More...

`#include <mfs.h>`

## Data Fields
func_ptr_t | pfnTxIntCb
| LIN TX interrupt callback function.
func_ptr_t | pfnRxIntCb
| LIN RX interrupt callback function.
func_ptr_t | pfnLinBreakIntCb
| LIN break field interrupt callback function.
func_ptr_t | pfnTxIdleIntCb
| LIN TX idle interrupt callback function.
func_ptr_t | pfnTxFifoIntCb
| LIN TX FIFO interrupt callback function.

## Detailed Description

LIN interrupt callback function.

Definition at line 1014 of file mfs.h.

## Field Documentation

func_ptr_t pfnLinBreakIntCb

LIN break field interrupt callback function.

Definition at line 1018 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), Mfs_Lin_EnableInt(), and MfsLinIrqHandlerStatus().

func_ptr_t pfnRxIntCb

LIN RX interrupt callback function.

Definition at line 1017 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), Mfs_Lin_EnableInt(), and MfsLinIrqHandlerRx().

func_ptr_t pfnTxFifoIntCb

LIN TX FIFO interrupt callback function.

Definition at line 1020 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), Mfs_Lin_EnableInt(), and MfsLinIrqHandlerTx().

func_ptr_t pfnTxIdleIntCb

LIN TX idle interrupt callback function.

Definition at line 1019 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), Mfs_Lin_EnableInt(), and MfsLinIrqHandlerTx().

func_ptr_t pfnTxIntCb

LIN TX interrupt callback function.

Definition at line 1016 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), Mfs_Lin_EnableInt(), and MfsLinIrqHandlerTx().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h