| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Defines
C:/pdl_v10/library/driver/gpio/gpio_s6e1a1xb0a.h File Reference
`#include <stdint.h>`
Include dependency graph for gpio_s6e1a1xb0a.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines
#define | GPIO1PIN_P01_GET ( bFM0P_GPIO_PDIR0_P01 )
#define | GPIO1PIN_P01_PUT(v) ( bFM0P_GPIO_PDOR0_P01=(v) )
#define | GPIO1PIN_P01_INIT(v)
#define | GPIO1PIN_P01_INITIN(v)
#define | GPIO1PIN_P01_INITOUT(v)
#define | GPIO1PIN_NP01_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P01)) )
#define | GPIO1PIN_NP01_PUT(v) ( bFM0P_GPIO_PDOR0_P01=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP01_INIT(v)
#define | GPIO1PIN_NP01_INITIN(v)
#define | GPIO1PIN_NP01_INITOUT(v)
#define | GPIO1PIN_P03_GET ( bFM0P_GPIO_PDIR0_P03 )
#define | GPIO1PIN_P03_PUT(v) ( bFM0P_GPIO_PDOR0_P03=(v) )
#define | GPIO1PIN_P03_INIT(v)
#define | GPIO1PIN_P03_INITIN(v)
#define | GPIO1PIN_P03_INITOUT(v)
#define | GPIO1PIN_NP03_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P03)) )
#define | GPIO1PIN_NP03_PUT(v) ( bFM0P_GPIO_PDOR0_P03=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP03_INIT(v)
#define | GPIO1PIN_NP03_INITIN(v)
#define | GPIO1PIN_NP03_INITOUT(v)
#define | GPIO1PIN_P04_GET ( bFM0P_GPIO_PDIR0_P04 )
#define | GPIO1PIN_P04_PUT(v) ( bFM0P_GPIO_PDOR0_P04=(v) )
#define | GPIO1PIN_P04_INIT(v)
#define | GPIO1PIN_P04_INITIN(v)
#define | GPIO1PIN_P04_INITOUT(v)
#define | GPIO1PIN_NP04_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P04)) )
#define | GPIO1PIN_NP04_PUT(v) ( bFM0P_GPIO_PDOR0_P04=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP04_INIT(v)
#define | GPIO1PIN_NP04_INITIN(v)
#define | GPIO1PIN_NP04_INITOUT(v)
#define | GPIO1PIN_P0F_GET ( bFM0P_GPIO_PDIR0_P0F )
#define | GPIO1PIN_P0F_PUT(v) ( bFM0P_GPIO_PDOR0_P0F=(v) )
#define | GPIO1PIN_P0F_INIT(v)
#define | GPIO1PIN_P0F_INITIN(v)
#define | GPIO1PIN_P0F_INITOUT(v)
#define | GPIO1PIN_NP0F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P0F)) )
#define | GPIO1PIN_NP0F_PUT(v) ( bFM0P_GPIO_PDOR0_P0F=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP0F_INIT(v)
#define | GPIO1PIN_NP0F_INITIN(v)
#define | GPIO1PIN_NP0F_INITOUT(v)
#define | GPIO1PIN_P11_GET ( bFM0P_GPIO_PDIR1_P11 )
#define | GPIO1PIN_P11_PUT(v) ( bFM0P_GPIO_PDOR1_P11=(v) )
#define | GPIO1PIN_P11_INIT(v)
#define | GPIO1PIN_P11_INITIN(v)
#define | GPIO1PIN_P11_INITOUT(v)
#define | GPIO1PIN_NP11_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P11)) )
#define | GPIO1PIN_NP11_PUT(v) ( bFM0P_GPIO_PDOR1_P11=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP11_INIT(v)
#define | GPIO1PIN_NP11_INITIN(v)
#define | GPIO1PIN_NP11_INITOUT(v)
#define | GPIO1PIN_P12_GET ( bFM0P_GPIO_PDIR1_P12 )
#define | GPIO1PIN_P12_PUT(v) ( bFM0P_GPIO_PDOR1_P12=(v) )
#define | GPIO1PIN_P12_INIT(v)
#define | GPIO1PIN_P12_INITIN(v)
#define | GPIO1PIN_P12_INITOUT(v)
#define | GPIO1PIN_NP12_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P12)) )
#define | GPIO1PIN_NP12_PUT(v) ( bFM0P_GPIO_PDOR1_P12=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP12_INIT(v)
#define | GPIO1PIN_NP12_INITIN(v)
#define | GPIO1PIN_NP12_INITOUT(v)
#define | GPIO1PIN_P13_GET ( bFM0P_GPIO_PDIR1_P13 )
#define | GPIO1PIN_P13_PUT(v) ( bFM0P_GPIO_PDOR1_P13=(v) )
#define | GPIO1PIN_P13_INIT(v)
#define | GPIO1PIN_P13_INITIN(v)
#define | GPIO1PIN_P13_INITOUT(v)
#define | GPIO1PIN_NP13_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P13)) )
#define | GPIO1PIN_NP13_PUT(v) ( bFM0P_GPIO_PDOR1_P13=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP13_INIT(v)
#define | GPIO1PIN_NP13_INITIN(v)
#define | GPIO1PIN_NP13_INITOUT(v)
#define | GPIO1PIN_P21_GET ( bFM0P_GPIO_PDIR2_P21 )
#define | GPIO1PIN_P21_PUT(v) ( bFM0P_GPIO_PDOR2_P21=(v) )
#define | GPIO1PIN_P21_INIT(v)
#define | GPIO1PIN_P21_INITIN(v)
#define | GPIO1PIN_P21_INITOUT(v)
#define | GPIO1PIN_NP21_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P21)) )
#define | GPIO1PIN_NP21_PUT(v) ( bFM0P_GPIO_PDOR2_P21=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP21_INIT(v)
#define | GPIO1PIN_NP21_INITIN(v)
#define | GPIO1PIN_NP21_INITOUT(v)
#define | GPIO1PIN_P22_GET ( bFM0P_GPIO_PDIR2_P22 )
#define | GPIO1PIN_P22_PUT(v) ( bFM0P_GPIO_PDOR2_P22=(v) )
#define | GPIO1PIN_P22_INIT(v)
#define | GPIO1PIN_P22_INITIN(v)
#define | GPIO1PIN_P22_INITOUT(v)
#define | GPIO1PIN_NP22_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P22)) )
#define | GPIO1PIN_NP22_PUT(v) ( bFM0P_GPIO_PDOR2_P22=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP22_INIT(v)
#define | GPIO1PIN_NP22_INITIN(v)
#define | GPIO1PIN_NP22_INITOUT(v)
#define | GPIO1PIN_P23_GET ( bFM0P_GPIO_PDIR2_P23 )
#define | GPIO1PIN_P23_PUT(v) ( bFM0P_GPIO_PDOR2_P23=(v) )
#define | GPIO1PIN_P23_INIT(v)
#define | GPIO1PIN_P23_INITIN(v)
#define | GPIO1PIN_P23_INITOUT(v)
#define | GPIO1PIN_NP23_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P23)) )
#define | GPIO1PIN_NP23_PUT(v) ( bFM0P_GPIO_PDOR2_P23=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP23_INIT(v)
#define | GPIO1PIN_NP23_INITIN(v)
#define | GPIO1PIN_NP23_INITOUT(v)
#define | GPIO1PIN_P3A_GET ( bFM0P_GPIO_PDIR3_P3A )
#define | GPIO1PIN_P3A_PUT(v) ( bFM0P_GPIO_PDOR3_P3A=(v) )
#define | GPIO1PIN_P3A_INIT(v)
#define | GPIO1PIN_P3A_INITIN(v)
#define | GPIO1PIN_P3A_INITOUT(v)
#define | GPIO1PIN_NP3A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3A)) )
#define | GPIO1PIN_NP3A_PUT(v) ( bFM0P_GPIO_PDOR3_P3A=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3A_INIT(v)
#define | GPIO1PIN_NP3A_INITIN(v)
#define | GPIO1PIN_NP3A_INITOUT(v)
#define | GPIO1PIN_P3B_GET ( bFM0P_GPIO_PDIR3_P3B )
#define | GPIO1PIN_P3B_PUT(v) ( bFM0P_GPIO_PDOR3_P3B=(v) )
#define | GPIO1PIN_P3B_INIT(v)
#define | GPIO1PIN_P3B_INITIN(v)
#define | GPIO1PIN_P3B_INITOUT(v)
#define | GPIO1PIN_NP3B_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3B)) )
#define | GPIO1PIN_NP3B_PUT(v) ( bFM0P_GPIO_PDOR3_P3B=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3B_INIT(v)
#define | GPIO1PIN_NP3B_INITIN(v)
#define | GPIO1PIN_NP3B_INITOUT(v)
#define | GPIO1PIN_P3C_GET ( bFM0P_GPIO_PDIR3_P3C )
#define | GPIO1PIN_P3C_PUT(v) ( bFM0P_GPIO_PDOR3_P3C=(v) )
#define | GPIO1PIN_P3C_INIT(v)
#define | GPIO1PIN_P3C_INITIN(v)
#define | GPIO1PIN_P3C_INITOUT(v)
#define | GPIO1PIN_NP3C_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3C)) )
#define | GPIO1PIN_NP3C_PUT(v) ( bFM0P_GPIO_PDOR3_P3C=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3C_INIT(v)
#define | GPIO1PIN_NP3C_INITIN(v)
#define | GPIO1PIN_NP3C_INITOUT(v)
#define | GPIO1PIN_P3D_GET ( bFM0P_GPIO_PDIR3_P3D )
#define | GPIO1PIN_P3D_PUT(v) ( bFM0P_GPIO_PDOR3_P3D=(v) )
#define | GPIO1PIN_P3D_INIT(v)
#define | GPIO1PIN_P3D_INITIN(v)
#define | GPIO1PIN_P3D_INITOUT(v)
#define | GPIO1PIN_NP3D_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3D)) )
#define | GPIO1PIN_NP3D_PUT(v) ( bFM0P_GPIO_PDOR3_P3D=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3D_INIT(v)
#define | GPIO1PIN_NP3D_INITIN(v)
#define | GPIO1PIN_NP3D_INITOUT(v)
#define | GPIO1PIN_P3E_GET ( bFM0P_GPIO_PDIR3_P3E )
#define | GPIO1PIN_P3E_PUT(v) ( bFM0P_GPIO_PDOR3_P3E=(v) )
#define | GPIO1PIN_P3E_INIT(v)
#define | GPIO1PIN_P3E_INITIN(v)
#define | GPIO1PIN_P3E_INITOUT(v)
#define | GPIO1PIN_NP3E_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3E)) )
#define | GPIO1PIN_NP3E_PUT(v) ( bFM0P_GPIO_PDOR3_P3E=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3E_INIT(v)
#define | GPIO1PIN_NP3E_INITIN(v)
#define | GPIO1PIN_NP3E_INITOUT(v)
#define | GPIO1PIN_P3F_GET ( bFM0P_GPIO_PDIR3_P3F )
#define | GPIO1PIN_P3F_PUT(v) ( bFM0P_GPIO_PDOR3_P3F=(v) )
#define | GPIO1PIN_P3F_INIT(v)
#define | GPIO1PIN_P3F_INITIN(v)
#define | GPIO1PIN_P3F_INITOUT(v)
#define | GPIO1PIN_NP3F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3F)) )
#define | GPIO1PIN_NP3F_PUT(v) ( bFM0P_GPIO_PDOR3_P3F=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3F_INIT(v)
#define | GPIO1PIN_NP3F_INITIN(v)
#define | GPIO1PIN_NP3F_INITOUT(v)
#define | GPIO1PIN_P46_GET ( bFM0P_GPIO_PDIR4_P46 )
#define | GPIO1PIN_P46_PUT(v) ( bFM0P_GPIO_PDOR4_P46=(v) )
#define | GPIO1PIN_P46_INIT(v)
#define | GPIO1PIN_P46_INITIN(v)
#define | GPIO1PIN_P46_INITOUT(v)
#define | GPIO1PIN_NP46_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P46)) )
#define | GPIO1PIN_NP46_PUT(v) ( bFM0P_GPIO_PDOR4_P46=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP46_INIT(v)
#define | GPIO1PIN_NP46_INITIN(v)
#define | GPIO1PIN_NP46_INITOUT(v)
#define | GPIO1PIN_P47_GET ( bFM0P_GPIO_PDIR4_P47 )
#define | GPIO1PIN_P47_PUT(v) ( bFM0P_GPIO_PDOR4_P47=(v) )
#define | GPIO1PIN_P47_INIT(v)
#define | GPIO1PIN_P47_INITIN(v)
#define | GPIO1PIN_P47_INITOUT(v)
#define | GPIO1PIN_NP47_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P47)) )
#define | GPIO1PIN_NP47_PUT(v) ( bFM0P_GPIO_PDOR4_P47=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP47_INIT(v)
#define | GPIO1PIN_NP47_INITIN(v)
#define | GPIO1PIN_NP47_INITOUT(v)
#define | GPIO1PIN_P60_GET ( bFM0P_GPIO_PDIR6_P60 )
#define | GPIO1PIN_P60_PUT(v) ( bFM0P_GPIO_PDOR6_P60=(v) )
#define | GPIO1PIN_P60_INIT(v)
#define | GPIO1PIN_P60_INITIN(v)
#define | GPIO1PIN_P60_INITOUT(v)
#define | GPIO1PIN_NP60_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P60)) )
#define | GPIO1PIN_NP60_PUT(v) ( bFM0P_GPIO_PDOR6_P60=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP60_INIT(v)
#define | GPIO1PIN_NP60_INITIN(v)
#define | GPIO1PIN_NP60_INITOUT(v)
#define | GPIO1PIN_P61_GET ( bFM0P_GPIO_PDIR6_P61 )
#define | GPIO1PIN_P61_PUT(v) ( bFM0P_GPIO_PDOR6_P61=(v) )
#define | GPIO1PIN_P61_INIT(v)
#define | GPIO1PIN_P61_INITIN(v)
#define | GPIO1PIN_P61_INITOUT(v)
#define | GPIO1PIN_NP61_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P61)) )
#define | GPIO1PIN_NP61_PUT(v) ( bFM0P_GPIO_PDOR6_P61=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP61_INIT(v)
#define | GPIO1PIN_NP61_INITIN(v)
#define | GPIO1PIN_NP61_INITOUT(v)
#define | GPIO1PIN_PE0_GET ( bFM0P_GPIO_PDIRE_PE0 )
#define | GPIO1PIN_PE0_PUT(v) ( bFM0P_GPIO_PDORE_PE0=(v) )
#define | GPIO1PIN_PE0_INIT(v)
#define | GPIO1PIN_PE0_INITIN(v)
#define | GPIO1PIN_PE0_INITOUT(v)
#define | GPIO1PIN_NPE0_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE0)) )
#define | GPIO1PIN_NPE0_PUT(v) ( bFM0P_GPIO_PDORE_PE0=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE0_INIT(v)
#define | GPIO1PIN_NPE0_INITIN(v)
#define | GPIO1PIN_NPE0_INITOUT(v)
#define | GPIO1PIN_PE2_GET ( bFM0P_GPIO_PDIRE_PE2 )
#define | GPIO1PIN_PE2_PUT(v) ( bFM0P_GPIO_PDORE_PE2=(v) )
#define | GPIO1PIN_PE2_INIT(v)
#define | GPIO1PIN_PE2_INITIN(v)
#define | GPIO1PIN_PE2_INITOUT(v)
#define | GPIO1PIN_NPE2_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE2)) )
#define | GPIO1PIN_NPE2_PUT(v) ( bFM0P_GPIO_PDORE_PE2=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE2_INIT(v)
#define | GPIO1PIN_NPE2_INITIN(v)
#define | GPIO1PIN_NPE2_INITOUT(v)
#define | GPIO1PIN_PE3_GET ( bFM0P_GPIO_PDIRE_PE3 )
#define | GPIO1PIN_PE3_PUT(v) ( bFM0P_GPIO_PDORE_PE3=(v) )
#define | GPIO1PIN_PE3_INIT(v)
#define | GPIO1PIN_PE3_INITIN(v)
#define | GPIO1PIN_PE3_INITOUT(v)
#define | GPIO1PIN_NPE3_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE3)) )
#define | GPIO1PIN_NPE3_PUT(v) ( bFM0P_GPIO_PDORE_PE3=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE3_INIT(v)
#define | GPIO1PIN_NPE3_INITIN(v)
#define | GPIO1PIN_NPE3_INITOUT(v)
#define | FGPIO1PIN_P01_GET ( FM0P_FASTIO->FPDIR0_f.P01 )
#define | FGPIO1PIN_P01_PUT(v) ( bFM0P_GPIO_FPDOR0_P01=(v) )
#define | FGPIO1PIN_P01_INIT(v)
#define | FGPIO1PIN_P01_INITIN(v)
#define | FGPIO1PIN_P01_INITOUT(v)
#define | FGPIO1PIN_NP01_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P01)) )
#define | FGPIO1PIN_NP01_PUT(v) ( bFM0P_GPIO_FPDOR0_P01=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP01_INIT(v)
#define | FGPIO1PIN_NP01_INITIN(v)
#define | FGPIO1PIN_NP01_INITOUT(v)
#define | FGPIO1PIN_P03_GET ( FM0P_FASTIO->FPDIR0_f.P03 )
#define | FGPIO1PIN_P03_PUT(v) ( bFM0P_GPIO_FPDOR0_P03=(v) )
#define | FGPIO1PIN_P03_INIT(v)
#define | FGPIO1PIN_P03_INITIN(v)
#define | FGPIO1PIN_P03_INITOUT(v)
#define | FGPIO1PIN_NP03_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P03)) )
#define | FGPIO1PIN_NP03_PUT(v) ( bFM0P_GPIO_FPDOR0_P03=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP03_INIT(v)
#define | FGPIO1PIN_NP03_INITIN(v)
#define | FGPIO1PIN_NP03_INITOUT(v)
#define | FGPIO1PIN_P04_GET ( FM0P_FASTIO->FPDIR0_f.P04 )
#define | FGPIO1PIN_P04_PUT(v) ( bFM0P_GPIO_FPDOR0_P04=(v) )
#define | FGPIO1PIN_P04_INIT(v)
#define | FGPIO1PIN_P04_INITIN(v)
#define | FGPIO1PIN_P04_INITOUT(v)
#define | FGPIO1PIN_NP04_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P04)) )
#define | FGPIO1PIN_NP04_PUT(v) ( bFM0P_GPIO_FPDOR0_P04=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP04_INIT(v)
#define | FGPIO1PIN_NP04_INITIN(v)
#define | FGPIO1PIN_NP04_INITOUT(v)
#define | FGPIO1PIN_P0F_GET ( FM0P_FASTIO->FPDIR0_f.P0F )
#define | FGPIO1PIN_P0F_PUT(v) ( bFM0P_GPIO_FPDOR0_P0F=(v) )
#define | FGPIO1PIN_P0F_INIT(v)
#define | FGPIO1PIN_P0F_INITIN(v)
#define | FGPIO1PIN_P0F_INITOUT(v)
#define | FGPIO1PIN_NP0F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P0F)) )
#define | FGPIO1PIN_NP0F_PUT(v) ( bFM0P_GPIO_FPDOR0_P0F=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP0F_INIT(v)
#define | FGPIO1PIN_NP0F_INITIN(v)
#define | FGPIO1PIN_NP0F_INITOUT(v)
#define | FGPIO1PIN_P11_GET ( FM0P_FASTIO->FPDIR1_f.P11 )
#define | FGPIO1PIN_P11_PUT(v) ( bFM0P_GPIO_FPDOR1_P11=(v) )
#define | FGPIO1PIN_P11_INIT(v)
#define | FGPIO1PIN_P11_INITIN(v)
#define | FGPIO1PIN_P11_INITOUT(v)
#define | FGPIO1PIN_NP11_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P11)) )
#define | FGPIO1PIN_NP11_PUT(v) ( bFM0P_GPIO_FPDOR1_P11=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP11_INIT(v)
#define | FGPIO1PIN_NP11_INITIN(v)
#define | FGPIO1PIN_NP11_INITOUT(v)
#define | FGPIO1PIN_P12_GET ( FM0P_FASTIO->FPDIR1_f.P12 )
#define | FGPIO1PIN_P12_PUT(v) ( bFM0P_GPIO_FPDOR1_P12=(v) )
#define | FGPIO1PIN_P12_INIT(v)
#define | FGPIO1PIN_P12_INITIN(v)
#define | FGPIO1PIN_P12_INITOUT(v)
#define | FGPIO1PIN_NP12_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P12)) )
#define | FGPIO1PIN_NP12_PUT(v) ( bFM0P_GPIO_FPDOR1_P12=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP12_INIT(v)
#define | FGPIO1PIN_NP12_INITIN(v)
#define | FGPIO1PIN_NP12_INITOUT(v)
#define | FGPIO1PIN_P13_GET ( FM0P_FASTIO->FPDIR1_f.P13 )
#define | FGPIO1PIN_P13_PUT(v) ( bFM0P_GPIO_FPDOR1_P13=(v) )
#define | FGPIO1PIN_P13_INIT(v)
#define | FGPIO1PIN_P13_INITIN(v)
#define | FGPIO1PIN_P13_INITOUT(v)
#define | FGPIO1PIN_NP13_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P13)) )
#define | FGPIO1PIN_NP13_PUT(v) ( bFM0P_GPIO_FPDOR1_P13=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP13_INIT(v)
#define | FGPIO1PIN_NP13_INITIN(v)
#define | FGPIO1PIN_NP13_INITOUT(v)
#define | FGPIO1PIN_P21_GET ( FM0P_FASTIO->FPDIR2_f.P21 )
#define | FGPIO1PIN_P21_PUT(v) ( bFM0P_GPIO_FPDOR2_P21=(v) )
#define | FGPIO1PIN_P21_INIT(v)
#define | FGPIO1PIN_P21_INITIN(v)
#define | FGPIO1PIN_P21_INITOUT(v)
#define | FGPIO1PIN_NP21_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P21)) )
#define | FGPIO1PIN_NP21_PUT(v) ( bFM0P_GPIO_FPDOR2_P21=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP21_INIT(v)
#define | FGPIO1PIN_NP21_INITIN(v)
#define | FGPIO1PIN_NP21_INITOUT(v)
#define | FGPIO1PIN_P22_GET ( FM0P_FASTIO->FPDIR2_f.P22 )
#define | FGPIO1PIN_P22_PUT(v) ( bFM0P_GPIO_FPDOR2_P22=(v) )
#define | FGPIO1PIN_P22_INIT(v)
#define | FGPIO1PIN_P22_INITIN(v)
#define | FGPIO1PIN_P22_INITOUT(v)
#define | FGPIO1PIN_NP22_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P22)) )
#define | FGPIO1PIN_NP22_PUT(v) ( bFM0P_GPIO_FPDOR2_P22=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP22_INIT(v)
#define | FGPIO1PIN_NP22_INITIN(v)
#define | FGPIO1PIN_NP22_INITOUT(v)
#define | FGPIO1PIN_P23_GET ( FM0P_FASTIO->FPDIR2_f.P23 )
#define | FGPIO1PIN_P23_PUT(v) ( bFM0P_GPIO_FPDOR2_P23=(v) )
#define | FGPIO1PIN_P23_INIT(v)
#define | FGPIO1PIN_P23_INITIN(v)
#define | FGPIO1PIN_P23_INITOUT(v)
#define | FGPIO1PIN_NP23_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P23)) )
#define | FGPIO1PIN_NP23_PUT(v) ( bFM0P_GPIO_FPDOR2_P23=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP23_INIT(v)
#define | FGPIO1PIN_NP23_INITIN(v)
#define | FGPIO1PIN_NP23_INITOUT(v)
#define | FGPIO1PIN_P3A_GET ( FM0P_FASTIO->FPDIR3_f.P3A )
#define | FGPIO1PIN_P3A_PUT(v) ( bFM0P_GPIO_FPDOR3_P3A=(v) )
#define | FGPIO1PIN_P3A_INIT(v)
#define | FGPIO1PIN_P3A_INITIN(v)
#define | FGPIO1PIN_P3A_INITOUT(v)
#define | FGPIO1PIN_NP3A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3A)) )
#define | FGPIO1PIN_NP3A_PUT(v) ( bFM0P_GPIO_FPDOR3_P3A=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3A_INIT(v)
#define | FGPIO1PIN_NP3A_INITIN(v)
#define | FGPIO1PIN_NP3A_INITOUT(v)
#define | FGPIO1PIN_P3B_GET ( FM0P_FASTIO->FPDIR3_f.P3B )
#define | FGPIO1PIN_P3B_PUT(v) ( bFM0P_GPIO_FPDOR3_P3B=(v) )
#define | FGPIO1PIN_P3B_INIT(v)
#define | FGPIO1PIN_P3B_INITIN(v)
#define | FGPIO1PIN_P3B_INITOUT(v)
#define | FGPIO1PIN_NP3B_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3B)) )
#define | FGPIO1PIN_NP3B_PUT(v) ( bFM0P_GPIO_FPDOR3_P3B=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3B_INIT(v)
#define | FGPIO1PIN_NP3B_INITIN(v)
#define | FGPIO1PIN_NP3B_INITOUT(v)
#define | FGPIO1PIN_P3C_GET ( FM0P_FASTIO->FPDIR3_f.P3C )
#define | FGPIO1PIN_P3C_PUT(v) ( bFM0P_GPIO_FPDOR3_P3C=(v) )
#define | FGPIO1PIN_P3C_INIT(v)
#define | FGPIO1PIN_P3C_INITIN(v)
#define | FGPIO1PIN_P3C_INITOUT(v)
#define | FGPIO1PIN_NP3C_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3C)) )
#define | FGPIO1PIN_NP3C_PUT(v) ( bFM0P_GPIO_FPDOR3_P3C=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3C_INIT(v)
#define | FGPIO1PIN_NP3C_INITIN(v)
#define | FGPIO1PIN_NP3C_INITOUT(v)
#define | FGPIO1PIN_P3D_GET ( FM0P_FASTIO->FPDIR3_f.P3D )
#define | FGPIO1PIN_P3D_PUT(v) ( bFM0P_GPIO_FPDOR3_P3D=(v) )
#define | FGPIO1PIN_P3D_INIT(v)
#define | FGPIO1PIN_P3D_INITIN(v)
#define | FGPIO1PIN_P3D_INITOUT(v)
#define | FGPIO1PIN_NP3D_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3D)) )
#define | FGPIO1PIN_NP3D_PUT(v) ( bFM0P_GPIO_FPDOR3_P3D=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3D_INIT(v)
#define | FGPIO1PIN_NP3D_INITIN(v)
#define | FGPIO1PIN_NP3D_INITOUT(v)
#define | FGPIO1PIN_P3E_GET ( FM0P_FASTIO->FPDIR3_f.P3E )
#define | FGPIO1PIN_P3E_PUT(v) ( bFM0P_GPIO_FPDOR3_P3E=(v) )
#define | FGPIO1PIN_P3E_INIT(v)
#define | FGPIO1PIN_P3E_INITIN(v)
#define | FGPIO1PIN_P3E_INITOUT(v)
#define | FGPIO1PIN_NP3E_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3E)) )
#define | FGPIO1PIN_NP3E_PUT(v) ( bFM0P_GPIO_FPDOR3_P3E=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3E_INIT(v)
#define | FGPIO1PIN_NP3E_INITIN(v)
#define | FGPIO1PIN_NP3E_INITOUT(v)
#define | FGPIO1PIN_P3F_GET ( FM0P_FASTIO->FPDIR3_f.P3F )
#define | FGPIO1PIN_P3F_PUT(v) ( bFM0P_GPIO_FPDOR3_P3F=(v) )
#define | FGPIO1PIN_P3F_INIT(v)
#define | FGPIO1PIN_P3F_INITIN(v)
#define | FGPIO1PIN_P3F_INITOUT(v)
#define | FGPIO1PIN_NP3F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3F)) )
#define | FGPIO1PIN_NP3F_PUT(v) ( bFM0P_GPIO_FPDOR3_P3F=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3F_INIT(v)
#define | FGPIO1PIN_NP3F_INITIN(v)
#define | FGPIO1PIN_NP3F_INITOUT(v)
#define | FGPIO1PIN_P46_GET ( FM0P_FASTIO->FPDIR4_f.P46 )
#define | FGPIO1PIN_P46_PUT(v) ( bFM0P_GPIO_FPDOR4_P46=(v) )
#define | FGPIO1PIN_P46_INIT(v)
#define | FGPIO1PIN_P46_INITIN(v)
#define | FGPIO1PIN_P46_INITOUT(v)
#define | FGPIO1PIN_NP46_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P46)) )
#define | FGPIO1PIN_NP46_PUT(v) ( bFM0P_GPIO_FPDOR4_P46=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP46_INIT(v)
#define | FGPIO1PIN_NP46_INITIN(v)
#define | FGPIO1PIN_NP46_INITOUT(v)
#define | FGPIO1PIN_P47_GET ( FM0P_FASTIO->FPDIR4_f.P47 )
#define | FGPIO1PIN_P47_PUT(v) ( bFM0P_GPIO_FPDOR4_P47=(v) )
#define | FGPIO1PIN_P47_INIT(v)
#define | FGPIO1PIN_P47_INITIN(v)
#define | FGPIO1PIN_P47_INITOUT(v)
#define | FGPIO1PIN_NP47_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P47)) )
#define | FGPIO1PIN_NP47_PUT(v) ( bFM0P_GPIO_FPDOR4_P47=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP47_INIT(v)
#define | FGPIO1PIN_NP47_INITIN(v)
#define | FGPIO1PIN_NP47_INITOUT(v)
#define | FGPIO1PIN_P60_GET ( FM0P_FASTIO->FPDIR6_f.P60 )
#define | FGPIO1PIN_P60_PUT(v) ( bFM0P_GPIO_FPDOR6_P60=(v) )
#define | FGPIO1PIN_P60_INIT(v)
#define | FGPIO1PIN_P60_INITIN(v)
#define | FGPIO1PIN_P60_INITOUT(v)
#define | FGPIO1PIN_NP60_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P60)) )
#define | FGPIO1PIN_NP60_PUT(v) ( bFM0P_GPIO_FPDOR6_P60=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP60_INIT(v)
#define | FGPIO1PIN_NP60_INITIN(v)
#define | FGPIO1PIN_NP60_INITOUT(v)
#define | FGPIO1PIN_P61_GET ( FM0P_FASTIO->FPDIR6_f.P61 )
#define | FGPIO1PIN_P61_PUT(v) ( bFM0P_GPIO_FPDOR6_P61=(v) )
#define | FGPIO1PIN_P61_INIT(v)
#define | FGPIO1PIN_P61_INITIN(v)
#define | FGPIO1PIN_P61_INITOUT(v)
#define | FGPIO1PIN_NP61_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P61)) )
#define | FGPIO1PIN_NP61_PUT(v) ( bFM0P_GPIO_FPDOR6_P61=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP61_INIT(v)
#define | FGPIO1PIN_NP61_INITIN(v)
#define | FGPIO1PIN_NP61_INITOUT(v)
#define | FGPIO1PIN_PE0_GET ( FM0P_FASTIO->FPDIRE_f.PE0 )
#define | FGPIO1PIN_PE0_PUT(v) ( bFM0P_GPIO_FPDORE_PE0=(v) )
#define | FGPIO1PIN_PE0_INIT(v)
#define | FGPIO1PIN_PE0_INITIN(v)
#define | FGPIO1PIN_PE0_INITOUT(v)
#define | FGPIO1PIN_NPE0_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE0)) )
#define | FGPIO1PIN_NPE0_PUT(v) ( bFM0P_GPIO_FPDORE_PE0=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE0_INIT(v)
#define | FGPIO1PIN_NPE0_INITIN(v)
#define | FGPIO1PIN_NPE0_INITOUT(v)
#define | FGPIO1PIN_PE2_GET ( FM0P_FASTIO->FPDIRE_f.PE2 )
#define | FGPIO1PIN_PE2_PUT(v) ( bFM0P_GPIO_FPDORE_PE2=(v) )
#define | FGPIO1PIN_PE2_INIT(v)
#define | FGPIO1PIN_PE2_INITIN(v)
#define | FGPIO1PIN_PE2_INITOUT(v)
#define | FGPIO1PIN_NPE2_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE2)) )
#define | FGPIO1PIN_NPE2_PUT(v) ( bFM0P_GPIO_FPDORE_PE2=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE2_INIT(v)
#define | FGPIO1PIN_NPE2_INITIN(v)
#define | FGPIO1PIN_NPE2_INITOUT(v)
#define | FGPIO1PIN_PE3_GET ( FM0P_FASTIO->FPDIRE_f.PE3 )
#define | FGPIO1PIN_PE3_PUT(v) ( bFM0P_GPIO_FPDORE_PE3=(v) )
#define | FGPIO1PIN_PE3_INIT(v)
#define | FGPIO1PIN_PE3_INITIN(v)
#define | FGPIO1PIN_PE3_INITOUT(v)
#define | FGPIO1PIN_NPE3_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE3)) )
#define | FGPIO1PIN_NPE3_PUT(v) ( bFM0P_GPIO_FPDORE_PE3=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE3_INIT(v)
#define | FGPIO1PIN_NPE3_INITIN(v)
#define | FGPIO1PIN_NPE3_INITOUT(v)
#define | SetPinFunc_ADTG_1_ADC0(dummy)
#define | SetPinFunc_ADTG_1_ADC1(dummy)
#define | SetPinFunc_ADTG_1_ADC2(dummy)
#define | SetPinFunc_AIN0_0(dummy)
#define | SetPinFunc_AIN0_1(dummy)
#define | SetPinFunc_AIN0_3(dummy)
#define | SetPinFunc_BIN0_0(dummy)
#define | SetPinFunc_BIN0_1(dummy)
#define | SetPinFunc_BIN0_3(dummy)
#define | SetPinFunc_CROUT_1(dummy)
#define | SetPinFunc_DTTI0X_1(dummy)
#define | SetPinFunc_DTTI0X_2(dummy)
#define | SetPinFunc_FRCK0_0(dummy)
#define | SetPinFunc_FRCK0_2(dummy)
#define | SetPinFunc_IC00_0(dummy)
#define | SetPinFunc_IC00_2(dummy)
#define | SetPinFunc_IC01_1(dummy)
#define | SetPinFunc_IC01_2(dummy)
#define | SetPinFunc_IC02_0(dummy)
#define | SetPinFunc_IC02_1(dummy)
#define | SetPinFunc_IC03_1(dummy)
#define | SetPinFunc_IGTRG0_0(dummy)
#define | SetPinFunc_IGTRG0_1(dummy)
#define | SetPinFunc_INT00_1(dummy)
#define | SetPinFunc_INT01_1(dummy)
#define | SetPinFunc_INT02_1(dummy)
#define | SetPinFunc_INT02_2(dummy)
#define | SetPinFunc_INT03_0(dummy)
#define | SetPinFunc_INT03_2(dummy)
#define | SetPinFunc_INT04_0(dummy)
#define | SetPinFunc_INT04_1(dummy)
#define | SetPinFunc_INT05_0(dummy)
#define | SetPinFunc_INT05_1(dummy)
#define | SetPinFunc_INT06_0(dummy)
#define | SetPinFunc_INT06_1(dummy)
#define | SetPinFunc_INT15_0(dummy)
#define | SetPinFunc_INT15_1(dummy)
#define | SetPinFunc_NMIX(dummy)
#define | SetPinFunc_RTCCO_0(dummy)
#define | SetPinFunc_RTCCO_1(dummy)
#define | SetPinFunc_RTCCO_2(dummy)
#define | SetPinFunc_RTO00_0(dummy)
#define | SetPinFunc_RTO01_0(dummy)
#define | SetPinFunc_RTO02_0(dummy)
#define | SetPinFunc_RTO03_0(dummy)
#define | SetPinFunc_RTO04_0(dummy)
#define | SetPinFunc_RTO05_0(dummy)
#define | SetPinFunc_SCK0_0(dummy)
#define | SetPinFunc_SCK0_2(dummy)
#define | SetPinFunc_SCK1_1(dummy)
#define | SetPinFunc_SCK3_0(dummy)
#define | SetPinFunc_SCK3_2(dummy)
#define | SetPinFunc_SCS10_2(dummy)
#define | SetPinFunc_SCS11_2(dummy)
#define | SetPinFunc_SCS30_2(dummy)
#define | SetPinFunc_SCS31_2(dummy)
#define | SetPinFunc_SIN0_0(dummy)
#define | SetPinFunc_SIN0_2(dummy)
#define | SetPinFunc_SIN1_1(dummy)
#define | SetPinFunc_SIN3_0(dummy)
#define | SetPinFunc_SIN3_2(dummy)
#define | SetPinFunc_SOT0_0(dummy)
#define | SetPinFunc_SOT0_2(dummy)
#define | SetPinFunc_SOT1_1(dummy)
#define | SetPinFunc_SOT3_0(dummy)
#define | SetPinFunc_SOT3_2(dummy)
#define | SetPinFunc_SUBOUT_0(dummy)
#define | SetPinFunc_SUBOUT_1(dummy)
#define | SetPinFunc_SUBOUT_2(dummy)
#define | SetPinFunc_TIOA0_0_OUT(dummy)
#define | SetPinFunc_TIOA0_1_OUT(dummy)
#define | SetPinFunc_TIOA1_0_IN(dummy)
#define | SetPinFunc_TIOA1_0_OUT(dummy)
#define | SetPinFunc_TIOA1_1_IN(dummy)
#define | SetPinFunc_TIOA1_1_OUT(dummy)
#define | SetPinFunc_TIOA2_0_OUT(dummy)
#define | SetPinFunc_TIOA2_1_OUT(dummy)
#define | SetPinFunc_TIOA2_2_OUT(dummy)
#define | SetPinFunc_TIOA3_1_IN(dummy)
#define | SetPinFunc_TIOA3_1_OUT(dummy)
#define | SetPinFunc_TIOB0_1_IN(dummy)
#define | SetPinFunc_TIOB1_1_IN(dummy)
#define | SetPinFunc_TIOB2_0_IN(dummy)
#define | SetPinFunc_TIOB2_2_IN(dummy)
#define | SetPinFunc_ZIN0_0(dummy)
#define | SetPinFunc_ZIN0_1(dummy)
#define | SetPinFunc_ZIN0_3(dummy)
#define | SetPinFunc_AN01(dummy) ( bFM0P_GPIO_ADE_AN01 = 1 )
#define | SetPinFunc_AN02(dummy) ( bFM0P_GPIO_ADE_AN02 = 1 )
#define | SetPinFunc_AN03(dummy) ( bFM0P_GPIO_ADE_AN03 = 1 )
#define | SetPinFunc_AN06(dummy) ( bFM0P_GPIO_ADE_AN06 = 1 )
#define | SetPinFunc_AN07(dummy) ( bFM0P_GPIO_ADE_AN07 = 1 )

## Detailed Description

Headerfile for S6E1A1XB0A GPIO functions, included in gpio1pin.h

History:

- 2013-12-04 1.0 Edison Zhang First version
- 2014-05-14 1.1 Edison Zhang Update P46/P47, PE2/PE3 initialization

Definition in file gpio_s6e1a1xb0a.h.

## Define Documentation

#define FGPIO1PIN_NP01_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P01)) )

Definition at line 951 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP01_INITIN(v) \
                                                             : FGPIO1PIN_NP01_INITOUT(v) )

Definition at line 955 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P01=0u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 958 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P01=1u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 962 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP01_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P01=(uint8_t)(~(v)) )

Definition at line 953 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP03_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P03)) )

Definition at line 986 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP03_INITIN(v) \
                                                             : FGPIO1PIN_NP03_INITOUT(v) )

Definition at line 990 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P03=0u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 993 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P03=1u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 997 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP03_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P03=(uint8_t)(~(v)) )

Definition at line 988 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP04_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P04)) )

Definition at line 1021 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP04_INITIN(v) \
                                                             : FGPIO1PIN_NP04_INITOUT(v) )

Definition at line 1025 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P04=0u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1028 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P04=1u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1032 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP04_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P04=(uint8_t)(~(v)) )

Definition at line 1023 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP0F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P0F)) )

Definition at line 1056 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP0F_INITIN(v) \
                                                             : FGPIO1PIN_NP0F_INITOUT(v) )

Definition at line 1060 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P0F=0u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1063 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P0F=1u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1067 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P0F=(uint8_t)(~(v)) )

Definition at line 1058 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP11_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P11)) )

Definition at line 1094 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP11_INITIN(v) \
                                                             : FGPIO1PIN_NP11_INITOUT(v) )

Definition at line 1098 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P11=0u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1101 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P11=1u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1107 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP11_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P11=(uint8_t)(~(v)) )

Definition at line 1096 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP12_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P12)) )

Definition at line 1135 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP12_INITIN(v) \
                                                             : FGPIO1PIN_NP12_INITOUT(v) )

Definition at line 1139 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P12=0u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1142 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P12=1u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1148 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP12_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P12=(uint8_t)(~(v)) )

Definition at line 1137 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP13_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P13)) )

Definition at line 1176 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP13_INITIN(v) \
                                                             : FGPIO1PIN_NP13_INITOUT(v) )

Definition at line 1180 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P13=0u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1183 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P13=1u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1189 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP13_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P13=(uint8_t)(~(v)) )

Definition at line 1178 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP21_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P21)) )

Definition at line 1214 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP21_INITIN(v) \
                                                             : FGPIO1PIN_NP21_INITOUT(v) )

Definition at line 1218 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P21=0u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1221 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P21=1u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1225 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP21_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P21=(uint8_t)(~(v)) )

Definition at line 1216 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP22_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P22)) )

Definition at line 1252 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP22_INITIN(v) \
                                                             : FGPIO1PIN_NP22_INITOUT(v) )

Definition at line 1256 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P22=0u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1259 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P22=1u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1265 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP22_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P22=(uint8_t)(~(v)) )

Definition at line 1254 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP23_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P23)) )

Definition at line 1293 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP23_INITIN(v) \
                                                             : FGPIO1PIN_NP23_INITOUT(v) )

Definition at line 1297 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P23=0u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1300 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P23=1u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1306 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP23_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P23=(uint8_t)(~(v)) )

Definition at line 1295 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3A)) )

Definition at line 1331 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3A_INITIN(v) \
                                                             : FGPIO1PIN_NP3A_INITOUT(v) )

Definition at line 1335 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3A=0u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 1338 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3A=1u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 1342 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3A=(uint8_t)(~(v)) )

Definition at line 1333 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3B_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3B)) )

Definition at line 1366 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3B_INITIN(v) \
                                                             : FGPIO1PIN_NP3B_INITOUT(v) )

Definition at line 1370 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3B=0u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 1373 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3B=1u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 1377 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3B=(uint8_t)(~(v)) )

Definition at line 1368 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3C_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3C)) )

Definition at line 1401 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3C_INITIN(v) \
                                                             : FGPIO1PIN_NP3C_INITOUT(v) )

Definition at line 1405 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3C=0u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 1408 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3C=1u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 1412 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3C=(uint8_t)(~(v)) )

Definition at line 1403 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3D_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3D)) )

Definition at line 1436 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3D_INITIN(v) \
                                                             : FGPIO1PIN_NP3D_INITOUT(v) )

Definition at line 1440 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3D=0u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 1443 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3D=1u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 1447 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3D=(uint8_t)(~(v)) )

Definition at line 1438 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3E_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3E)) )

Definition at line 1471 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3E_INITIN(v) \
                                                             : FGPIO1PIN_NP3E_INITOUT(v) )

Definition at line 1475 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3E=0u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 1478 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3E=1u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 1482 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3E=(uint8_t)(~(v)) )

Definition at line 1473 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3F)) )

Definition at line 1506 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3F_INITIN(v) \
                                                             : FGPIO1PIN_NP3F_INITOUT(v) )

Definition at line 1510 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3F=0u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 1513 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3F=1u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 1517 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3F=(uint8_t)(~(v)) )

Definition at line 1508 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP46_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P46)) )

Definition at line 1545 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP46_INITIN(v) \
                                                             : FGPIO1PIN_NP46_INITOUT(v) )

Definition at line 1549 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P46=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 1552 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P46=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 1558 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP46_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P46=(uint8_t)(~(v)) )

Definition at line 1547 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP47_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P47)) )

Definition at line 1588 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP47_INITIN(v) \
                                                             : FGPIO1PIN_NP47_INITOUT(v) )

Definition at line 1592 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P47=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 1595 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P47=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 1601 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP47_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P47=(uint8_t)(~(v)) )

Definition at line 1590 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP60_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P60)) )

Definition at line 1627 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP60_INITIN(v) \
                                                             : FGPIO1PIN_NP60_INITOUT(v) )

Definition at line 1631 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P60=0u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1634 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR6_P60=1u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1638 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP60_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P60=(uint8_t)(~(v)) )

Definition at line 1629 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP61_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P61)) )

Definition at line 1662 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP61_INITIN(v) \
                                                             : FGPIO1PIN_NP61_INITOUT(v) )

Definition at line 1666 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P61=0u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1669 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR6_P61=1u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1673 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NP61_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P61=(uint8_t)(~(v)) )

Definition at line 1664 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE0_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE0)) )

Definition at line 1697 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE0_INITIN(v) \
                                                             : FGPIO1PIN_NPE0_INITOUT(v) )

Definition at line 1701 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE0=0u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1704 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE0=1u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1708 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE0=(uint8_t)(~(v)) )

Definition at line 1699 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE2_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE2)) )

Definition at line 1736 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE2_INITIN(v) \
                                                             : FGPIO1PIN_NPE2_INITOUT(v) )

Definition at line 1740 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE2=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1743 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE2=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1749 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE2=(uint8_t)(~(v)) )

Definition at line 1738 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE3_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE3)) )

Definition at line 1779 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE3_INITIN(v) \
                                                             : FGPIO1PIN_NPE3_INITOUT(v) )

Definition at line 1783 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE3=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1786 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE3=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1792 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_NPE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE3=(uint8_t)(~(v)) )

Definition at line 1781 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P01_GET ( FM0P_FASTIO->FPDIR0_f.P01 )

Definition at line 934 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P01_INITIN(v) \
                                                             : FGPIO1PIN_P01_INITOUT(v) )

Definition at line 938 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P01=0u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 941 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P01=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P01=1u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 945 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P01_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P01=(v) )

Definition at line 936 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P03_GET ( FM0P_FASTIO->FPDIR0_f.P03 )

Definition at line 969 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P03_INITIN(v) \
                                                             : FGPIO1PIN_P03_INITOUT(v) )

Definition at line 973 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P03=0u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 976 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P03=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P03=1u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 980 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P03_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P03=(v) )

Definition at line 971 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P04_GET ( FM0P_FASTIO->FPDIR0_f.P04 )

Definition at line 1004 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P04_INITIN(v) \
                                                             : FGPIO1PIN_P04_INITOUT(v) )

Definition at line 1008 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P04=0u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1011 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P04=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P04=1u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1015 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P04_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P04=(v) )

Definition at line 1006 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P0F_GET ( FM0P_FASTIO->FPDIR0_f.P0F )

Definition at line 1039 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P0F_INITIN(v) \
                                                             : FGPIO1PIN_P0F_INITOUT(v) )

Definition at line 1043 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P0F=0u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1046 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P0F=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P0F=1u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1050 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P0F=(v) )

Definition at line 1041 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P11_GET ( FM0P_FASTIO->FPDIR1_f.P11 )

Definition at line 1074 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P11_INITIN(v) \
                                                             : FGPIO1PIN_P11_INITOUT(v) )

Definition at line 1078 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P11=0u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1081 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P11=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P11=1u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1087 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P11_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P11=(v) )

Definition at line 1076 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P12_GET ( FM0P_FASTIO->FPDIR1_f.P12 )

Definition at line 1115 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P12_INITIN(v) \
                                                             : FGPIO1PIN_P12_INITOUT(v) )

Definition at line 1119 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P12=0u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1122 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P12=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P12=1u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1128 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P12_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P12=(v) )

Definition at line 1117 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P13_GET ( FM0P_FASTIO->FPDIR1_f.P13 )

Definition at line 1156 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P13_INITIN(v) \
                                                             : FGPIO1PIN_P13_INITOUT(v) )

Definition at line 1160 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P13=0u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1163 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P13=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P13=1u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1169 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P13_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P13=(v) )

Definition at line 1158 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P21_GET ( FM0P_FASTIO->FPDIR2_f.P21 )

Definition at line 1197 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P21_INITIN(v) \
                                                             : FGPIO1PIN_P21_INITOUT(v) )

Definition at line 1201 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P21=0u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1204 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P21=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P21=1u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1208 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P21_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P21=(v) )

Definition at line 1199 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P22_GET ( FM0P_FASTIO->FPDIR2_f.P22 )

Definition at line 1232 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P22_INITIN(v) \
                                                             : FGPIO1PIN_P22_INITOUT(v) )

Definition at line 1236 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P22=0u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1239 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P22=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P22=1u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1245 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P22_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P22=(v) )

Definition at line 1234 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P23_GET ( FM0P_FASTIO->FPDIR2_f.P23 )

Definition at line 1273 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P23_INITIN(v) \
                                                             : FGPIO1PIN_P23_INITOUT(v) )

Definition at line 1277 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P23=0u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1280 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P23=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P23=1u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1286 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P23_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P23=(v) )

Definition at line 1275 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3A_GET ( FM0P_FASTIO->FPDIR3_f.P3A )

Definition at line 1314 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3A_INITIN(v) \
                                                             : FGPIO1PIN_P3A_INITOUT(v) )

Definition at line 1318 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3A=0u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 1321 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3A=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3A=1u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 1325 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3A=(v) )

Definition at line 1316 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3B_GET ( FM0P_FASTIO->FPDIR3_f.P3B )

Definition at line 1349 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3B_INITIN(v) \
                                                             : FGPIO1PIN_P3B_INITOUT(v) )

Definition at line 1353 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3B=0u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 1356 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3B=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3B=1u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 1360 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3B=(v) )

Definition at line 1351 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3C_GET ( FM0P_FASTIO->FPDIR3_f.P3C )

Definition at line 1384 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3C_INITIN(v) \
                                                             : FGPIO1PIN_P3C_INITOUT(v) )

Definition at line 1388 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3C=0u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 1391 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3C=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3C=1u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 1395 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3C=(v) )

Definition at line 1386 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3D_GET ( FM0P_FASTIO->FPDIR3_f.P3D )

Definition at line 1419 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3D_INITIN(v) \
                                                             : FGPIO1PIN_P3D_INITOUT(v) )

Definition at line 1423 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3D=0u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 1426 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3D=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3D=1u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 1430 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3D=(v) )

Definition at line 1421 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3E_GET ( FM0P_FASTIO->FPDIR3_f.P3E )

Definition at line 1454 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3E_INITIN(v) \
                                                             : FGPIO1PIN_P3E_INITOUT(v) )

Definition at line 1458 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3E=0u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 1461 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3E=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3E=1u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 1465 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3E=(v) )

Definition at line 1456 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3F_GET ( FM0P_FASTIO->FPDIR3_f.P3F )

Definition at line 1489 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3F_INITIN(v) \
                                                             : FGPIO1PIN_P3F_INITOUT(v) )

Definition at line 1493 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3F=0u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 1496 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3F=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3F=1u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 1500 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3F=(v) )

Definition at line 1491 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P46_GET ( FM0P_FASTIO->FPDIR4_f.P46 )

Definition at line 1524 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P46_INITIN(v) \
                                                             : FGPIO1PIN_P46_INITOUT(v) )

Definition at line 1528 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P46=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 1531 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P46=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P46=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 1537 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P46_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P46=(v) )

Definition at line 1526 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P47_GET ( FM0P_FASTIO->FPDIR4_f.P47 )

Definition at line 1567 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P47_INITIN(v) \
                                                             : FGPIO1PIN_P47_INITOUT(v) )

Definition at line 1571 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P47=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 1574 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P47=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P47=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 1580 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P47_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P47=(v) )

Definition at line 1569 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P60_GET ( FM0P_FASTIO->FPDIR6_f.P60 )

Definition at line 1610 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P60_INITIN(v) \
                                                             : FGPIO1PIN_P60_INITOUT(v) )

Definition at line 1614 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P60=0u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1617 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR6_P60=(v).bInitVal; \
                                              bFM0P_GPIO_DDR6_P60=1u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1621 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P60_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P60=(v) )

Definition at line 1612 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P61_GET ( FM0P_FASTIO->FPDIR6_f.P61 )

Definition at line 1645 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P61_INITIN(v) \
                                                             : FGPIO1PIN_P61_INITOUT(v) )

Definition at line 1649 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P61=0u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1652 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR6_P61=(v).bInitVal; \
                                              bFM0P_GPIO_DDR6_P61=1u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1656 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_P61_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P61=(v) )

Definition at line 1647 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE0_GET ( FM0P_FASTIO->FPDIRE_f.PE0 )

Definition at line 1680 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE0_INITIN(v) \
                                                             : FGPIO1PIN_PE0_INITOUT(v) )

Definition at line 1684 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE0=0u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1687 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE0=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE0=1u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1691 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE0=(v) )

Definition at line 1682 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE2_GET ( FM0P_FASTIO->FPDIRE_f.PE2 )

Definition at line 1715 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE2_INITIN(v) \
                                                             : FGPIO1PIN_PE2_INITOUT(v) )

Definition at line 1719 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE2=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1722 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE2=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE2=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1728 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE2=(v) )

Definition at line 1717 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE3_GET ( FM0P_FASTIO->FPDIRE_f.PE3 )

Definition at line 1758 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE3_INITIN(v) \
                                                             : FGPIO1PIN_PE3_INITOUT(v) )

Definition at line 1762 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE3=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1765 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE3=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE3=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1771 of file gpio_s6e1a1xb0a.h.

#define FGPIO1PIN_PE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE3=(v) )

Definition at line 1760 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP01_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P01)) )

Definition at line 80 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP01_INITIN(v) \
                                                            : GPIO1PIN_NP01_INITOUT(v) )

Definition at line 84 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P01=0u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 87 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P01=1u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 91 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP01_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P01=(uint32_t)(!(v)) )

Definition at line 82 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP03_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P03)) )

Definition at line 115 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP03_INITIN(v) \
                                                            : GPIO1PIN_NP03_INITOUT(v) )

Definition at line 119 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P03=0u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 122 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P03=1u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 126 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP03_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P03=(uint32_t)(!(v)) )

Definition at line 117 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP04_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P04)) )

Definition at line 150 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP04_INITIN(v) \
                                                            : GPIO1PIN_NP04_INITOUT(v) )

Definition at line 154 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P04=0u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 157 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P04=1u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 161 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP04_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P04=(uint32_t)(!(v)) )

Definition at line 152 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP0F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P0F)) )

Definition at line 185 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP0F_INITIN(v) \
                                                            : GPIO1PIN_NP0F_INITOUT(v) )

Definition at line 189 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P0F=0u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 192 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P0F=1u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 196 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P0F=(uint32_t)(!(v)) )

Definition at line 187 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP11_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P11)) )

Definition at line 223 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP11_INITIN(v) \
                                                            : GPIO1PIN_NP11_INITOUT(v) )

Definition at line 227 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P11=0u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 230 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P11=1u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 236 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP11_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P11=(uint32_t)(!(v)) )

Definition at line 225 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP12_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P12)) )

Definition at line 264 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP12_INITIN(v) \
                                                            : GPIO1PIN_NP12_INITOUT(v) )

Definition at line 268 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P12=0u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 271 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P12=1u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 277 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP12_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P12=(uint32_t)(!(v)) )

Definition at line 266 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP13_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P13)) )

Definition at line 305 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP13_INITIN(v) \
                                                            : GPIO1PIN_NP13_INITOUT(v) )

Definition at line 309 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P13=0u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 312 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P13=1u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 318 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP13_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P13=(uint32_t)(!(v)) )

Definition at line 307 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP21_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P21)) )

Definition at line 343 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP21_INITIN(v) \
                                                            : GPIO1PIN_NP21_INITOUT(v) )

Definition at line 347 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P21=0u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 350 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P21=1u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 354 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP21_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P21=(uint32_t)(!(v)) )

Definition at line 345 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP22_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P22)) )

Definition at line 381 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP22_INITIN(v) \
                                                            : GPIO1PIN_NP22_INITOUT(v) )

Definition at line 385 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P22=0u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 388 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P22=1u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 394 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP22_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P22=(uint32_t)(!(v)) )

Definition at line 383 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP23_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P23)) )

Definition at line 422 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP23_INITIN(v) \
                                                            : GPIO1PIN_NP23_INITOUT(v) )

Definition at line 426 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P23=0u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 429 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P23=1u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 435 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP23_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P23=(uint32_t)(!(v)) )

Definition at line 424 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3A)) )

Definition at line 460 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3A_INITIN(v) \
                                                            : GPIO1PIN_NP3A_INITOUT(v) )

Definition at line 464 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3A=0u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 467 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3A=1u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 471 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3A=(uint32_t)(!(v)) )

Definition at line 462 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3B_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3B)) )

Definition at line 495 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3B_INITIN(v) \
                                                            : GPIO1PIN_NP3B_INITOUT(v) )

Definition at line 499 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3B=0u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 502 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3B=1u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 506 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3B=(uint32_t)(!(v)) )

Definition at line 497 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3C_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3C)) )

Definition at line 530 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3C_INITIN(v) \
                                                            : GPIO1PIN_NP3C_INITOUT(v) )

Definition at line 534 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3C=0u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 537 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3C=1u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 541 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3C=(uint32_t)(!(v)) )

Definition at line 532 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3D_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3D)) )

Definition at line 565 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3D_INITIN(v) \
                                                            : GPIO1PIN_NP3D_INITOUT(v) )

Definition at line 569 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3D=0u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 572 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3D=1u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 576 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3D=(uint32_t)(!(v)) )

Definition at line 567 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3E_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3E)) )

Definition at line 600 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3E_INITIN(v) \
                                                            : GPIO1PIN_NP3E_INITOUT(v) )

Definition at line 604 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3E=0u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 607 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3E=1u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 611 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3E=(uint32_t)(!(v)) )

Definition at line 602 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3F)) )

Definition at line 635 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3F_INITIN(v) \
                                                            : GPIO1PIN_NP3F_INITOUT(v) )

Definition at line 639 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3F=0u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 642 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3F=1u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 646 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3F=(uint32_t)(!(v)) )

Definition at line 637 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP46_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P46)) )

Definition at line 674 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP46_INITIN(v) \
                                                            : GPIO1PIN_NP46_INITOUT(v) )

Definition at line 678 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P46=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 681 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P46=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 687 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP46_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P46=(uint32_t)(!(v)) )

Definition at line 676 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP47_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P47)) )

Definition at line 717 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP47_INITIN(v) \
                                                            : GPIO1PIN_NP47_INITOUT(v) )

Definition at line 721 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P47=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 724 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P47=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 730 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP47_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P47=(uint32_t)(!(v)) )

Definition at line 719 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP60_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P60)) )

Definition at line 756 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP60_INITIN(v) \
                                                            : GPIO1PIN_NP60_INITOUT(v) )

Definition at line 760 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P60=0u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 763 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR6_P60=1u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 767 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP60_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P60=(uint32_t)(!(v)) )

Definition at line 758 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP61_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P61)) )

Definition at line 791 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP61_INITIN(v) \
                                                            : GPIO1PIN_NP61_INITOUT(v) )

Definition at line 795 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P61=0u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 798 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR6_P61=1u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 802 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NP61_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P61=(uint32_t)(!(v)) )

Definition at line 793 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE0_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE0)) )

Definition at line 826 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE0_INITIN(v) \
                                                            : GPIO1PIN_NPE0_INITOUT(v) )

Definition at line 830 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE0=0u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 833 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE0=1u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 837 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE0=(uint32_t)(!(v)) )

Definition at line 828 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE2_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE2)) )

Definition at line 865 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE2_INITIN(v) \
                                                            : GPIO1PIN_NPE2_INITOUT(v) )

Definition at line 869 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE2=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 872 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE2=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 878 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE2=(uint32_t)(!(v)) )

Definition at line 867 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE3_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE3)) )

Definition at line 908 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE3_INITIN(v) \
                                                            : GPIO1PIN_NPE3_INITOUT(v) )

Definition at line 912 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE3=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 915 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE3=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 921 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_NPE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE3=(uint32_t)(!(v)) )

Definition at line 910 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P01_GET ( bFM0P_GPIO_PDIR0_P01 )

Definition at line 63 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P01_INITIN(v) \
                                                            : GPIO1PIN_P01_INITOUT(v) )

Definition at line 67 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P01=0u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 70 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P01=1u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 74 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P01_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P01=(v) )

Definition at line 65 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P03_GET ( bFM0P_GPIO_PDIR0_P03 )

Definition at line 98 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P03_INITIN(v) \
                                                            : GPIO1PIN_P03_INITOUT(v) )

Definition at line 102 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P03=0u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 105 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P03=1u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 109 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P03_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P03=(v) )

Definition at line 100 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P04_GET ( bFM0P_GPIO_PDIR0_P04 )

Definition at line 133 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P04_INITIN(v) \
                                                            : GPIO1PIN_P04_INITOUT(v) )

Definition at line 137 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P04=0u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 140 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P04=1u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 144 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P04_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P04=(v) )

Definition at line 135 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P0F_GET ( bFM0P_GPIO_PDIR0_P0F )

Definition at line 168 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P0F_INITIN(v) \
                                                            : GPIO1PIN_P0F_INITOUT(v) )

Definition at line 172 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P0F=0u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 175 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P0F=1u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 179 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P0F=(v) )

Definition at line 170 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P11_GET ( bFM0P_GPIO_PDIR1_P11 )

Definition at line 203 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P11_INITIN(v) \
                                                            : GPIO1PIN_P11_INITOUT(v) )

Definition at line 207 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P11=0u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 210 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P11=1u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 216 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P11_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P11=(v) )

Definition at line 205 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P12_GET ( bFM0P_GPIO_PDIR1_P12 )

Definition at line 244 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P12_INITIN(v) \
                                                            : GPIO1PIN_P12_INITOUT(v) )

Definition at line 248 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P12=0u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 251 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P12=1u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 257 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P12_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P12=(v) )

Definition at line 246 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P13_GET ( bFM0P_GPIO_PDIR1_P13 )

Definition at line 285 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P13_INITIN(v) \
                                                            : GPIO1PIN_P13_INITOUT(v) )

Definition at line 289 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P13=0u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 292 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P13=1u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 298 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P13_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P13=(v) )

Definition at line 287 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P21_GET ( bFM0P_GPIO_PDIR2_P21 )

Definition at line 326 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P21_INITIN(v) \
                                                            : GPIO1PIN_P21_INITOUT(v) )

Definition at line 330 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P21=0u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 333 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P21=1u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 337 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P21_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P21=(v) )

Definition at line 328 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P22_GET ( bFM0P_GPIO_PDIR2_P22 )

Definition at line 361 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P22_INITIN(v) \
                                                            : GPIO1PIN_P22_INITOUT(v) )

Definition at line 365 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P22=0u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 368 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P22=1u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 374 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P22_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P22=(v) )

Definition at line 363 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P23_GET ( bFM0P_GPIO_PDIR2_P23 )

Definition at line 402 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P23_INITIN(v) \
                                                            : GPIO1PIN_P23_INITOUT(v) )

Definition at line 406 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P23=0u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 409 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P23=1u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 415 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P23_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P23=(v) )

Definition at line 404 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3A_GET ( bFM0P_GPIO_PDIR3_P3A )

Definition at line 443 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3A_INITIN(v) \
                                                            : GPIO1PIN_P3A_INITOUT(v) )

Definition at line 447 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3A=0u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 450 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3A=1u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 454 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3A=(v) )

Definition at line 445 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3B_GET ( bFM0P_GPIO_PDIR3_P3B )

Definition at line 478 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3B_INITIN(v) \
                                                            : GPIO1PIN_P3B_INITOUT(v) )

Definition at line 482 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3B=0u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 485 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3B=1u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 489 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3B=(v) )

Definition at line 480 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3C_GET ( bFM0P_GPIO_PDIR3_P3C )

Definition at line 513 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3C_INITIN(v) \
                                                            : GPIO1PIN_P3C_INITOUT(v) )

Definition at line 517 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3C=0u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 520 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3C=1u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 524 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3C=(v) )

Definition at line 515 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3D_GET ( bFM0P_GPIO_PDIR3_P3D )

Definition at line 548 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3D_INITIN(v) \
                                                            : GPIO1PIN_P3D_INITOUT(v) )

Definition at line 552 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3D=0u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 555 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3D=1u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 559 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3D=(v) )

Definition at line 550 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3E_GET ( bFM0P_GPIO_PDIR3_P3E )

Definition at line 583 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3E_INITIN(v) \
                                                            : GPIO1PIN_P3E_INITOUT(v) )

Definition at line 587 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3E=0u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 590 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3E=1u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 594 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3E=(v) )

Definition at line 585 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3F_GET ( bFM0P_GPIO_PDIR3_P3F )

Definition at line 618 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3F_INITIN(v) \
                                                            : GPIO1PIN_P3F_INITOUT(v) )

Definition at line 622 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3F=0u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 625 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3F=1u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 629 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3F=(v) )

Definition at line 620 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P46_GET ( bFM0P_GPIO_PDIR4_P46 )

Definition at line 653 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P46_INITIN(v) \
                                                            : GPIO1PIN_P46_INITOUT(v) )

Definition at line 657 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P46=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 660 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P46=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 666 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P46_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P46=(v) )

Definition at line 655 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P47_GET ( bFM0P_GPIO_PDIR4_P47 )

Definition at line 696 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P47_INITIN(v) \
                                                            : GPIO1PIN_P47_INITOUT(v) )

Definition at line 700 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P47=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 703 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P47=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 709 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P47_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P47=(v) )

Definition at line 698 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P60_GET ( bFM0P_GPIO_PDIR6_P60 )

Definition at line 739 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P60_INITIN(v) \
                                                            : GPIO1PIN_P60_INITOUT(v) )

Definition at line 743 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P60=0u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 746 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(v).bInitVal; \
                                             bFM0P_GPIO_DDR6_P60=1u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 750 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P60_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P60=(v) )

Definition at line 741 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P61_GET ( bFM0P_GPIO_PDIR6_P61 )

Definition at line 774 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P61_INITIN(v) \
                                                            : GPIO1PIN_P61_INITOUT(v) )

Definition at line 778 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P61=0u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 781 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(v).bInitVal; \
                                             bFM0P_GPIO_DDR6_P61=1u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 785 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_P61_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P61=(v) )

Definition at line 776 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE0_GET ( bFM0P_GPIO_PDIRE_PE0 )

Definition at line 809 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE0_INITIN(v) \
                                                            : GPIO1PIN_PE0_INITOUT(v) )

Definition at line 813 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE0=0u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 816 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE0=1u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 820 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE0=(v) )

Definition at line 811 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE2_GET ( bFM0P_GPIO_PDIRE_PE2 )

Definition at line 844 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE2_INITIN(v) \
                                                            : GPIO1PIN_PE2_INITOUT(v) )

Definition at line 848 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE2=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 851 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE2=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 857 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE2=(v) )

Definition at line 846 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE3_GET ( bFM0P_GPIO_PDIRE_PE3 )

Definition at line 887 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE3_INITIN(v) \
                                                            : GPIO1PIN_PE3_INITOUT(v) )

Definition at line 891 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE3=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 894 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE3=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 900 of file gpio_s6e1a1xb0a.h.

#define GPIO1PIN_PE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE3=(v) )

Definition at line 889 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ADTG_1_ADC0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 12u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 1805 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ADTG_1_ADC1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 16u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 1809 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ADTG_1_ADC2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 20u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 1813 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 1817 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 1821 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QAIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 1826 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AN01 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN01 = 1 )

Definition at line 2183 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AN02 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN02 = 1 )

Definition at line 2186 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AN03 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN03 = 1 )

Definition at line 2189 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AN06 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN06 = 1 )

Definition at line 2192 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_AN07 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN07 = 1 )

Definition at line 2195 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_BIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 1831 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_BIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 1835 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_BIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QBIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 1839 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_CROUT_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 1u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 1844 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_DTTI0X_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 16u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 1848 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_DTTI0X_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 16u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 1852 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_FRCK0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 18u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 1856 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_FRCK0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 18u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 1860 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC00_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 20u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 1865 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC00_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 20u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 1869 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC01_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 23u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 1874 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC01_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 23u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 1878 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC02_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 26u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 1883 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC02_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 26u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 1888 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IC03_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 29u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 1893 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IGTRG0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 13u, 1u, 0x00u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 1898 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_IGTRG0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 13u, 1u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 1902 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT00_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 0u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 1906 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT01_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 1911 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT02_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 1916 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT02_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 1921 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT03_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 1925 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT03_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 1929 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT04_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 1933 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT04_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 8u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 1937 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT05_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 1942 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT05_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 1946 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT06_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 12u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 1951 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT06_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 1955 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT15_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 30u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 1959 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_INT15_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 30u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 1963 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_NMIX | ( |  | dummy | ) |

Value:

    do{ bFM0P_GPIO_EPFR00_NMIS = 1; \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 1967 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTCCO_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 1971 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTCCO_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 1975 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTCCO_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 1980 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO00_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 0u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 1984 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO01_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 1988 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO02_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 1992 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO03_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 1996 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO04_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 2000 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_RTO05_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 2004 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCK0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 2008 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCK0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 8u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 2013 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCK1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 14u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 2017 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCK3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 26u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 2022 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCK3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 26u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 2026 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCS10_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 2030 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCS11_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 2034 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCS30_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 12u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 2038 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SCS31_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 14u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 2042 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 2046 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SIN0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 2050 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SIN1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 2054 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SIN3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 22u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 2059 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SIN3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 22u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 2063 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SOT0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 2067 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SOT0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 2072 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SOT1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 2076 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SOT3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 24u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 2081 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SOT3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 24u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 2085 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SUBOUT_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 2089 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SUBOUT_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 2093 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_SUBOUT_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 2098 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA0_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 2102 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA0_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 2106 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA1_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 2110 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA1_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 2114 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA1_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 8u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 2118 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA1_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 2122 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA2_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 2126 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA2_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 2131 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA2_2_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 2135 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA3_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 24u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 2139 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOA3_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 26u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 2143 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOB0_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 4u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 2147 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOB1_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 2151 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOB2_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 20u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 2155 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_TIOB2_2_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 20u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 2160 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ZIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 2164 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ZIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 2168 of file gpio_s6e1a1xb0a.h.

#define SetPinFunc_ZIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QZIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 2173 of file gpio_s6e1a1xb0a.h.