| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Defines
C:/pdl_v10/library/driver/gpio/gpio_s6e1a1xc0a.h File Reference
`#include <stdint.h>`
Include dependency graph for gpio_s6e1a1xc0a.h:

Go to the source code of this file.

## Defines
#define | GPIO1PIN_P00_GET ( bFM0P_GPIO_PDIR0_P00 )
#define | GPIO1PIN_P00_PUT(v) ( bFM0P_GPIO_PDOR0_P00=(v) )
#define | GPIO1PIN_P00_INIT(v)
#define | GPIO1PIN_P00_INITIN(v)
#define | GPIO1PIN_P00_INITOUT(v)
#define | GPIO1PIN_NP00_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P00)) )
#define | GPIO1PIN_NP00_PUT(v) ( bFM0P_GPIO_PDOR0_P00=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP00_INIT(v)
#define | GPIO1PIN_NP00_INITIN(v)
#define | GPIO1PIN_NP00_INITOUT(v)
#define | GPIO1PIN_P01_GET ( bFM0P_GPIO_PDIR0_P01 )
#define | GPIO1PIN_P01_PUT(v) ( bFM0P_GPIO_PDOR0_P01=(v) )
#define | GPIO1PIN_P01_INIT(v)
#define | GPIO1PIN_P01_INITIN(v)
#define | GPIO1PIN_P01_INITOUT(v)
#define | GPIO1PIN_NP01_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P01)) )
#define | GPIO1PIN_NP01_PUT(v) ( bFM0P_GPIO_PDOR0_P01=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP01_INIT(v)
#define | GPIO1PIN_NP01_INITIN(v)
#define | GPIO1PIN_NP01_INITOUT(v)
#define | GPIO1PIN_P02_GET ( bFM0P_GPIO_PDIR0_P02 )
#define | GPIO1PIN_P02_PUT(v) ( bFM0P_GPIO_PDOR0_P02=(v) )
#define | GPIO1PIN_P02_INIT(v)
#define | GPIO1PIN_P02_INITIN(v)
#define | GPIO1PIN_P02_INITOUT(v)
#define | GPIO1PIN_NP02_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P02)) )
#define | GPIO1PIN_NP02_PUT(v) ( bFM0P_GPIO_PDOR0_P02=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP02_INIT(v)
#define | GPIO1PIN_NP02_INITIN(v)
#define | GPIO1PIN_NP02_INITOUT(v)
#define | GPIO1PIN_P03_GET ( bFM0P_GPIO_PDIR0_P03 )
#define | GPIO1PIN_P03_PUT(v) ( bFM0P_GPIO_PDOR0_P03=(v) )
#define | GPIO1PIN_P03_INIT(v)
#define | GPIO1PIN_P03_INITIN(v)
#define | GPIO1PIN_P03_INITOUT(v)
#define | GPIO1PIN_NP03_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P03)) )
#define | GPIO1PIN_NP03_PUT(v) ( bFM0P_GPIO_PDOR0_P03=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP03_INIT(v)
#define | GPIO1PIN_NP03_INITIN(v)
#define | GPIO1PIN_NP03_INITOUT(v)
#define | GPIO1PIN_P04_GET ( bFM0P_GPIO_PDIR0_P04 )
#define | GPIO1PIN_P04_PUT(v) ( bFM0P_GPIO_PDOR0_P04=(v) )
#define | GPIO1PIN_P04_INIT(v)
#define | GPIO1PIN_P04_INITIN(v)
#define | GPIO1PIN_P04_INITOUT(v)
#define | GPIO1PIN_NP04_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P04)) )
#define | GPIO1PIN_NP04_PUT(v) ( bFM0P_GPIO_PDOR0_P04=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP04_INIT(v)
#define | GPIO1PIN_NP04_INITIN(v)
#define | GPIO1PIN_NP04_INITOUT(v)
#define | GPIO1PIN_P0F_GET ( bFM0P_GPIO_PDIR0_P0F )
#define | GPIO1PIN_P0F_PUT(v) ( bFM0P_GPIO_PDOR0_P0F=(v) )
#define | GPIO1PIN_P0F_INIT(v)
#define | GPIO1PIN_P0F_INITIN(v)
#define | GPIO1PIN_P0F_INITOUT(v)
#define | GPIO1PIN_NP0F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P0F)) )
#define | GPIO1PIN_NP0F_PUT(v) ( bFM0P_GPIO_PDOR0_P0F=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP0F_INIT(v)
#define | GPIO1PIN_NP0F_INITIN(v)
#define | GPIO1PIN_NP0F_INITOUT(v)
#define | GPIO1PIN_P10_GET ( bFM0P_GPIO_PDIR1_P10 )
#define | GPIO1PIN_P10_PUT(v) ( bFM0P_GPIO_PDOR1_P10=(v) )
#define | GPIO1PIN_P10_INIT(v)
#define | GPIO1PIN_P10_INITIN(v)
#define | GPIO1PIN_P10_INITOUT(v)
#define | GPIO1PIN_NP10_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P10)) )
#define | GPIO1PIN_NP10_PUT(v) ( bFM0P_GPIO_PDOR1_P10=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP10_INIT(v)
#define | GPIO1PIN_NP10_INITIN(v)
#define | GPIO1PIN_NP10_INITOUT(v)
#define | GPIO1PIN_P11_GET ( bFM0P_GPIO_PDIR1_P11 )
#define | GPIO1PIN_P11_PUT(v) ( bFM0P_GPIO_PDOR1_P11=(v) )
#define | GPIO1PIN_P11_INIT(v)
#define | GPIO1PIN_P11_INITIN(v)
#define | GPIO1PIN_P11_INITOUT(v)
#define | GPIO1PIN_NP11_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P11)) )
#define | GPIO1PIN_NP11_PUT(v) ( bFM0P_GPIO_PDOR1_P11=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP11_INIT(v)
#define | GPIO1PIN_NP11_INITIN(v)
#define | GPIO1PIN_NP11_INITOUT(v)
#define | GPIO1PIN_P12_GET ( bFM0P_GPIO_PDIR1_P12 )
#define | GPIO1PIN_P12_PUT(v) ( bFM0P_GPIO_PDOR1_P12=(v) )
#define | GPIO1PIN_P12_INIT(v)
#define | GPIO1PIN_P12_INITIN(v)
#define | GPIO1PIN_P12_INITOUT(v)
#define | GPIO1PIN_NP12_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P12)) )
#define | GPIO1PIN_NP12_PUT(v) ( bFM0P_GPIO_PDOR1_P12=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP12_INIT(v)
#define | GPIO1PIN_NP12_INITIN(v)
#define | GPIO1PIN_NP12_INITOUT(v)
#define | GPIO1PIN_P13_GET ( bFM0P_GPIO_PDIR1_P13 )
#define | GPIO1PIN_P13_PUT(v) ( bFM0P_GPIO_PDOR1_P13=(v) )
#define | GPIO1PIN_P13_INIT(v)
#define | GPIO1PIN_P13_INITIN(v)
#define | GPIO1PIN_P13_INITOUT(v)
#define | GPIO1PIN_NP13_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P13)) )
#define | GPIO1PIN_NP13_PUT(v) ( bFM0P_GPIO_PDOR1_P13=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP13_INIT(v)
#define | GPIO1PIN_NP13_INITIN(v)
#define | GPIO1PIN_NP13_INITOUT(v)
#define | GPIO1PIN_P14_GET ( bFM0P_GPIO_PDIR1_P14 )
#define | GPIO1PIN_P14_PUT(v) ( bFM0P_GPIO_PDOR1_P14=(v) )
#define | GPIO1PIN_P14_INIT(v)
#define | GPIO1PIN_P14_INITIN(v)
#define | GPIO1PIN_P14_INITOUT(v)
#define | GPIO1PIN_NP14_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P14)) )
#define | GPIO1PIN_NP14_PUT(v) ( bFM0P_GPIO_PDOR1_P14=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP14_INIT(v)
#define | GPIO1PIN_NP14_INITIN(v)
#define | GPIO1PIN_NP14_INITOUT(v)
#define | GPIO1PIN_P15_GET ( bFM0P_GPIO_PDIR1_P15 )
#define | GPIO1PIN_P15_PUT(v) ( bFM0P_GPIO_PDOR1_P15=(v) )
#define | GPIO1PIN_P15_INIT(v)
#define | GPIO1PIN_P15_INITIN(v)
#define | GPIO1PIN_P15_INITOUT(v)
#define | GPIO1PIN_NP15_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P15)) )
#define | GPIO1PIN_NP15_PUT(v) ( bFM0P_GPIO_PDOR1_P15=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP15_INIT(v)
#define | GPIO1PIN_NP15_INITIN(v)
#define | GPIO1PIN_NP15_INITOUT(v)
#define | GPIO1PIN_P21_GET ( bFM0P_GPIO_PDIR2_P21 )
#define | GPIO1PIN_P21_PUT(v) ( bFM0P_GPIO_PDOR2_P21=(v) )
#define | GPIO1PIN_P21_INIT(v)
#define | GPIO1PIN_P21_INITIN(v)
#define | GPIO1PIN_P21_INITOUT(v)
#define | GPIO1PIN_NP21_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P21)) )
#define | GPIO1PIN_NP21_PUT(v) ( bFM0P_GPIO_PDOR2_P21=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP21_INIT(v)
#define | GPIO1PIN_NP21_INITIN(v)
#define | GPIO1PIN_NP21_INITOUT(v)
#define | GPIO1PIN_P22_GET ( bFM0P_GPIO_PDIR2_P22 )
#define | GPIO1PIN_P22_PUT(v) ( bFM0P_GPIO_PDOR2_P22=(v) )
#define | GPIO1PIN_P22_INIT(v)
#define | GPIO1PIN_P22_INITIN(v)
#define | GPIO1PIN_P22_INITOUT(v)
#define | GPIO1PIN_NP22_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P22)) )
#define | GPIO1PIN_NP22_PUT(v) ( bFM0P_GPIO_PDOR2_P22=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP22_INIT(v)
#define | GPIO1PIN_NP22_INITIN(v)
#define | GPIO1PIN_NP22_INITOUT(v)
#define | GPIO1PIN_P23_GET ( bFM0P_GPIO_PDIR2_P23 )
#define | GPIO1PIN_P23_PUT(v) ( bFM0P_GPIO_PDOR2_P23=(v) )
#define | GPIO1PIN_P23_INIT(v)
#define | GPIO1PIN_P23_INITIN(v)
#define | GPIO1PIN_P23_INITOUT(v)
#define | GPIO1PIN_NP23_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P23)) )
#define | GPIO1PIN_NP23_PUT(v) ( bFM0P_GPIO_PDOR2_P23=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP23_INIT(v)
#define | GPIO1PIN_NP23_INITIN(v)
#define | GPIO1PIN_NP23_INITOUT(v)
#define | GPIO1PIN_P39_GET ( bFM0P_GPIO_PDIR3_P39 )
#define | GPIO1PIN_P39_PUT(v) ( bFM0P_GPIO_PDOR3_P39=(v) )
#define | GPIO1PIN_P39_INIT(v)
#define | GPIO1PIN_P39_INITIN(v)
#define | GPIO1PIN_P39_INITOUT(v)
#define | GPIO1PIN_NP39_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P39)) )
#define | GPIO1PIN_NP39_PUT(v) ( bFM0P_GPIO_PDOR3_P39=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP39_INIT(v)
#define | GPIO1PIN_NP39_INITIN(v)
#define | GPIO1PIN_NP39_INITOUT(v)
#define | GPIO1PIN_P3A_GET ( bFM0P_GPIO_PDIR3_P3A )
#define | GPIO1PIN_P3A_PUT(v) ( bFM0P_GPIO_PDOR3_P3A=(v) )
#define | GPIO1PIN_P3A_INIT(v)
#define | GPIO1PIN_P3A_INITIN(v)
#define | GPIO1PIN_P3A_INITOUT(v)
#define | GPIO1PIN_NP3A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3A)) )
#define | GPIO1PIN_NP3A_PUT(v) ( bFM0P_GPIO_PDOR3_P3A=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3A_INIT(v)
#define | GPIO1PIN_NP3A_INITIN(v)
#define | GPIO1PIN_NP3A_INITOUT(v)
#define | GPIO1PIN_P3B_GET ( bFM0P_GPIO_PDIR3_P3B )
#define | GPIO1PIN_P3B_PUT(v) ( bFM0P_GPIO_PDOR3_P3B=(v) )
#define | GPIO1PIN_P3B_INIT(v)
#define | GPIO1PIN_P3B_INITIN(v)
#define | GPIO1PIN_P3B_INITOUT(v)
#define | GPIO1PIN_NP3B_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3B)) )
#define | GPIO1PIN_NP3B_PUT(v) ( bFM0P_GPIO_PDOR3_P3B=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3B_INIT(v)
#define | GPIO1PIN_NP3B_INITIN(v)
#define | GPIO1PIN_NP3B_INITOUT(v)
#define | GPIO1PIN_P3C_GET ( bFM0P_GPIO_PDIR3_P3C )
#define | GPIO1PIN_P3C_PUT(v) ( bFM0P_GPIO_PDOR3_P3C=(v) )
#define | GPIO1PIN_P3C_INIT(v)
#define | GPIO1PIN_P3C_INITIN(v)
#define | GPIO1PIN_P3C_INITOUT(v)
#define | GPIO1PIN_NP3C_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3C)) )
#define | GPIO1PIN_NP3C_PUT(v) ( bFM0P_GPIO_PDOR3_P3C=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3C_INIT(v)
#define | GPIO1PIN_NP3C_INITIN(v)
#define | GPIO1PIN_NP3C_INITOUT(v)
#define | GPIO1PIN_P3D_GET ( bFM0P_GPIO_PDIR3_P3D )
#define | GPIO1PIN_P3D_PUT(v) ( bFM0P_GPIO_PDOR3_P3D=(v) )
#define | GPIO1PIN_P3D_INIT(v)
#define | GPIO1PIN_P3D_INITIN(v)
#define | GPIO1PIN_P3D_INITOUT(v)
#define | GPIO1PIN_NP3D_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3D)) )
#define | GPIO1PIN_NP3D_PUT(v) ( bFM0P_GPIO_PDOR3_P3D=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3D_INIT(v)
#define | GPIO1PIN_NP3D_INITIN(v)
#define | GPIO1PIN_NP3D_INITOUT(v)
#define | GPIO1PIN_P3E_GET ( bFM0P_GPIO_PDIR3_P3E )
#define | GPIO1PIN_P3E_PUT(v) ( bFM0P_GPIO_PDOR3_P3E=(v) )
#define | GPIO1PIN_P3E_INIT(v)
#define | GPIO1PIN_P3E_INITIN(v)
#define | GPIO1PIN_P3E_INITOUT(v)
#define | GPIO1PIN_NP3E_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3E)) )
#define | GPIO1PIN_NP3E_PUT(v) ( bFM0P_GPIO_PDOR3_P3E=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3E_INIT(v)
#define | GPIO1PIN_NP3E_INITIN(v)
#define | GPIO1PIN_NP3E_INITOUT(v)
#define | GPIO1PIN_P3F_GET ( bFM0P_GPIO_PDIR3_P3F )
#define | GPIO1PIN_P3F_PUT(v) ( bFM0P_GPIO_PDOR3_P3F=(v) )
#define | GPIO1PIN_P3F_INIT(v)
#define | GPIO1PIN_P3F_INITIN(v)
#define | GPIO1PIN_P3F_INITOUT(v)
#define | GPIO1PIN_NP3F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3F)) )
#define | GPIO1PIN_NP3F_PUT(v) ( bFM0P_GPIO_PDOR3_P3F=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP3F_INIT(v)
#define | GPIO1PIN_NP3F_INITIN(v)
#define | GPIO1PIN_NP3F_INITOUT(v)
#define | GPIO1PIN_P46_GET ( bFM0P_GPIO_PDIR4_P46 )
#define | GPIO1PIN_P46_PUT(v) ( bFM0P_GPIO_PDOR4_P46=(v) )
#define | GPIO1PIN_P46_INIT(v)
#define | GPIO1PIN_P46_INITIN(v)
#define | GPIO1PIN_P46_INITOUT(v)
#define | GPIO1PIN_NP46_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P46)) )
#define | GPIO1PIN_NP46_PUT(v) ( bFM0P_GPIO_PDOR4_P46=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP46_INIT(v)
#define | GPIO1PIN_NP46_INITIN(v)
#define | GPIO1PIN_NP46_INITOUT(v)
#define | GPIO1PIN_P47_GET ( bFM0P_GPIO_PDIR4_P47 )
#define | GPIO1PIN_P47_PUT(v) ( bFM0P_GPIO_PDOR4_P47=(v) )
#define | GPIO1PIN_P47_INIT(v)
#define | GPIO1PIN_P47_INITIN(v)
#define | GPIO1PIN_P47_INITOUT(v)
#define | GPIO1PIN_NP47_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P47)) )
#define | GPIO1PIN_NP47_PUT(v) ( bFM0P_GPIO_PDOR4_P47=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP47_INIT(v)
#define | GPIO1PIN_NP47_INITIN(v)
#define | GPIO1PIN_NP47_INITOUT(v)
#define | GPIO1PIN_P49_GET ( bFM0P_GPIO_PDIR4_P49 )
#define | GPIO1PIN_P49_PUT(v) ( bFM0P_GPIO_PDOR4_P49=(v) )
#define | GPIO1PIN_P49_INIT(v)
#define | GPIO1PIN_P49_INITIN(v)
#define | GPIO1PIN_P49_INITOUT(v)
#define | GPIO1PIN_NP49_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P49)) )
#define | GPIO1PIN_NP49_PUT(v) ( bFM0P_GPIO_PDOR4_P49=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP49_INIT(v)
#define | GPIO1PIN_NP49_INITIN(v)
#define | GPIO1PIN_NP49_INITOUT(v)
#define | GPIO1PIN_P4A_GET ( bFM0P_GPIO_PDIR4_P4A )
#define | GPIO1PIN_P4A_PUT(v) ( bFM0P_GPIO_PDOR4_P4A=(v) )
#define | GPIO1PIN_P4A_INIT(v)
#define | GPIO1PIN_P4A_INITIN(v)
#define | GPIO1PIN_P4A_INITOUT(v)
#define | GPIO1PIN_NP4A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P4A)) )
#define | GPIO1PIN_NP4A_PUT(v) ( bFM0P_GPIO_PDOR4_P4A=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP4A_INIT(v)
#define | GPIO1PIN_NP4A_INITIN(v)
#define | GPIO1PIN_NP4A_INITOUT(v)
#define | GPIO1PIN_P50_GET ( bFM0P_GPIO_PDIR5_P50 )
#define | GPIO1PIN_P50_PUT(v) ( bFM0P_GPIO_PDOR5_P50=(v) )
#define | GPIO1PIN_P50_INIT(v)
#define | GPIO1PIN_P50_INITIN(v)
#define | GPIO1PIN_P50_INITOUT(v)
#define | GPIO1PIN_NP50_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P50)) )
#define | GPIO1PIN_NP50_PUT(v) ( bFM0P_GPIO_PDOR5_P50=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP50_INIT(v)
#define | GPIO1PIN_NP50_INITIN(v)
#define | GPIO1PIN_NP50_INITOUT(v)
#define | GPIO1PIN_P51_GET ( bFM0P_GPIO_PDIR5_P51 )
#define | GPIO1PIN_P51_PUT(v) ( bFM0P_GPIO_PDOR5_P51=(v) )
#define | GPIO1PIN_P51_INIT(v)
#define | GPIO1PIN_P51_INITIN(v)
#define | GPIO1PIN_P51_INITOUT(v)
#define | GPIO1PIN_NP51_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P51)) )
#define | GPIO1PIN_NP51_PUT(v) ( bFM0P_GPIO_PDOR5_P51=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP51_INIT(v)
#define | GPIO1PIN_NP51_INITIN(v)
#define | GPIO1PIN_NP51_INITOUT(v)
#define | GPIO1PIN_P52_GET ( bFM0P_GPIO_PDIR5_P52 )
#define | GPIO1PIN_P52_PUT(v) ( bFM0P_GPIO_PDOR5_P52=(v) )
#define | GPIO1PIN_P52_INIT(v)
#define | GPIO1PIN_P52_INITIN(v)
#define | GPIO1PIN_P52_INITOUT(v)
#define | GPIO1PIN_NP52_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P52)) )
#define | GPIO1PIN_NP52_PUT(v) ( bFM0P_GPIO_PDOR5_P52=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP52_INIT(v)
#define | GPIO1PIN_NP52_INITIN(v)
#define | GPIO1PIN_NP52_INITOUT(v)
#define | GPIO1PIN_P60_GET ( bFM0P_GPIO_PDIR6_P60 )
#define | GPIO1PIN_P60_PUT(v) ( bFM0P_GPIO_PDOR6_P60=(v) )
#define | GPIO1PIN_P60_INIT(v)
#define | GPIO1PIN_P60_INITIN(v)
#define | GPIO1PIN_P60_INITOUT(v)
#define | GPIO1PIN_NP60_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P60)) )
#define | GPIO1PIN_NP60_PUT(v) ( bFM0P_GPIO_PDOR6_P60=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP60_INIT(v)
#define | GPIO1PIN_NP60_INITIN(v)
#define | GPIO1PIN_NP60_INITOUT(v)
#define | GPIO1PIN_P61_GET ( bFM0P_GPIO_PDIR6_P61 )
#define | GPIO1PIN_P61_PUT(v) ( bFM0P_GPIO_PDOR6_P61=(v) )
#define | GPIO1PIN_P61_INIT(v)
#define | GPIO1PIN_P61_INITIN(v)
#define | GPIO1PIN_P61_INITOUT(v)
#define | GPIO1PIN_NP61_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P61)) )
#define | GPIO1PIN_NP61_PUT(v) ( bFM0P_GPIO_PDOR6_P61=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP61_INIT(v)
#define | GPIO1PIN_NP61_INITIN(v)
#define | GPIO1PIN_NP61_INITOUT(v)
#define | GPIO1PIN_P80_GET ( bFM0P_GPIO_PDIR8_P80 )
#define | GPIO1PIN_P80_PUT(v) ( bFM0P_GPIO_PDOR8_P80=(v) )
#define | GPIO1PIN_P80_INIT(v)
#define | GPIO1PIN_P80_INITIN(v)
#define | GPIO1PIN_P80_INITOUT(v)
#define | GPIO1PIN_NP80_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P80)) )
#define | GPIO1PIN_NP80_PUT(v) ( bFM0P_GPIO_PDOR8_P80=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP80_INIT(v)
#define | GPIO1PIN_NP80_INITIN(v)
#define | GPIO1PIN_NP80_INITOUT(v)
#define | GPIO1PIN_P81_GET ( bFM0P_GPIO_PDIR8_P81 )
#define | GPIO1PIN_P81_PUT(v) ( bFM0P_GPIO_PDOR8_P81=(v) )
#define | GPIO1PIN_P81_INIT(v)
#define | GPIO1PIN_P81_INITIN(v)
#define | GPIO1PIN_P81_INITOUT(v)
#define | GPIO1PIN_NP81_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P81)) )
#define | GPIO1PIN_NP81_PUT(v) ( bFM0P_GPIO_PDOR8_P81=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP81_INIT(v)
#define | GPIO1PIN_NP81_INITIN(v)
#define | GPIO1PIN_NP81_INITOUT(v)
#define | GPIO1PIN_P82_GET ( bFM0P_GPIO_PDIR8_P82 )
#define | GPIO1PIN_P82_PUT(v) ( bFM0P_GPIO_PDOR8_P82=(v) )
#define | GPIO1PIN_P82_INIT(v)
#define | GPIO1PIN_P82_INITIN(v)
#define | GPIO1PIN_P82_INITOUT(v)
#define | GPIO1PIN_NP82_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P82)) )
#define | GPIO1PIN_NP82_PUT(v) ( bFM0P_GPIO_PDOR8_P82=(uint32_t)(!(v)) )
#define | GPIO1PIN_NP82_INIT(v)
#define | GPIO1PIN_NP82_INITIN(v)
#define | GPIO1PIN_NP82_INITOUT(v)
#define | GPIO1PIN_PE0_GET ( bFM0P_GPIO_PDIRE_PE0 )
#define | GPIO1PIN_PE0_PUT(v) ( bFM0P_GPIO_PDORE_PE0=(v) )
#define | GPIO1PIN_PE0_INIT(v)
#define | GPIO1PIN_PE0_INITIN(v)
#define | GPIO1PIN_PE0_INITOUT(v)
#define | GPIO1PIN_NPE0_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE0)) )
#define | GPIO1PIN_NPE0_PUT(v) ( bFM0P_GPIO_PDORE_PE0=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE0_INIT(v)
#define | GPIO1PIN_NPE0_INITIN(v)
#define | GPIO1PIN_NPE0_INITOUT(v)
#define | GPIO1PIN_PE2_GET ( bFM0P_GPIO_PDIRE_PE2 )
#define | GPIO1PIN_PE2_PUT(v) ( bFM0P_GPIO_PDORE_PE2=(v) )
#define | GPIO1PIN_PE2_INIT(v)
#define | GPIO1PIN_PE2_INITIN(v)
#define | GPIO1PIN_PE2_INITOUT(v)
#define | GPIO1PIN_NPE2_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE2)) )
#define | GPIO1PIN_NPE2_PUT(v) ( bFM0P_GPIO_PDORE_PE2=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE2_INIT(v)
#define | GPIO1PIN_NPE2_INITIN(v)
#define | GPIO1PIN_NPE2_INITOUT(v)
#define | GPIO1PIN_PE3_GET ( bFM0P_GPIO_PDIRE_PE3 )
#define | GPIO1PIN_PE3_PUT(v) ( bFM0P_GPIO_PDORE_PE3=(v) )
#define | GPIO1PIN_PE3_INIT(v)
#define | GPIO1PIN_PE3_INITIN(v)
#define | GPIO1PIN_PE3_INITOUT(v)
#define | GPIO1PIN_NPE3_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE3)) )
#define | GPIO1PIN_NPE3_PUT(v) ( bFM0P_GPIO_PDORE_PE3=(uint32_t)(!(v)) )
#define | GPIO1PIN_NPE3_INIT(v)
#define | GPIO1PIN_NPE3_INITIN(v)
#define | GPIO1PIN_NPE3_INITOUT(v)
#define | FGPIO1PIN_P00_GET ( FM0P_FASTIO->FPDIR0_f.P00 )
#define | FGPIO1PIN_P00_PUT(v) ( bFM0P_GPIO_FPDOR0_P00=(v) )
#define | FGPIO1PIN_P00_INIT(v)
#define | FGPIO1PIN_P00_INITIN(v)
#define | FGPIO1PIN_P00_INITOUT(v)
#define | FGPIO1PIN_NP00_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P00)) )
#define | FGPIO1PIN_NP00_PUT(v) ( bFM0P_GPIO_FPDOR0_P00=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP00_INIT(v)
#define | FGPIO1PIN_NP00_INITIN(v)
#define | FGPIO1PIN_NP00_INITOUT(v)
#define | FGPIO1PIN_P01_GET ( FM0P_FASTIO->FPDIR0_f.P01 )
#define | FGPIO1PIN_P01_PUT(v) ( bFM0P_GPIO_FPDOR0_P01=(v) )
#define | FGPIO1PIN_P01_INIT(v)
#define | FGPIO1PIN_P01_INITIN(v)
#define | FGPIO1PIN_P01_INITOUT(v)
#define | FGPIO1PIN_NP01_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P01)) )
#define | FGPIO1PIN_NP01_PUT(v) ( bFM0P_GPIO_FPDOR0_P01=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP01_INIT(v)
#define | FGPIO1PIN_NP01_INITIN(v)
#define | FGPIO1PIN_NP01_INITOUT(v)
#define | FGPIO1PIN_P02_GET ( FM0P_FASTIO->FPDIR0_f.P02 )
#define | FGPIO1PIN_P02_PUT(v) ( bFM0P_GPIO_FPDOR0_P02=(v) )
#define | FGPIO1PIN_P02_INIT(v)
#define | FGPIO1PIN_P02_INITIN(v)
#define | FGPIO1PIN_P02_INITOUT(v)
#define | FGPIO1PIN_NP02_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P02)) )
#define | FGPIO1PIN_NP02_PUT(v) ( bFM0P_GPIO_FPDOR0_P02=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP02_INIT(v)
#define | FGPIO1PIN_NP02_INITIN(v)
#define | FGPIO1PIN_NP02_INITOUT(v)
#define | FGPIO1PIN_P03_GET ( FM0P_FASTIO->FPDIR0_f.P03 )
#define | FGPIO1PIN_P03_PUT(v) ( bFM0P_GPIO_FPDOR0_P03=(v) )
#define | FGPIO1PIN_P03_INIT(v)
#define | FGPIO1PIN_P03_INITIN(v)
#define | FGPIO1PIN_P03_INITOUT(v)
#define | FGPIO1PIN_NP03_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P03)) )
#define | FGPIO1PIN_NP03_PUT(v) ( bFM0P_GPIO_FPDOR0_P03=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP03_INIT(v)
#define | FGPIO1PIN_NP03_INITIN(v)
#define | FGPIO1PIN_NP03_INITOUT(v)
#define | FGPIO1PIN_P04_GET ( FM0P_FASTIO->FPDIR0_f.P04 )
#define | FGPIO1PIN_P04_PUT(v) ( bFM0P_GPIO_FPDOR0_P04=(v) )
#define | FGPIO1PIN_P04_INIT(v)
#define | FGPIO1PIN_P04_INITIN(v)
#define | FGPIO1PIN_P04_INITOUT(v)
#define | FGPIO1PIN_NP04_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P04)) )
#define | FGPIO1PIN_NP04_PUT(v) ( bFM0P_GPIO_FPDOR0_P04=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP04_INIT(v)
#define | FGPIO1PIN_NP04_INITIN(v)
#define | FGPIO1PIN_NP04_INITOUT(v)
#define | FGPIO1PIN_P0F_GET ( FM0P_FASTIO->FPDIR0_f.P0F )
#define | FGPIO1PIN_P0F_PUT(v) ( bFM0P_GPIO_FPDOR0_P0F=(v) )
#define | FGPIO1PIN_P0F_INIT(v)
#define | FGPIO1PIN_P0F_INITIN(v)
#define | FGPIO1PIN_P0F_INITOUT(v)
#define | FGPIO1PIN_NP0F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P0F)) )
#define | FGPIO1PIN_NP0F_PUT(v) ( bFM0P_GPIO_FPDOR0_P0F=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP0F_INIT(v)
#define | FGPIO1PIN_NP0F_INITIN(v)
#define | FGPIO1PIN_NP0F_INITOUT(v)
#define | FGPIO1PIN_P10_GET ( FM0P_FASTIO->FPDIR1_f.P10 )
#define | FGPIO1PIN_P10_PUT(v) ( bFM0P_GPIO_FPDOR1_P10=(v) )
#define | FGPIO1PIN_P10_INIT(v)
#define | FGPIO1PIN_P10_INITIN(v)
#define | FGPIO1PIN_P10_INITOUT(v)
#define | FGPIO1PIN_NP10_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P10)) )
#define | FGPIO1PIN_NP10_PUT(v) ( bFM0P_GPIO_FPDOR1_P10=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP10_INIT(v)
#define | FGPIO1PIN_NP10_INITIN(v)
#define | FGPIO1PIN_NP10_INITOUT(v)
#define | FGPIO1PIN_P11_GET ( FM0P_FASTIO->FPDIR1_f.P11 )
#define | FGPIO1PIN_P11_PUT(v) ( bFM0P_GPIO_FPDOR1_P11=(v) )
#define | FGPIO1PIN_P11_INIT(v)
#define | FGPIO1PIN_P11_INITIN(v)
#define | FGPIO1PIN_P11_INITOUT(v)
#define | FGPIO1PIN_NP11_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P11)) )
#define | FGPIO1PIN_NP11_PUT(v) ( bFM0P_GPIO_FPDOR1_P11=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP11_INIT(v)
#define | FGPIO1PIN_NP11_INITIN(v)
#define | FGPIO1PIN_NP11_INITOUT(v)
#define | FGPIO1PIN_P12_GET ( FM0P_FASTIO->FPDIR1_f.P12 )
#define | FGPIO1PIN_P12_PUT(v) ( bFM0P_GPIO_FPDOR1_P12=(v) )
#define | FGPIO1PIN_P12_INIT(v)
#define | FGPIO1PIN_P12_INITIN(v)
#define | FGPIO1PIN_P12_INITOUT(v)
#define | FGPIO1PIN_NP12_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P12)) )
#define | FGPIO1PIN_NP12_PUT(v) ( bFM0P_GPIO_FPDOR1_P12=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP12_INIT(v)
#define | FGPIO1PIN_NP12_INITIN(v)
#define | FGPIO1PIN_NP12_INITOUT(v)
#define | FGPIO1PIN_P13_GET ( FM0P_FASTIO->FPDIR1_f.P13 )
#define | FGPIO1PIN_P13_PUT(v) ( bFM0P_GPIO_FPDOR1_P13=(v) )
#define | FGPIO1PIN_P13_INIT(v)
#define | FGPIO1PIN_P13_INITIN(v)
#define | FGPIO1PIN_P13_INITOUT(v)
#define | FGPIO1PIN_NP13_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P13)) )
#define | FGPIO1PIN_NP13_PUT(v) ( bFM0P_GPIO_FPDOR1_P13=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP13_INIT(v)
#define | FGPIO1PIN_NP13_INITIN(v)
#define | FGPIO1PIN_NP13_INITOUT(v)
#define | FGPIO1PIN_P14_GET ( FM0P_FASTIO->FPDIR1_f.P14 )
#define | FGPIO1PIN_P14_PUT(v) ( bFM0P_GPIO_FPDOR1_P14=(v) )
#define | FGPIO1PIN_P14_INIT(v)
#define | FGPIO1PIN_P14_INITIN(v)
#define | FGPIO1PIN_P14_INITOUT(v)
#define | FGPIO1PIN_NP14_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P14)) )
#define | FGPIO1PIN_NP14_PUT(v) ( bFM0P_GPIO_FPDOR1_P14=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP14_INIT(v)
#define | FGPIO1PIN_NP14_INITIN(v)
#define | FGPIO1PIN_NP14_INITOUT(v)
#define | FGPIO1PIN_P15_GET ( FM0P_FASTIO->FPDIR1_f.P15 )
#define | FGPIO1PIN_P15_PUT(v) ( bFM0P_GPIO_FPDOR1_P15=(v) )
#define | FGPIO1PIN_P15_INIT(v)
#define | FGPIO1PIN_P15_INITIN(v)
#define | FGPIO1PIN_P15_INITOUT(v)
#define | FGPIO1PIN_NP15_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P15)) )
#define | FGPIO1PIN_NP15_PUT(v) ( bFM0P_GPIO_FPDOR1_P15=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP15_INIT(v)
#define | FGPIO1PIN_NP15_INITIN(v)
#define | FGPIO1PIN_NP15_INITOUT(v)
#define | FGPIO1PIN_P21_GET ( FM0P_FASTIO->FPDIR2_f.P21 )
#define | FGPIO1PIN_P21_PUT(v) ( bFM0P_GPIO_FPDOR2_P21=(v) )
#define | FGPIO1PIN_P21_INIT(v)
#define | FGPIO1PIN_P21_INITIN(v)
#define | FGPIO1PIN_P21_INITOUT(v)
#define | FGPIO1PIN_NP21_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P21)) )
#define | FGPIO1PIN_NP21_PUT(v) ( bFM0P_GPIO_FPDOR2_P21=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP21_INIT(v)
#define | FGPIO1PIN_NP21_INITIN(v)
#define | FGPIO1PIN_NP21_INITOUT(v)
#define | FGPIO1PIN_P22_GET ( FM0P_FASTIO->FPDIR2_f.P22 )
#define | FGPIO1PIN_P22_PUT(v) ( bFM0P_GPIO_FPDOR2_P22=(v) )
#define | FGPIO1PIN_P22_INIT(v)
#define | FGPIO1PIN_P22_INITIN(v)
#define | FGPIO1PIN_P22_INITOUT(v)
#define | FGPIO1PIN_NP22_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P22)) )
#define | FGPIO1PIN_NP22_PUT(v) ( bFM0P_GPIO_FPDOR2_P22=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP22_INIT(v)
#define | FGPIO1PIN_NP22_INITIN(v)
#define | FGPIO1PIN_NP22_INITOUT(v)
#define | FGPIO1PIN_P23_GET ( FM0P_FASTIO->FPDIR2_f.P23 )
#define | FGPIO1PIN_P23_PUT(v) ( bFM0P_GPIO_FPDOR2_P23=(v) )
#define | FGPIO1PIN_P23_INIT(v)
#define | FGPIO1PIN_P23_INITIN(v)
#define | FGPIO1PIN_P23_INITOUT(v)
#define | FGPIO1PIN_NP23_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P23)) )
#define | FGPIO1PIN_NP23_PUT(v) ( bFM0P_GPIO_FPDOR2_P23=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP23_INIT(v)
#define | FGPIO1PIN_NP23_INITIN(v)
#define | FGPIO1PIN_NP23_INITOUT(v)
#define | FGPIO1PIN_P39_GET ( FM0P_FASTIO->FPDIR3_f.P39 )
#define | FGPIO1PIN_P39_PUT(v) ( bFM0P_GPIO_FPDOR3_P39=(v) )
#define | FGPIO1PIN_P39_INIT(v)
#define | FGPIO1PIN_P39_INITIN(v)
#define | FGPIO1PIN_P39_INITOUT(v)
#define | FGPIO1PIN_NP39_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P39)) )
#define | FGPIO1PIN_NP39_PUT(v) ( bFM0P_GPIO_FPDOR3_P39=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP39_INIT(v)
#define | FGPIO1PIN_NP39_INITIN(v)
#define | FGPIO1PIN_NP39_INITOUT(v)
#define | FGPIO1PIN_P3A_GET ( FM0P_FASTIO->FPDIR3_f.P3A )
#define | FGPIO1PIN_P3A_PUT(v) ( bFM0P_GPIO_FPDOR3_P3A=(v) )
#define | FGPIO1PIN_P3A_INIT(v)
#define | FGPIO1PIN_P3A_INITIN(v)
#define | FGPIO1PIN_P3A_INITOUT(v)
#define | FGPIO1PIN_NP3A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3A)) )
#define | FGPIO1PIN_NP3A_PUT(v) ( bFM0P_GPIO_FPDOR3_P3A=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3A_INIT(v)
#define | FGPIO1PIN_NP3A_INITIN(v)
#define | FGPIO1PIN_NP3A_INITOUT(v)
#define | FGPIO1PIN_P3B_GET ( FM0P_FASTIO->FPDIR3_f.P3B )
#define | FGPIO1PIN_P3B_PUT(v) ( bFM0P_GPIO_FPDOR3_P3B=(v) )
#define | FGPIO1PIN_P3B_INIT(v)
#define | FGPIO1PIN_P3B_INITIN(v)
#define | FGPIO1PIN_P3B_INITOUT(v)
#define | FGPIO1PIN_NP3B_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3B)) )
#define | FGPIO1PIN_NP3B_PUT(v) ( bFM0P_GPIO_FPDOR3_P3B=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3B_INIT(v)
#define | FGPIO1PIN_NP3B_INITIN(v)
#define | FGPIO1PIN_NP3B_INITOUT(v)
#define | FGPIO1PIN_P3C_GET ( FM0P_FASTIO->FPDIR3_f.P3C )
#define | FGPIO1PIN_P3C_PUT(v) ( bFM0P_GPIO_FPDOR3_P3C=(v) )
#define | FGPIO1PIN_P3C_INIT(v)
#define | FGPIO1PIN_P3C_INITIN(v)
#define | FGPIO1PIN_P3C_INITOUT(v)
#define | FGPIO1PIN_NP3C_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3C)) )
#define | FGPIO1PIN_NP3C_PUT(v) ( bFM0P_GPIO_FPDOR3_P3C=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3C_INIT(v)
#define | FGPIO1PIN_NP3C_INITIN(v)
#define | FGPIO1PIN_NP3C_INITOUT(v)
#define | FGPIO1PIN_P3D_GET ( FM0P_FASTIO->FPDIR3_f.P3D )
#define | FGPIO1PIN_P3D_PUT(v) ( bFM0P_GPIO_FPDOR3_P3D=(v) )
#define | FGPIO1PIN_P3D_INIT(v)
#define | FGPIO1PIN_P3D_INITIN(v)
#define | FGPIO1PIN_P3D_INITOUT(v)
#define | FGPIO1PIN_NP3D_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3D)) )
#define | FGPIO1PIN_NP3D_PUT(v) ( bFM0P_GPIO_FPDOR3_P3D=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3D_INIT(v)
#define | FGPIO1PIN_NP3D_INITIN(v)
#define | FGPIO1PIN_NP3D_INITOUT(v)
#define | FGPIO1PIN_P3E_GET ( FM0P_FASTIO->FPDIR3_f.P3E )
#define | FGPIO1PIN_P3E_PUT(v) ( bFM0P_GPIO_FPDOR3_P3E=(v) )
#define | FGPIO1PIN_P3E_INIT(v)
#define | FGPIO1PIN_P3E_INITIN(v)
#define | FGPIO1PIN_P3E_INITOUT(v)
#define | FGPIO1PIN_NP3E_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3E)) )
#define | FGPIO1PIN_NP3E_PUT(v) ( bFM0P_GPIO_FPDOR3_P3E=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3E_INIT(v)
#define | FGPIO1PIN_NP3E_INITIN(v)
#define | FGPIO1PIN_NP3E_INITOUT(v)
#define | FGPIO1PIN_P3F_GET ( FM0P_FASTIO->FPDIR3_f.P3F )
#define | FGPIO1PIN_P3F_PUT(v) ( bFM0P_GPIO_FPDOR3_P3F=(v) )
#define | FGPIO1PIN_P3F_INIT(v)
#define | FGPIO1PIN_P3F_INITIN(v)
#define | FGPIO1PIN_P3F_INITOUT(v)
#define | FGPIO1PIN_NP3F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3F)) )
#define | FGPIO1PIN_NP3F_PUT(v) ( bFM0P_GPIO_FPDOR3_P3F=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP3F_INIT(v)
#define | FGPIO1PIN_NP3F_INITIN(v)
#define | FGPIO1PIN_NP3F_INITOUT(v)
#define | FGPIO1PIN_P46_GET ( FM0P_FASTIO->FPDIR4_f.P46 )
#define | FGPIO1PIN_P46_PUT(v) ( bFM0P_GPIO_FPDOR4_P46=(v) )
#define | FGPIO1PIN_P46_INIT(v)
#define | FGPIO1PIN_P46_INITIN(v)
#define | FGPIO1PIN_P46_INITOUT(v)
#define | FGPIO1PIN_NP46_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P46)) )
#define | FGPIO1PIN_NP46_PUT(v) ( bFM0P_GPIO_FPDOR4_P46=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP46_INIT(v)
#define | FGPIO1PIN_NP46_INITIN(v)
#define | FGPIO1PIN_NP46_INITOUT(v)
#define | FGPIO1PIN_P47_GET ( FM0P_FASTIO->FPDIR4_f.P47 )
#define | FGPIO1PIN_P47_PUT(v) ( bFM0P_GPIO_FPDOR4_P47=(v) )
#define | FGPIO1PIN_P47_INIT(v)
#define | FGPIO1PIN_P47_INITIN(v)
#define | FGPIO1PIN_P47_INITOUT(v)
#define | FGPIO1PIN_NP47_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P47)) )
#define | FGPIO1PIN_NP47_PUT(v) ( bFM0P_GPIO_FPDOR4_P47=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP47_INIT(v)
#define | FGPIO1PIN_NP47_INITIN(v)
#define | FGPIO1PIN_NP47_INITOUT(v)
#define | FGPIO1PIN_P49_GET ( FM0P_FASTIO->FPDIR4_f.P49 )
#define | FGPIO1PIN_P49_PUT(v) ( bFM0P_GPIO_FPDOR4_P49=(v) )
#define | FGPIO1PIN_P49_INIT(v)
#define | FGPIO1PIN_P49_INITIN(v)
#define | FGPIO1PIN_P49_INITOUT(v)
#define | FGPIO1PIN_NP49_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P49)) )
#define | FGPIO1PIN_NP49_PUT(v) ( bFM0P_GPIO_FPDOR4_P49=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP49_INIT(v)
#define | FGPIO1PIN_NP49_INITIN(v)
#define | FGPIO1PIN_NP49_INITOUT(v)
#define | FGPIO1PIN_P4A_GET ( FM0P_FASTIO->FPDIR4_f.P4A )
#define | FGPIO1PIN_P4A_PUT(v) ( bFM0P_GPIO_FPDOR4_P4A=(v) )
#define | FGPIO1PIN_P4A_INIT(v)
#define | FGPIO1PIN_P4A_INITIN(v)
#define | FGPIO1PIN_P4A_INITOUT(v)
#define | FGPIO1PIN_NP4A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P4A)) )
#define | FGPIO1PIN_NP4A_PUT(v) ( bFM0P_GPIO_FPDOR4_P4A=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP4A_INIT(v)
#define | FGPIO1PIN_NP4A_INITIN(v)
#define | FGPIO1PIN_NP4A_INITOUT(v)
#define | FGPIO1PIN_P50_GET ( FM0P_FASTIO->FPDIR5_f.P50 )
#define | FGPIO1PIN_P50_PUT(v) ( bFM0P_GPIO_FPDOR5_P50=(v) )
#define | FGPIO1PIN_P50_INIT(v)
#define | FGPIO1PIN_P50_INITIN(v)
#define | FGPIO1PIN_P50_INITOUT(v)
#define | FGPIO1PIN_NP50_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P50)) )
#define | FGPIO1PIN_NP50_PUT(v) ( bFM0P_GPIO_FPDOR5_P50=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP50_INIT(v)
#define | FGPIO1PIN_NP50_INITIN(v)
#define | FGPIO1PIN_NP50_INITOUT(v)
#define | FGPIO1PIN_P51_GET ( FM0P_FASTIO->FPDIR5_f.P51 )
#define | FGPIO1PIN_P51_PUT(v) ( bFM0P_GPIO_FPDOR5_P51=(v) )
#define | FGPIO1PIN_P51_INIT(v)
#define | FGPIO1PIN_P51_INITIN(v)
#define | FGPIO1PIN_P51_INITOUT(v)
#define | FGPIO1PIN_NP51_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P51)) )
#define | FGPIO1PIN_NP51_PUT(v) ( bFM0P_GPIO_FPDOR5_P51=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP51_INIT(v)
#define | FGPIO1PIN_NP51_INITIN(v)
#define | FGPIO1PIN_NP51_INITOUT(v)
#define | FGPIO1PIN_P52_GET ( FM0P_FASTIO->FPDIR5_f.P52 )
#define | FGPIO1PIN_P52_PUT(v) ( bFM0P_GPIO_FPDOR5_P52=(v) )
#define | FGPIO1PIN_P52_INIT(v)
#define | FGPIO1PIN_P52_INITIN(v)
#define | FGPIO1PIN_P52_INITOUT(v)
#define | FGPIO1PIN_NP52_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P52)) )
#define | FGPIO1PIN_NP52_PUT(v) ( bFM0P_GPIO_FPDOR5_P52=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP52_INIT(v)
#define | FGPIO1PIN_NP52_INITIN(v)
#define | FGPIO1PIN_NP52_INITOUT(v)
#define | FGPIO1PIN_P60_GET ( FM0P_FASTIO->FPDIR6_f.P60 )
#define | FGPIO1PIN_P60_PUT(v) ( bFM0P_GPIO_FPDOR6_P60=(v) )
#define | FGPIO1PIN_P60_INIT(v)
#define | FGPIO1PIN_P60_INITIN(v)
#define | FGPIO1PIN_P60_INITOUT(v)
#define | FGPIO1PIN_NP60_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P60)) )
#define | FGPIO1PIN_NP60_PUT(v) ( bFM0P_GPIO_FPDOR6_P60=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP60_INIT(v)
#define | FGPIO1PIN_NP60_INITIN(v)
#define | FGPIO1PIN_NP60_INITOUT(v)
#define | FGPIO1PIN_P61_GET ( FM0P_FASTIO->FPDIR6_f.P61 )
#define | FGPIO1PIN_P61_PUT(v) ( bFM0P_GPIO_FPDOR6_P61=(v) )
#define | FGPIO1PIN_P61_INIT(v)
#define | FGPIO1PIN_P61_INITIN(v)
#define | FGPIO1PIN_P61_INITOUT(v)
#define | FGPIO1PIN_NP61_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P61)) )
#define | FGPIO1PIN_NP61_PUT(v) ( bFM0P_GPIO_FPDOR6_P61=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP61_INIT(v)
#define | FGPIO1PIN_NP61_INITIN(v)
#define | FGPIO1PIN_NP61_INITOUT(v)
#define | FGPIO1PIN_P80_GET ( FM0P_FASTIO->FPDIR8_f.P80 )
#define | FGPIO1PIN_P80_PUT(v) ( bFM0P_GPIO_FPDOR8_P80=(v) )
#define | FGPIO1PIN_P80_INIT(v)
#define | FGPIO1PIN_P80_INITIN(v)
#define | FGPIO1PIN_P80_INITOUT(v)
#define | FGPIO1PIN_NP80_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P80)) )
#define | FGPIO1PIN_NP80_PUT(v) ( bFM0P_GPIO_FPDOR8_P80=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP80_INIT(v)
#define | FGPIO1PIN_NP80_INITIN(v)
#define | FGPIO1PIN_NP80_INITOUT(v)
#define | FGPIO1PIN_P81_GET ( FM0P_FASTIO->FPDIR8_f.P81 )
#define | FGPIO1PIN_P81_PUT(v) ( bFM0P_GPIO_FPDOR8_P81=(v) )
#define | FGPIO1PIN_P81_INIT(v)
#define | FGPIO1PIN_P81_INITIN(v)
#define | FGPIO1PIN_P81_INITOUT(v)
#define | FGPIO1PIN_NP81_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P81)) )
#define | FGPIO1PIN_NP81_PUT(v) ( bFM0P_GPIO_FPDOR8_P81=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP81_INIT(v)
#define | FGPIO1PIN_NP81_INITIN(v)
#define | FGPIO1PIN_NP81_INITOUT(v)
#define | FGPIO1PIN_P82_GET ( FM0P_FASTIO->FPDIR8_f.P82 )
#define | FGPIO1PIN_P82_PUT(v) ( bFM0P_GPIO_FPDOR8_P82=(v) )
#define | FGPIO1PIN_P82_INIT(v)
#define | FGPIO1PIN_P82_INITIN(v)
#define | FGPIO1PIN_P82_INITOUT(v)
#define | FGPIO1PIN_NP82_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P82)) )
#define | FGPIO1PIN_NP82_PUT(v) ( bFM0P_GPIO_FPDOR8_P82=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NP82_INIT(v)
#define | FGPIO1PIN_NP82_INITIN(v)
#define | FGPIO1PIN_NP82_INITOUT(v)
#define | FGPIO1PIN_PE0_GET ( FM0P_FASTIO->FPDIRE_f.PE0 )
#define | FGPIO1PIN_PE0_PUT(v) ( bFM0P_GPIO_FPDORE_PE0=(v) )
#define | FGPIO1PIN_PE0_INIT(v)
#define | FGPIO1PIN_PE0_INITIN(v)
#define | FGPIO1PIN_PE0_INITOUT(v)
#define | FGPIO1PIN_NPE0_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE0)) )
#define | FGPIO1PIN_NPE0_PUT(v) ( bFM0P_GPIO_FPDORE_PE0=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE0_INIT(v)
#define | FGPIO1PIN_NPE0_INITIN(v)
#define | FGPIO1PIN_NPE0_INITOUT(v)
#define | FGPIO1PIN_PE2_GET ( FM0P_FASTIO->FPDIRE_f.PE2 )
#define | FGPIO1PIN_PE2_PUT(v) ( bFM0P_GPIO_FPDORE_PE2=(v) )
#define | FGPIO1PIN_PE2_INIT(v)
#define | FGPIO1PIN_PE2_INITIN(v)
#define | FGPIO1PIN_PE2_INITOUT(v)
#define | FGPIO1PIN_NPE2_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE2)) )
#define | FGPIO1PIN_NPE2_PUT(v) ( bFM0P_GPIO_FPDORE_PE2=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE2_INIT(v)
#define | FGPIO1PIN_NPE2_INITIN(v)
#define | FGPIO1PIN_NPE2_INITOUT(v)
#define | FGPIO1PIN_PE3_GET ( FM0P_FASTIO->FPDIRE_f.PE3 )
#define | FGPIO1PIN_PE3_PUT(v) ( bFM0P_GPIO_FPDORE_PE3=(v) )
#define | FGPIO1PIN_PE3_INIT(v)
#define | FGPIO1PIN_PE3_INITIN(v)
#define | FGPIO1PIN_PE3_INITOUT(v)
#define | FGPIO1PIN_NPE3_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE3)) )
#define | FGPIO1PIN_NPE3_PUT(v) ( bFM0P_GPIO_FPDORE_PE3=(uint8_t)(~(v)) )
#define | FGPIO1PIN_NPE3_INIT(v)
#define | FGPIO1PIN_NPE3_INITIN(v)
#define | FGPIO1PIN_NPE3_INITOUT(v)
#define | SetPinFunc_ADTG_1_ADC0(dummy)
#define | SetPinFunc_ADTG_1_ADC1(dummy)
#define | SetPinFunc_ADTG_1_ADC2(dummy)
#define | SetPinFunc_ADTG_2_ADC0(dummy)
#define | SetPinFunc_ADTG_2_ADC1(dummy)
#define | SetPinFunc_ADTG_2_ADC2(dummy)
#define | SetPinFunc_AIN0_0(dummy)
#define | SetPinFunc_AIN0_1(dummy)
#define | SetPinFunc_AIN0_2(dummy)
#define | SetPinFunc_AIN0_3(dummy)
#define | SetPinFunc_BIN0_0(dummy)
#define | SetPinFunc_BIN0_1(dummy)
#define | SetPinFunc_BIN0_2(dummy)
#define | SetPinFunc_BIN0_3(dummy)
#define | SetPinFunc_CROUT_1(dummy)
#define | SetPinFunc_DTTI0X_0(dummy)
#define | SetPinFunc_DTTI0X_1(dummy)
#define | SetPinFunc_DTTI0X_2(dummy)
#define | SetPinFunc_FRCK0_0(dummy)
#define | SetPinFunc_FRCK0_1(dummy)
#define | SetPinFunc_FRCK0_2(dummy)
#define | SetPinFunc_IC00_0(dummy)
#define | SetPinFunc_IC00_2(dummy)
#define | SetPinFunc_IC01_0(dummy)
#define | SetPinFunc_IC01_1(dummy)
#define | SetPinFunc_IC01_2(dummy)
#define | SetPinFunc_IC02_0(dummy)
#define | SetPinFunc_IC02_1(dummy)
#define | SetPinFunc_IC02_2(dummy)
#define | SetPinFunc_IC03_1(dummy)
#define | SetPinFunc_IC03_2(dummy)
#define | SetPinFunc_IGTRG0_0(dummy)
#define | SetPinFunc_IGTRG0_1(dummy)
#define | SetPinFunc_INT00_0(dummy)
#define | SetPinFunc_INT00_1(dummy)
#define | SetPinFunc_INT01_0(dummy)
#define | SetPinFunc_INT01_1(dummy)
#define | SetPinFunc_INT02_0(dummy)
#define | SetPinFunc_INT02_1(dummy)
#define | SetPinFunc_INT02_2(dummy)
#define | SetPinFunc_INT03_0(dummy)
#define | SetPinFunc_INT03_1(dummy)
#define | SetPinFunc_INT03_2(dummy)
#define | SetPinFunc_INT04_0(dummy)
#define | SetPinFunc_INT04_1(dummy)
#define | SetPinFunc_INT05_0(dummy)
#define | SetPinFunc_INT05_1(dummy)
#define | SetPinFunc_INT06_0(dummy)
#define | SetPinFunc_INT06_1(dummy)
#define | SetPinFunc_INT15_0(dummy)
#define | SetPinFunc_INT15_1(dummy)
#define | SetPinFunc_INT15_2(dummy)
#define | SetPinFunc_NMIX(dummy)
#define | SetPinFunc_RTCCO_0(dummy)
#define | SetPinFunc_RTCCO_1(dummy)
#define | SetPinFunc_RTCCO_2(dummy)
#define | SetPinFunc_RTO00_0(dummy)
#define | SetPinFunc_RTO01_0(dummy)
#define | SetPinFunc_RTO02_0(dummy)
#define | SetPinFunc_RTO03_0(dummy)
#define | SetPinFunc_RTO04_0(dummy)
#define | SetPinFunc_RTO05_0(dummy)
#define | SetPinFunc_SCK0_0(dummy)
#define | SetPinFunc_SCK0_2(dummy)
#define | SetPinFunc_SCK1_1(dummy)
#define | SetPinFunc_SCK1_2(dummy)
#define | SetPinFunc_SCK3_0(dummy)
#define | SetPinFunc_SCK3_1(dummy)
#define | SetPinFunc_SCK3_2(dummy)
#define | SetPinFunc_SCS10_1(dummy)
#define | SetPinFunc_SCS10_2(dummy)
#define | SetPinFunc_SCS11_1(dummy)
#define | SetPinFunc_SCS11_2(dummy)
#define | SetPinFunc_SCS30_2(dummy)
#define | SetPinFunc_SCS31_2(dummy)
#define | SetPinFunc_SIN0_0(dummy)
#define | SetPinFunc_SIN0_1(dummy)
#define | SetPinFunc_SIN0_2(dummy)
#define | SetPinFunc_SIN1_1(dummy)
#define | SetPinFunc_SIN1_2(dummy)
#define | SetPinFunc_SIN3_0(dummy)
#define | SetPinFunc_SIN3_1(dummy)
#define | SetPinFunc_SIN3_2(dummy)
#define | SetPinFunc_SOT0_0(dummy)
#define | SetPinFunc_SOT0_1(dummy)
#define | SetPinFunc_SOT0_2(dummy)
#define | SetPinFunc_SOT1_1(dummy)
#define | SetPinFunc_SOT1_2(dummy)
#define | SetPinFunc_SOT3_0(dummy)
#define | SetPinFunc_SOT3_1(dummy)
#define | SetPinFunc_SOT3_2(dummy)
#define | SetPinFunc_SUBOUT_0(dummy)
#define | SetPinFunc_SUBOUT_1(dummy)
#define | SetPinFunc_SUBOUT_2(dummy)
#define | SetPinFunc_TIOA0_0_OUT(dummy)
#define | SetPinFunc_TIOA0_1_OUT(dummy)
#define | SetPinFunc_TIOA1_0_IN(dummy)
#define | SetPinFunc_TIOA1_0_OUT(dummy)
#define | SetPinFunc_TIOA1_1_IN(dummy)
#define | SetPinFunc_TIOA1_1_OUT(dummy)
#define | SetPinFunc_TIOA2_0_OUT(dummy)
#define | SetPinFunc_TIOA2_1_OUT(dummy)
#define | SetPinFunc_TIOA2_2_OUT(dummy)
#define | SetPinFunc_TIOA3_1_IN(dummy)
#define | SetPinFunc_TIOA3_1_OUT(dummy)
#define | SetPinFunc_TIOB0_0_IN(dummy)
#define | SetPinFunc_TIOB0_1_IN(dummy)
#define | SetPinFunc_TIOB1_0_IN(dummy)
#define | SetPinFunc_TIOB1_1_IN(dummy)
#define | SetPinFunc_TIOB2_0_IN(dummy)
#define | SetPinFunc_TIOB2_2_IN(dummy)
#define | SetPinFunc_ZIN0_0(dummy)
#define | SetPinFunc_ZIN0_1(dummy)
#define | SetPinFunc_ZIN0_2(dummy)
#define | SetPinFunc_ZIN0_3(dummy)
#define | SetPinFunc_AN00(dummy) ( bFM0P_GPIO_ADE_AN00 = 1 )
#define | SetPinFunc_AN01(dummy) ( bFM0P_GPIO_ADE_AN01 = 1 )
#define | SetPinFunc_AN02(dummy) ( bFM0P_GPIO_ADE_AN02 = 1 )
#define | SetPinFunc_AN03(dummy) ( bFM0P_GPIO_ADE_AN03 = 1 )
#define | SetPinFunc_AN04(dummy) ( bFM0P_GPIO_ADE_AN04 = 1 )
#define | SetPinFunc_AN05(dummy) ( bFM0P_GPIO_ADE_AN05 = 1 )
#define | SetPinFunc_AN06(dummy) ( bFM0P_GPIO_ADE_AN06 = 1 )
#define | SetPinFunc_AN07(dummy) ( bFM0P_GPIO_ADE_AN07 = 1 )

## Detailed Description

Header file for S6E1A1XC0A GPIO functions, included in gpio.h

History:

- 2013-12-04 1.0 Edison Zhang First version
- 2014-05-14 1.1 Edison Zhang Update P46/P47, PE2/PE3 initialization

Definition in file gpio_s6e1a1xc0a.h.

## Define Documentation

#define FGPIO1PIN_NP00_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P00)) )

Definition at line 1459 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP00_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP00_INITIN(v) \
                                                             : FGPIO1PIN_NP00_INITOUT(v) )

Definition at line 1463 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP00_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P00=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P00=0u; \
                                              bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 1466 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP00_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P00=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P00=1u; \
                                              bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 1470 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP00_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P00=(uint8_t)(~(v)) )

Definition at line 1461 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP01_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P01)) )

Definition at line 1494 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP01_INITIN(v) \
                                                             : FGPIO1PIN_NP01_INITOUT(v) )

Definition at line 1498 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P01=0u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 1501 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P01=1u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 1505 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP01_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P01=(uint8_t)(~(v)) )

Definition at line 1496 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP02_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P02)) )

Definition at line 1529 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP02_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP02_INITIN(v) \
                                                             : FGPIO1PIN_NP02_INITOUT(v) )

Definition at line 1533 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP02_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P02=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P02=0u; \
                                              bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 1536 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP02_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P02=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P02=1u; \
                                              bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 1540 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP02_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P02=(uint8_t)(~(v)) )

Definition at line 1531 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP03_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P03)) )

Definition at line 1564 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP03_INITIN(v) \
                                                             : FGPIO1PIN_NP03_INITOUT(v) )

Definition at line 1568 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P03=0u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 1571 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P03=1u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 1575 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP03_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P03=(uint8_t)(~(v)) )

Definition at line 1566 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP04_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P04)) )

Definition at line 1599 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP04_INITIN(v) \
                                                             : FGPIO1PIN_NP04_INITOUT(v) )

Definition at line 1603 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P04=0u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1606 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P04=1u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1610 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP04_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P04=(uint8_t)(~(v)) )

Definition at line 1601 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP0F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR0_f.P0F)) )

Definition at line 1634 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP0F_INITIN(v) \
                                                             : FGPIO1PIN_NP0F_INITOUT(v) )

Definition at line 1638 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P0F=0u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1641 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR0_P0F=1u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1645 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P0F=(uint8_t)(~(v)) )

Definition at line 1636 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP10_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P10)) )

Definition at line 1672 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP10_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP10_INITIN(v) \
                                                             : FGPIO1PIN_NP10_INITOUT(v) )

Definition at line 1676 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP10_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P10=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P10=0u; \
                                              bFM0P_GPIO_PFR1_P10=0u; \
                                              bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 1679 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP10_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P10=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P10=1u; \
                                              bFM0P_GPIO_PFR1_P10=0u; \
                                              bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 1685 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP10_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P10=(uint8_t)(~(v)) )

Definition at line 1674 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP11_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P11)) )

Definition at line 1713 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP11_INITIN(v) \
                                                             : FGPIO1PIN_NP11_INITOUT(v) )

Definition at line 1717 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P11=0u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1720 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P11=1u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1726 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP11_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P11=(uint8_t)(~(v)) )

Definition at line 1715 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP12_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P12)) )

Definition at line 1754 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP12_INITIN(v) \
                                                             : FGPIO1PIN_NP12_INITOUT(v) )

Definition at line 1758 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P12=0u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1761 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P12=1u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1767 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP12_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P12=(uint8_t)(~(v)) )

Definition at line 1756 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP13_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P13)) )

Definition at line 1795 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP13_INITIN(v) \
                                                             : FGPIO1PIN_NP13_INITOUT(v) )

Definition at line 1799 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P13=0u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1802 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P13=1u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1808 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP13_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P13=(uint8_t)(~(v)) )

Definition at line 1797 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP14_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P14)) )

Definition at line 1836 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP14_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP14_INITIN(v) \
                                                             : FGPIO1PIN_NP14_INITOUT(v) )

Definition at line 1840 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP14_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P14=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P14=0u; \
                                              bFM0P_GPIO_PFR1_P14=0u; \
                                              bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 1843 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP14_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P14=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P14=1u; \
                                              bFM0P_GPIO_PFR1_P14=0u; \
                                              bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 1849 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP14_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P14=(uint8_t)(~(v)) )

Definition at line 1838 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP15_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR1_f.P15)) )

Definition at line 1877 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP15_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP15_INITIN(v) \
                                                             : FGPIO1PIN_NP15_INITOUT(v) )

Definition at line 1881 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP15_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P15=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P15=0u; \
                                              bFM0P_GPIO_PFR1_P15=0u; \
                                              bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 1884 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP15_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P15=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR1_P15=1u; \
                                              bFM0P_GPIO_PFR1_P15=0u; \
                                              bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 1890 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP15_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P15=(uint8_t)(~(v)) )

Definition at line 1879 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP21_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P21)) )

Definition at line 1915 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP21_INITIN(v) \
                                                             : FGPIO1PIN_NP21_INITOUT(v) )

Definition at line 1919 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P21=0u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1922 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P21=1u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1926 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP21_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P21=(uint8_t)(~(v)) )

Definition at line 1917 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP22_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P22)) )

Definition at line 1953 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP22_INITIN(v) \
                                                             : FGPIO1PIN_NP22_INITOUT(v) )

Definition at line 1957 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P22=0u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1960 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P22=1u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1966 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP22_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P22=(uint8_t)(~(v)) )

Definition at line 1955 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP23_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR2_f.P23)) )

Definition at line 1994 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP23_INITIN(v) \
                                                             : FGPIO1PIN_NP23_INITOUT(v) )

Definition at line 1998 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P23=0u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 2001 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR2_P23=1u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 2007 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP23_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P23=(uint8_t)(~(v)) )

Definition at line 1996 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP39_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P39)) )

Definition at line 2032 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP39_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP39_INITIN(v) \
                                                             : FGPIO1PIN_NP39_INITOUT(v) )

Definition at line 2036 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP39_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P39=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P39=0u; \
                                              bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 2039 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP39_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P39=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P39=1u; \
                                              bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 2043 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP39_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P39=(uint8_t)(~(v)) )

Definition at line 2034 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3A)) )

Definition at line 2067 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3A_INITIN(v) \
                                                             : FGPIO1PIN_NP3A_INITOUT(v) )

Definition at line 2071 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3A=0u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 2074 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3A=1u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 2078 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3A=(uint8_t)(~(v)) )

Definition at line 2069 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3B_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3B)) )

Definition at line 2102 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3B_INITIN(v) \
                                                             : FGPIO1PIN_NP3B_INITOUT(v) )

Definition at line 2106 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3B=0u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 2109 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3B=1u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 2113 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3B=(uint8_t)(~(v)) )

Definition at line 2104 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3C_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3C)) )

Definition at line 2137 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3C_INITIN(v) \
                                                             : FGPIO1PIN_NP3C_INITOUT(v) )

Definition at line 2141 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3C=0u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 2144 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3C=1u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 2148 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3C=(uint8_t)(~(v)) )

Definition at line 2139 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3D_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3D)) )

Definition at line 2172 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3D_INITIN(v) \
                                                             : FGPIO1PIN_NP3D_INITOUT(v) )

Definition at line 2176 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3D=0u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 2179 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3D=1u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 2183 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3D=(uint8_t)(~(v)) )

Definition at line 2174 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3E_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3E)) )

Definition at line 2207 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3E_INITIN(v) \
                                                             : FGPIO1PIN_NP3E_INITOUT(v) )

Definition at line 2211 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3E=0u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 2214 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3E=1u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 2218 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3E=(uint8_t)(~(v)) )

Definition at line 2209 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3F_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR3_f.P3F)) )

Definition at line 2242 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP3F_INITIN(v) \
                                                             : FGPIO1PIN_NP3F_INITOUT(v) )

Definition at line 2246 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3F=0u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 2249 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR3_P3F=1u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 2253 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3F=(uint8_t)(~(v)) )

Definition at line 2244 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP46_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P46)) )

Definition at line 2281 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP46_INITIN(v) \
                                                             : FGPIO1PIN_NP46_INITOUT(v) )

Definition at line 2285 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P46=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 2288 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P46=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 2294 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP46_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P46=(uint8_t)(~(v)) )

Definition at line 2283 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP47_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P47)) )

Definition at line 2324 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP47_INITIN(v) \
                                                             : FGPIO1PIN_NP47_INITOUT(v) )

Definition at line 2328 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P47=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 2331 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P47=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 2337 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP47_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P47=(uint8_t)(~(v)) )

Definition at line 2326 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP49_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P49)) )

Definition at line 2363 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP49_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP49_INITIN(v) \
                                                             : FGPIO1PIN_NP49_INITOUT(v) )

Definition at line 2367 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP49_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P49=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P49=0u; \
                                              bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 2370 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP49_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P49=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P49=1u; \
                                              bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 2374 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP49_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P49=(uint8_t)(~(v)) )

Definition at line 2365 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP4A_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR4_f.P4A)) )

Definition at line 2398 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP4A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP4A_INITIN(v) \
                                                             : FGPIO1PIN_NP4A_INITOUT(v) )

Definition at line 2402 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP4A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P4A=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P4A=0u; \
                                              bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 2405 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP4A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P4A=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR4_P4A=1u; \
                                              bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 2409 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP4A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P4A=(uint8_t)(~(v)) )

Definition at line 2400 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP50_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P50)) )

Definition at line 2433 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP50_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP50_INITIN(v) \
                                                             : FGPIO1PIN_NP50_INITOUT(v) )

Definition at line 2437 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP50_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P50=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P50=0u; \
                                              bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 2440 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP50_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P50=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR5_P50=1u; \
                                              bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 2444 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP50_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P50=(uint8_t)(~(v)) )

Definition at line 2435 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP51_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P51)) )

Definition at line 2468 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP51_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP51_INITIN(v) \
                                                             : FGPIO1PIN_NP51_INITOUT(v) )

Definition at line 2472 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP51_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P51=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P51=0u; \
                                              bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 2475 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP51_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P51=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR5_P51=1u; \
                                              bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 2479 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP51_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P51=(uint8_t)(~(v)) )

Definition at line 2470 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP52_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR5_f.P52)) )

Definition at line 2503 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP52_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP52_INITIN(v) \
                                                             : FGPIO1PIN_NP52_INITOUT(v) )

Definition at line 2507 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP52_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P52=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P52=0u; \
                                              bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 2510 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP52_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P52=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR5_P52=1u; \
                                              bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 2514 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP52_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P52=(uint8_t)(~(v)) )

Definition at line 2505 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP60_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P60)) )

Definition at line 2538 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP60_INITIN(v) \
                                                             : FGPIO1PIN_NP60_INITOUT(v) )

Definition at line 2542 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P60=0u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 2545 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR6_P60=1u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 2549 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP60_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P60=(uint8_t)(~(v)) )

Definition at line 2540 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP61_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR6_f.P61)) )

Definition at line 2573 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP61_INITIN(v) \
                                                             : FGPIO1PIN_NP61_INITOUT(v) )

Definition at line 2577 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P61=0u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 2580 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR6_P61=1u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 2584 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP61_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P61=(uint8_t)(~(v)) )

Definition at line 2575 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP80_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P80)) )

Definition at line 2608 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP80_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP80_INITIN(v) \
                                                             : FGPIO1PIN_NP80_INITOUT(v) )

Definition at line 2612 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP80_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P80=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P80=0u; \
                                              bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 2615 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP80_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P80=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR8_P80=1u; \
                                              bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 2619 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP80_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P80=(uint8_t)(~(v)) )

Definition at line 2610 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP81_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P81)) )

Definition at line 2643 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP81_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP81_INITIN(v) \
                                                             : FGPIO1PIN_NP81_INITOUT(v) )

Definition at line 2647 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP81_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P81=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P81=0u; \
                                              bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 2650 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP81_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P81=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR8_P81=1u; \
                                              bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 2654 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP81_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P81=(uint8_t)(~(v)) )

Definition at line 2645 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP82_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIR8_f.P82)) )

Definition at line 2678 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP82_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NP82_INITIN(v) \
                                                             : FGPIO1PIN_NP82_INITOUT(v) )

Definition at line 2682 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP82_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P82=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P82=0u; \
                                              bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 2685 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP82_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P82=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDR8_P82=1u; \
                                              bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 2689 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NP82_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P82=(uint8_t)(~(v)) )

Definition at line 2680 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE0_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE0)) )

Definition at line 2713 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE0_INITIN(v) \
                                                             : FGPIO1PIN_NPE0_INITOUT(v) )

Definition at line 2717 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE0=0u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 2720 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE0=1u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 2724 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE0=(uint8_t)(~(v)) )

Definition at line 2715 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE2_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE2)) )

Definition at line 2752 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE2_INITIN(v) \
                                                             : FGPIO1PIN_NPE2_INITOUT(v) )

Definition at line 2756 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE2=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 2759 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE2=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 2765 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE2=(uint8_t)(~(v)) )

Definition at line 2754 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE3_GET ( (uint8_t)(!(FM0P_FASTIO->FPDIRE_f.PE3)) )

Definition at line 2795 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_NPE3_INITIN(v) \
                                                             : FGPIO1PIN_NPE3_INITOUT(v) )

Definition at line 2799 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE3=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 2802 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(uint8_t)(~((uint8_t)(v).bInitVal)); \
                                              bFM0P_GPIO_DDRE_PE3=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 2808 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_NPE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE3=(uint8_t)(~(v)) )

Definition at line 2797 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P00_GET ( FM0P_FASTIO->FPDIR0_f.P00 )

Definition at line 1442 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P00_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P00_INITIN(v) \
                                                             : FGPIO1PIN_P00_INITOUT(v) )

Definition at line 1446 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P00_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P00=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P00=0u; \
                                              bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 1449 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P00_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P00=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P00=1u; \
                                              bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 1453 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P00_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P00=(v) )

Definition at line 1444 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P01_GET ( FM0P_FASTIO->FPDIR0_f.P01 )

Definition at line 1477 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P01_INITIN(v) \
                                                             : FGPIO1PIN_P01_INITOUT(v) )

Definition at line 1481 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P01=0u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 1484 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P01=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P01=1u; \
                                              bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 1488 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P01_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P01=(v) )

Definition at line 1479 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P02_GET ( FM0P_FASTIO->FPDIR0_f.P02 )

Definition at line 1512 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P02_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P02_INITIN(v) \
                                                             : FGPIO1PIN_P02_INITOUT(v) )

Definition at line 1516 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P02_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P02=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P02=0u; \
                                              bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 1519 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P02_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P02=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P02=1u; \
                                              bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 1523 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P02_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P02=(v) )

Definition at line 1514 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P03_GET ( FM0P_FASTIO->FPDIR0_f.P03 )

Definition at line 1547 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P03_INITIN(v) \
                                                             : FGPIO1PIN_P03_INITOUT(v) )

Definition at line 1551 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P03=0u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 1554 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P03=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P03=1u; \
                                              bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 1558 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P03_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P03=(v) )

Definition at line 1549 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P04_GET ( FM0P_FASTIO->FPDIR0_f.P04 )

Definition at line 1582 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P04_INITIN(v) \
                                                             : FGPIO1PIN_P04_INITOUT(v) )

Definition at line 1586 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P04=0u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1589 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P04=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P04=1u; \
                                              bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 1593 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P04_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P04=(v) )

Definition at line 1584 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P0F_GET ( FM0P_FASTIO->FPDIR0_f.P0F )

Definition at line 1617 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P0F_INITIN(v) \
                                                             : FGPIO1PIN_P0F_INITOUT(v) )

Definition at line 1621 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                              bFM0P_GPIO_DDR0_P0F=0u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1624 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR0_P0F=(v).bInitVal; \
                                              bFM0P_GPIO_DDR0_P0F=1u; \
                                              bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 1628 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR0_P0F=(v) )

Definition at line 1619 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P10_GET ( FM0P_FASTIO->FPDIR1_f.P10 )

Definition at line 1652 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P10_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P10_INITIN(v) \
                                                             : FGPIO1PIN_P10_INITOUT(v) )

Definition at line 1656 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P10_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P10=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P10=0u; \
                                              bFM0P_GPIO_PFR1_P10=0u; \
                                              bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 1659 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P10_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P10=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P10=1u; \
                                              bFM0P_GPIO_PFR1_P10=0u; \
                                              bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 1665 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P10_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P10=(v) )

Definition at line 1654 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P11_GET ( FM0P_FASTIO->FPDIR1_f.P11 )

Definition at line 1693 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P11_INITIN(v) \
                                                             : FGPIO1PIN_P11_INITOUT(v) )

Definition at line 1697 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P11=0u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1700 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P11=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P11=1u; \
                                              bFM0P_GPIO_PFR1_P11=0u; \
                                              bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 1706 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P11_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P11=(v) )

Definition at line 1695 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P12_GET ( FM0P_FASTIO->FPDIR1_f.P12 )

Definition at line 1734 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P12_INITIN(v) \
                                                             : FGPIO1PIN_P12_INITOUT(v) )

Definition at line 1738 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P12=0u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1741 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P12=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P12=1u; \
                                              bFM0P_GPIO_PFR1_P12=0u; \
                                              bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 1747 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P12_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P12=(v) )

Definition at line 1736 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P13_GET ( FM0P_FASTIO->FPDIR1_f.P13 )

Definition at line 1775 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P13_INITIN(v) \
                                                             : FGPIO1PIN_P13_INITOUT(v) )

Definition at line 1779 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P13=0u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1782 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P13=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P13=1u; \
                                              bFM0P_GPIO_PFR1_P13=0u; \
                                              bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 1788 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P13_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P13=(v) )

Definition at line 1777 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P14_GET ( FM0P_FASTIO->FPDIR1_f.P14 )

Definition at line 1816 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P14_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P14_INITIN(v) \
                                                             : FGPIO1PIN_P14_INITOUT(v) )

Definition at line 1820 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P14_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P14=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P14=0u; \
                                              bFM0P_GPIO_PFR1_P14=0u; \
                                              bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 1823 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P14_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P14=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P14=1u; \
                                              bFM0P_GPIO_PFR1_P14=0u; \
                                              bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 1829 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P14_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P14=(v) )

Definition at line 1818 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P15_GET ( FM0P_FASTIO->FPDIR1_f.P15 )

Definition at line 1857 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P15_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P15_INITIN(v) \
                                                             : FGPIO1PIN_P15_INITOUT(v) )

Definition at line 1861 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P15_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P15=(v).bPullup; \
                                              bFM0P_GPIO_DDR1_P15=0u; \
                                              bFM0P_GPIO_PFR1_P15=0u; \
                                              bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 1864 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P15_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR1_P15=(v).bInitVal; \
                                              bFM0P_GPIO_DDR1_P15=1u; \
                                              bFM0P_GPIO_PFR1_P15=0u; \
                                              bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 1870 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P15_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR1_P15=(v) )

Definition at line 1859 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P21_GET ( FM0P_FASTIO->FPDIR2_f.P21 )

Definition at line 1898 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P21_INITIN(v) \
                                                             : FGPIO1PIN_P21_INITOUT(v) )

Definition at line 1902 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P21=0u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1905 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P21=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P21=1u; \
                                              bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 1909 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P21_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P21=(v) )

Definition at line 1900 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P22_GET ( FM0P_FASTIO->FPDIR2_f.P22 )

Definition at line 1933 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P22_INITIN(v) \
                                                             : FGPIO1PIN_P22_INITOUT(v) )

Definition at line 1937 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P22=0u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1940 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P22=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P22=1u; \
                                              bFM0P_GPIO_PFR2_P22=0u; \
                                              bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 1946 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P22_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P22=(v) )

Definition at line 1935 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P23_GET ( FM0P_FASTIO->FPDIR2_f.P23 )

Definition at line 1974 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P23_INITIN(v) \
                                                             : FGPIO1PIN_P23_INITOUT(v) )

Definition at line 1978 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                              bFM0P_GPIO_DDR2_P23=0u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1981 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR2_P23=(v).bInitVal; \
                                              bFM0P_GPIO_DDR2_P23=1u; \
                                              bFM0P_GPIO_PFR2_P23=0u; \
                                              bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 1987 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P23_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR2_P23=(v) )

Definition at line 1976 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P39_GET ( FM0P_FASTIO->FPDIR3_f.P39 )

Definition at line 2015 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P39_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P39_INITIN(v) \
                                                             : FGPIO1PIN_P39_INITOUT(v) )

Definition at line 2019 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P39_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P39=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P39=0u; \
                                              bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 2022 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P39_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P39=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P39=1u; \
                                              bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 2026 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P39_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P39=(v) )

Definition at line 2017 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3A_GET ( FM0P_FASTIO->FPDIR3_f.P3A )

Definition at line 2050 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3A_INITIN(v) \
                                                             : FGPIO1PIN_P3A_INITOUT(v) )

Definition at line 2054 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3A=0u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 2057 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3A=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3A=1u; \
                                              bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 2061 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3A=(v) )

Definition at line 2052 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3B_GET ( FM0P_FASTIO->FPDIR3_f.P3B )

Definition at line 2085 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3B_INITIN(v) \
                                                             : FGPIO1PIN_P3B_INITOUT(v) )

Definition at line 2089 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3B=0u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 2092 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3B=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3B=1u; \
                                              bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 2096 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3B=(v) )

Definition at line 2087 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3C_GET ( FM0P_FASTIO->FPDIR3_f.P3C )

Definition at line 2120 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3C_INITIN(v) \
                                                             : FGPIO1PIN_P3C_INITOUT(v) )

Definition at line 2124 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3C=0u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 2127 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3C=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3C=1u; \
                                              bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 2131 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3C=(v) )

Definition at line 2122 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3D_GET ( FM0P_FASTIO->FPDIR3_f.P3D )

Definition at line 2155 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3D_INITIN(v) \
                                                             : FGPIO1PIN_P3D_INITOUT(v) )

Definition at line 2159 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3D=0u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 2162 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3D=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3D=1u; \
                                              bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 2166 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3D=(v) )

Definition at line 2157 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3E_GET ( FM0P_FASTIO->FPDIR3_f.P3E )

Definition at line 2190 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3E_INITIN(v) \
                                                             : FGPIO1PIN_P3E_INITOUT(v) )

Definition at line 2194 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3E=0u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 2197 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3E=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3E=1u; \
                                              bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 2201 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3E=(v) )

Definition at line 2192 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3F_GET ( FM0P_FASTIO->FPDIR3_f.P3F )

Definition at line 2225 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P3F_INITIN(v) \
                                                             : FGPIO1PIN_P3F_INITOUT(v) )

Definition at line 2229 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                              bFM0P_GPIO_DDR3_P3F=0u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 2232 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR3_P3F=(v).bInitVal; \
                                              bFM0P_GPIO_DDR3_P3F=1u; \
                                              bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 2236 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR3_P3F=(v) )

Definition at line 2227 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P46_GET ( FM0P_FASTIO->FPDIR4_f.P46 )

Definition at line 2260 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P46_INITIN(v) \
                                                             : FGPIO1PIN_P46_INITOUT(v) )

Definition at line 2264 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P46=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 2267 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P46=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P46=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 2273 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P46_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P46=(v) )

Definition at line 2262 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P47_GET ( FM0P_FASTIO->FPDIR4_f.P47 )

Definition at line 2303 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P47_INITIN(v) \
                                                             : FGPIO1PIN_P47_INITOUT(v) )

Definition at line 2307 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P47=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 2310 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P47=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P47=1u; \
                                              bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                              bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                              bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 2316 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P47_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P47=(v) )

Definition at line 2305 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P49_GET ( FM0P_FASTIO->FPDIR4_f.P49 )

Definition at line 2346 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P49_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P49_INITIN(v) \
                                                             : FGPIO1PIN_P49_INITOUT(v) )

Definition at line 2350 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P49_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P49=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P49=0u; \
                                              bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 2353 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P49_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P49=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P49=1u; \
                                              bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 2357 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P49_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P49=(v) )

Definition at line 2348 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P4A_GET ( FM0P_FASTIO->FPDIR4_f.P4A )

Definition at line 2381 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P4A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P4A_INITIN(v) \
                                                             : FGPIO1PIN_P4A_INITOUT(v) )

Definition at line 2385 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P4A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P4A=(v).bPullup; \
                                              bFM0P_GPIO_DDR4_P4A=0u; \
                                              bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 2388 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P4A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR4_P4A=(v).bInitVal; \
                                              bFM0P_GPIO_DDR4_P4A=1u; \
                                              bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 2392 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P4A_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR4_P4A=(v) )

Definition at line 2383 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P50_GET ( FM0P_FASTIO->FPDIR5_f.P50 )

Definition at line 2416 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P50_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P50_INITIN(v) \
                                                             : FGPIO1PIN_P50_INITOUT(v) )

Definition at line 2420 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P50_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P50=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P50=0u; \
                                              bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 2423 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P50_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR5_P50=(v).bInitVal; \
                                              bFM0P_GPIO_DDR5_P50=1u; \
                                              bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 2427 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P50_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P50=(v) )

Definition at line 2418 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P51_GET ( FM0P_FASTIO->FPDIR5_f.P51 )

Definition at line 2451 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P51_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P51_INITIN(v) \
                                                             : FGPIO1PIN_P51_INITOUT(v) )

Definition at line 2455 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P51_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P51=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P51=0u; \
                                              bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 2458 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P51_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR5_P51=(v).bInitVal; \
                                              bFM0P_GPIO_DDR5_P51=1u; \
                                              bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 2462 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P51_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P51=(v) )

Definition at line 2453 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P52_GET ( FM0P_FASTIO->FPDIR5_f.P52 )

Definition at line 2486 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P52_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P52_INITIN(v) \
                                                             : FGPIO1PIN_P52_INITOUT(v) )

Definition at line 2490 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P52_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P52=(v).bPullup; \
                                              bFM0P_GPIO_DDR5_P52=0u; \
                                              bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 2493 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P52_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR5_P52=(v).bInitVal; \
                                              bFM0P_GPIO_DDR5_P52=1u; \
                                              bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 2497 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P52_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR5_P52=(v) )

Definition at line 2488 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P60_GET ( FM0P_FASTIO->FPDIR6_f.P60 )

Definition at line 2521 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P60_INITIN(v) \
                                                             : FGPIO1PIN_P60_INITOUT(v) )

Definition at line 2525 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P60=0u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 2528 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR6_P60=(v).bInitVal; \
                                              bFM0P_GPIO_DDR6_P60=1u; \
                                              bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 2532 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P60_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P60=(v) )

Definition at line 2523 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P61_GET ( FM0P_FASTIO->FPDIR6_f.P61 )

Definition at line 2556 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P61_INITIN(v) \
                                                             : FGPIO1PIN_P61_INITOUT(v) )

Definition at line 2560 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                              bFM0P_GPIO_DDR6_P61=0u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 2563 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR6_P61=(v).bInitVal; \
                                              bFM0P_GPIO_DDR6_P61=1u; \
                                              bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 2567 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P61_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR6_P61=(v) )

Definition at line 2558 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P80_GET ( FM0P_FASTIO->FPDIR8_f.P80 )

Definition at line 2591 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P80_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P80_INITIN(v) \
                                                             : FGPIO1PIN_P80_INITOUT(v) )

Definition at line 2595 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P80_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P80=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P80=0u; \
                                              bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 2598 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P80_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR8_P80=(v).bInitVal; \
                                              bFM0P_GPIO_DDR8_P80=1u; \
                                              bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 2602 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P80_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P80=(v) )

Definition at line 2593 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P81_GET ( FM0P_FASTIO->FPDIR8_f.P81 )

Definition at line 2626 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P81_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P81_INITIN(v) \
                                                             : FGPIO1PIN_P81_INITOUT(v) )

Definition at line 2630 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P81_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P81=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P81=0u; \
                                              bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 2633 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P81_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR8_P81=(v).bInitVal; \
                                              bFM0P_GPIO_DDR8_P81=1u; \
                                              bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 2637 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P81_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P81=(v) )

Definition at line 2628 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P82_GET ( FM0P_FASTIO->FPDIR8_f.P82 )

Definition at line 2661 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P82_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_P82_INITIN(v) \
                                                             : FGPIO1PIN_P82_INITOUT(v) )

Definition at line 2665 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P82_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P82=(v).bPullup; \
                                              bFM0P_GPIO_DDR8_P82=0u; \
                                              bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 2668 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P82_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDOR8_P82=(v).bInitVal; \
                                              bFM0P_GPIO_DDR8_P82=1u; \
                                              bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 2672 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_P82_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDOR8_P82=(v) )

Definition at line 2663 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE0_GET ( FM0P_FASTIO->FPDIRE_f.PE0 )

Definition at line 2696 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE0_INITIN(v) \
                                                             : FGPIO1PIN_PE0_INITOUT(v) )

Definition at line 2700 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE0=0u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 2703 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE0=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE0=1u; \
                                              bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 2707 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE0=(v) )

Definition at line 2698 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE2_GET ( FM0P_FASTIO->FPDIRE_f.PE2 )

Definition at line 2731 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE2_INITIN(v) \
                                                             : FGPIO1PIN_PE2_INITOUT(v) )

Definition at line 2735 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE2=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 2738 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE2=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE2=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 2744 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE2=(v) )

Definition at line 2733 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE3_GET ( FM0P_FASTIO->FPDIRE_f.PE3 )

Definition at line 2774 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? FGPIO1PIN_PE3_INITIN(v) \
                                                             : FGPIO1PIN_PE3_INITOUT(v) )

Definition at line 2778 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                              bFM0P_GPIO_DDRE_PE3=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 2781 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_FPDORE_PE3=(v).bInitVal; \
                                              bFM0P_GPIO_DDRE_PE3=1u; \
                                              bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                              bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                              bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 2787 of file gpio_s6e1a1xc0a.h.

#define FGPIO1PIN_PE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_FPDORE_PE3=(v) )

Definition at line 2776 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP00_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P00)) )

Definition at line 80 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP00_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP00_INITIN(v) \
                                                            : GPIO1PIN_NP00_INITOUT(v) )

Definition at line 84 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP00_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P00=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P00=0u; \
                                             bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 87 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP00_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P00=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P00=1u; \
                                             bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 91 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP00_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P00=(uint32_t)(!(v)) )

Definition at line 82 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP01_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P01)) )

Definition at line 115 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP01_INITIN(v) \
                                                            : GPIO1PIN_NP01_INITOUT(v) )

Definition at line 119 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P01=0u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 122 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P01=1u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 126 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP01_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P01=(uint32_t)(!(v)) )

Definition at line 117 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP02_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P02)) )

Definition at line 150 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP02_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP02_INITIN(v) \
                                                            : GPIO1PIN_NP02_INITOUT(v) )

Definition at line 154 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP02_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P02=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P02=0u; \
                                             bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 157 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP02_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P02=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P02=1u; \
                                             bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 161 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP02_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P02=(uint32_t)(!(v)) )

Definition at line 152 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP03_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P03)) )

Definition at line 185 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP03_INITIN(v) \
                                                            : GPIO1PIN_NP03_INITOUT(v) )

Definition at line 189 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P03=0u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 192 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P03=1u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 196 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP03_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P03=(uint32_t)(!(v)) )

Definition at line 187 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP04_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P04)) )

Definition at line 220 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP04_INITIN(v) \
                                                            : GPIO1PIN_NP04_INITOUT(v) )

Definition at line 224 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P04=0u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 227 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P04=1u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 231 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP04_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P04=(uint32_t)(!(v)) )

Definition at line 222 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP0F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR0_P0F)) )

Definition at line 255 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP0F_INITIN(v) \
                                                            : GPIO1PIN_NP0F_INITOUT(v) )

Definition at line 259 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P0F=0u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 262 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR0_P0F=1u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 266 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P0F=(uint32_t)(!(v)) )

Definition at line 257 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP10_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P10)) )

Definition at line 293 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP10_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP10_INITIN(v) \
                                                            : GPIO1PIN_NP10_INITOUT(v) )

Definition at line 297 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP10_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P10=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P10=0u; \
                                             bFM0P_GPIO_PFR1_P10=0u; \
                                             bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 300 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP10_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P10=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P10=1u; \
                                             bFM0P_GPIO_PFR1_P10=0u; \
                                             bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 306 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP10_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P10=(uint32_t)(!(v)) )

Definition at line 295 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP11_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P11)) )

Definition at line 334 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP11_INITIN(v) \
                                                            : GPIO1PIN_NP11_INITOUT(v) )

Definition at line 338 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P11=0u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 341 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P11=1u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 347 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP11_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P11=(uint32_t)(!(v)) )

Definition at line 336 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP12_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P12)) )

Definition at line 375 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP12_INITIN(v) \
                                                            : GPIO1PIN_NP12_INITOUT(v) )

Definition at line 379 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P12=0u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 382 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P12=1u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 388 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP12_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P12=(uint32_t)(!(v)) )

Definition at line 377 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP13_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P13)) )

Definition at line 416 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP13_INITIN(v) \
                                                            : GPIO1PIN_NP13_INITOUT(v) )

Definition at line 420 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P13=0u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 423 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P13=1u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 429 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP13_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P13=(uint32_t)(!(v)) )

Definition at line 418 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP14_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P14)) )

Definition at line 457 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP14_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP14_INITIN(v) \
                                                            : GPIO1PIN_NP14_INITOUT(v) )

Definition at line 461 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP14_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P14=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P14=0u; \
                                             bFM0P_GPIO_PFR1_P14=0u; \
                                             bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 464 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP14_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P14=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P14=1u; \
                                             bFM0P_GPIO_PFR1_P14=0u; \
                                             bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 470 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP14_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P14=(uint32_t)(!(v)) )

Definition at line 459 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP15_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR1_P15)) )

Definition at line 498 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP15_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP15_INITIN(v) \
                                                            : GPIO1PIN_NP15_INITOUT(v) )

Definition at line 502 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP15_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P15=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P15=0u; \
                                             bFM0P_GPIO_PFR1_P15=0u; \
                                             bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 505 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP15_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P15=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR1_P15=1u; \
                                             bFM0P_GPIO_PFR1_P15=0u; \
                                             bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 511 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP15_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P15=(uint32_t)(!(v)) )

Definition at line 500 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP21_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P21)) )

Definition at line 536 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP21_INITIN(v) \
                                                            : GPIO1PIN_NP21_INITOUT(v) )

Definition at line 540 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P21=0u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 543 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P21=1u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 547 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP21_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P21=(uint32_t)(!(v)) )

Definition at line 538 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP22_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P22)) )

Definition at line 574 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP22_INITIN(v) \
                                                            : GPIO1PIN_NP22_INITOUT(v) )

Definition at line 578 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P22=0u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 581 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P22=1u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 587 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP22_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P22=(uint32_t)(!(v)) )

Definition at line 576 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP23_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR2_P23)) )

Definition at line 615 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP23_INITIN(v) \
                                                            : GPIO1PIN_NP23_INITOUT(v) )

Definition at line 619 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P23=0u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 622 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR2_P23=1u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 628 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP23_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P23=(uint32_t)(!(v)) )

Definition at line 617 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP39_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P39)) )

Definition at line 653 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP39_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP39_INITIN(v) \
                                                            : GPIO1PIN_NP39_INITOUT(v) )

Definition at line 657 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP39_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P39=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P39=0u; \
                                             bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 660 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP39_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P39=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P39=1u; \
                                             bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 664 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP39_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P39=(uint32_t)(!(v)) )

Definition at line 655 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3A)) )

Definition at line 688 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3A_INITIN(v) \
                                                            : GPIO1PIN_NP3A_INITOUT(v) )

Definition at line 692 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3A=0u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 695 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3A=1u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 699 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3A=(uint32_t)(!(v)) )

Definition at line 690 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3B_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3B)) )

Definition at line 723 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3B_INITIN(v) \
                                                            : GPIO1PIN_NP3B_INITOUT(v) )

Definition at line 727 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3B=0u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 730 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3B=1u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 734 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3B=(uint32_t)(!(v)) )

Definition at line 725 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3C_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3C)) )

Definition at line 758 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3C_INITIN(v) \
                                                            : GPIO1PIN_NP3C_INITOUT(v) )

Definition at line 762 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3C=0u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 765 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3C=1u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 769 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3C=(uint32_t)(!(v)) )

Definition at line 760 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3D_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3D)) )

Definition at line 793 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3D_INITIN(v) \
                                                            : GPIO1PIN_NP3D_INITOUT(v) )

Definition at line 797 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3D=0u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 800 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3D=1u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 804 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3D=(uint32_t)(!(v)) )

Definition at line 795 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3E_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3E)) )

Definition at line 828 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3E_INITIN(v) \
                                                            : GPIO1PIN_NP3E_INITOUT(v) )

Definition at line 832 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3E=0u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 835 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3E=1u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 839 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3E=(uint32_t)(!(v)) )

Definition at line 830 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3F_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR3_P3F)) )

Definition at line 863 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP3F_INITIN(v) \
                                                            : GPIO1PIN_NP3F_INITOUT(v) )

Definition at line 867 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3F=0u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 870 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR3_P3F=1u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 874 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3F=(uint32_t)(!(v)) )

Definition at line 865 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP46_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P46)) )

Definition at line 902 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP46_INITIN(v) \
                                                            : GPIO1PIN_NP46_INITOUT(v) )

Definition at line 906 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P46=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 909 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P46=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 915 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP46_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P46=(uint32_t)(!(v)) )

Definition at line 904 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP47_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P47)) )

Definition at line 945 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP47_INITIN(v) \
                                                            : GPIO1PIN_NP47_INITOUT(v) )

Definition at line 949 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P47=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 952 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P47=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 958 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP47_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P47=(uint32_t)(!(v)) )

Definition at line 947 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP49_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P49)) )

Definition at line 984 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP49_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP49_INITIN(v) \
                                                            : GPIO1PIN_NP49_INITOUT(v) )

Definition at line 988 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP49_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P49=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P49=0u; \
                                             bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 991 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP49_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P49=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P49=1u; \
                                             bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 995 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP49_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P49=(uint32_t)(!(v)) )

Definition at line 986 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP4A_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR4_P4A)) )

Definition at line 1019 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP4A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP4A_INITIN(v) \
                                                            : GPIO1PIN_NP4A_INITOUT(v) )

Definition at line 1023 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP4A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P4A=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P4A=0u; \
                                             bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 1026 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP4A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P4A=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR4_P4A=1u; \
                                             bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 1030 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP4A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P4A=(uint32_t)(!(v)) )

Definition at line 1021 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP50_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P50)) )

Definition at line 1054 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP50_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP50_INITIN(v) \
                                                            : GPIO1PIN_NP50_INITOUT(v) )

Definition at line 1058 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP50_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P50=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P50=0u; \
                                             bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 1061 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP50_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P50=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR5_P50=1u; \
                                             bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 1065 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP50_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P50=(uint32_t)(!(v)) )

Definition at line 1056 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP51_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P51)) )

Definition at line 1089 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP51_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP51_INITIN(v) \
                                                            : GPIO1PIN_NP51_INITOUT(v) )

Definition at line 1093 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP51_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P51=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P51=0u; \
                                             bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 1096 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP51_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P51=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR5_P51=1u; \
                                             bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 1100 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP51_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P51=(uint32_t)(!(v)) )

Definition at line 1091 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP52_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR5_P52)) )

Definition at line 1124 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP52_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP52_INITIN(v) \
                                                            : GPIO1PIN_NP52_INITOUT(v) )

Definition at line 1128 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP52_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P52=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P52=0u; \
                                             bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 1131 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP52_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P52=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR5_P52=1u; \
                                             bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 1135 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP52_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P52=(uint32_t)(!(v)) )

Definition at line 1126 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP60_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P60)) )

Definition at line 1159 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP60_INITIN(v) \
                                                            : GPIO1PIN_NP60_INITOUT(v) )

Definition at line 1163 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P60=0u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1166 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR6_P60=1u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1170 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP60_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P60=(uint32_t)(!(v)) )

Definition at line 1161 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP61_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR6_P61)) )

Definition at line 1194 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP61_INITIN(v) \
                                                            : GPIO1PIN_NP61_INITOUT(v) )

Definition at line 1198 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P61=0u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1201 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR6_P61=1u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1205 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP61_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P61=(uint32_t)(!(v)) )

Definition at line 1196 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP80_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P80)) )

Definition at line 1229 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP80_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP80_INITIN(v) \
                                                            : GPIO1PIN_NP80_INITOUT(v) )

Definition at line 1233 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP80_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P80=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P80=0u; \
                                             bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 1236 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP80_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P80=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR8_P80=1u; \
                                             bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 1240 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP80_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P80=(uint32_t)(!(v)) )

Definition at line 1231 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP81_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P81)) )

Definition at line 1264 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP81_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP81_INITIN(v) \
                                                            : GPIO1PIN_NP81_INITOUT(v) )

Definition at line 1268 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP81_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P81=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P81=0u; \
                                             bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 1271 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP81_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P81=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR8_P81=1u; \
                                             bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 1275 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP81_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P81=(uint32_t)(!(v)) )

Definition at line 1266 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP82_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIR8_P82)) )

Definition at line 1299 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP82_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NP82_INITIN(v) \
                                                            : GPIO1PIN_NP82_INITOUT(v) )

Definition at line 1303 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP82_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P82=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P82=0u; \
                                             bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 1306 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP82_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P82=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDR8_P82=1u; \
                                             bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 1310 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NP82_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P82=(uint32_t)(!(v)) )

Definition at line 1301 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE0_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE0)) )

Definition at line 1334 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE0_INITIN(v) \
                                                            : GPIO1PIN_NPE0_INITOUT(v) )

Definition at line 1338 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE0=0u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1341 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE0=1u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1345 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE0=(uint32_t)(!(v)) )

Definition at line 1336 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE2_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE2)) )

Definition at line 1373 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE2_INITIN(v) \
                                                            : GPIO1PIN_NPE2_INITOUT(v) )

Definition at line 1377 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE2=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1380 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE2=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1386 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE2=(uint32_t)(!(v)) )

Definition at line 1375 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE3_GET ( (uint32_t)(~(uint32_t)(bFM0P_GPIO_PDIRE_PE3)) )

Definition at line 1416 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_NPE3_INITIN(v) \
                                                            : GPIO1PIN_NPE3_INITOUT(v) )

Definition at line 1420 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE3=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1423 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(uint32_t)(~((uint32_t)(v).bInitVal)); \
                                             bFM0P_GPIO_DDRE_PE3=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1429 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_NPE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE3=(uint32_t)(!(v)) )

Definition at line 1418 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P00_GET ( bFM0P_GPIO_PDIR0_P00 )

Definition at line 63 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P00_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P00_INITIN(v) \
                                                            : GPIO1PIN_P00_INITOUT(v) )

Definition at line 67 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P00_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P00=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P00=0u; \
                                             bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 70 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P00_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P00=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P00=1u; \
                                             bFM0P_GPIO_PFR0_P00=0u; }while(0)

Definition at line 74 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P00_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P00=(v) )

Definition at line 65 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P01_GET ( bFM0P_GPIO_PDIR0_P01 )

Definition at line 98 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P01_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P01_INITIN(v) \
                                                            : GPIO1PIN_P01_INITOUT(v) )

Definition at line 102 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P01_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P01=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P01=0u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 105 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P01_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P01=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P01=1u; \
                                             bFM0P_GPIO_PFR0_P01=0u; }while(0)

Definition at line 109 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P01_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P01=(v) )

Definition at line 100 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P02_GET ( bFM0P_GPIO_PDIR0_P02 )

Definition at line 133 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P02_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P02_INITIN(v) \
                                                            : GPIO1PIN_P02_INITOUT(v) )

Definition at line 137 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P02_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P02=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P02=0u; \
                                             bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 140 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P02_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P02=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P02=1u; \
                                             bFM0P_GPIO_PFR0_P02=0u; }while(0)

Definition at line 144 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P02_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P02=(v) )

Definition at line 135 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P03_GET ( bFM0P_GPIO_PDIR0_P03 )

Definition at line 168 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P03_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P03_INITIN(v) \
                                                            : GPIO1PIN_P03_INITOUT(v) )

Definition at line 172 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P03_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P03=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P03=0u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 175 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P03_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P03=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P03=1u; \
                                             bFM0P_GPIO_PFR0_P03=0u; }while(0)

Definition at line 179 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P03_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P03=(v) )

Definition at line 170 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P04_GET ( bFM0P_GPIO_PDIR0_P04 )

Definition at line 203 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P04_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P04_INITIN(v) \
                                                            : GPIO1PIN_P04_INITOUT(v) )

Definition at line 207 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P04_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P04=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P04=0u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 210 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P04_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P04=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P04=1u; \
                                             bFM0P_GPIO_PFR0_P04=0u; }while(0)

Definition at line 214 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P04_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P04=(v) )

Definition at line 205 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P0F_GET ( bFM0P_GPIO_PDIR0_P0F )

Definition at line 238 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P0F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P0F_INITIN(v) \
                                                            : GPIO1PIN_P0F_INITOUT(v) )

Definition at line 242 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P0F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR0_P0F=(v).bPullup; \
                                             bFM0P_GPIO_DDR0_P0F=0u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 245 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P0F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR0_P0F=(v).bInitVal; \
                                             bFM0P_GPIO_DDR0_P0F=1u; \
                                             bFM0P_GPIO_PFR0_P0F=0u; }while(0)

Definition at line 249 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P0F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR0_P0F=(v) )

Definition at line 240 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P10_GET ( bFM0P_GPIO_PDIR1_P10 )

Definition at line 273 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P10_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P10_INITIN(v) \
                                                            : GPIO1PIN_P10_INITOUT(v) )

Definition at line 277 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P10_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P10=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P10=0u; \
                                             bFM0P_GPIO_PFR1_P10=0u; \
                                             bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 280 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P10_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P10=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P10=1u; \
                                             bFM0P_GPIO_PFR1_P10=0u; \
                                             bFM0P_GPIO_ADE_AN00=0u; }while(0)

Definition at line 286 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P10_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P10=(v) )

Definition at line 275 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P11_GET ( bFM0P_GPIO_PDIR1_P11 )

Definition at line 314 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P11_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P11_INITIN(v) \
                                                            : GPIO1PIN_P11_INITOUT(v) )

Definition at line 318 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P11_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P11=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P11=0u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 321 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P11_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P11=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P11=1u; \
                                             bFM0P_GPIO_PFR1_P11=0u; \
                                             bFM0P_GPIO_ADE_AN01=0u; }while(0)

Definition at line 327 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P11_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P11=(v) )

Definition at line 316 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P12_GET ( bFM0P_GPIO_PDIR1_P12 )

Definition at line 355 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P12_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P12_INITIN(v) \
                                                            : GPIO1PIN_P12_INITOUT(v) )

Definition at line 359 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P12_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P12=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P12=0u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 362 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P12_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P12=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P12=1u; \
                                             bFM0P_GPIO_PFR1_P12=0u; \
                                             bFM0P_GPIO_ADE_AN02=0u; }while(0)

Definition at line 368 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P12_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P12=(v) )

Definition at line 357 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P13_GET ( bFM0P_GPIO_PDIR1_P13 )

Definition at line 396 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P13_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P13_INITIN(v) \
                                                            : GPIO1PIN_P13_INITOUT(v) )

Definition at line 400 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P13_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P13=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P13=0u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 403 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P13_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P13=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P13=1u; \
                                             bFM0P_GPIO_PFR1_P13=0u; \
                                             bFM0P_GPIO_ADE_AN03=0u; }while(0)

Definition at line 409 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P13_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P13=(v) )

Definition at line 398 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P14_GET ( bFM0P_GPIO_PDIR1_P14 )

Definition at line 437 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P14_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P14_INITIN(v) \
                                                            : GPIO1PIN_P14_INITOUT(v) )

Definition at line 441 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P14_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P14=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P14=0u; \
                                             bFM0P_GPIO_PFR1_P14=0u; \
                                             bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 444 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P14_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P14=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P14=1u; \
                                             bFM0P_GPIO_PFR1_P14=0u; \
                                             bFM0P_GPIO_ADE_AN04=0u; }while(0)

Definition at line 450 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P14_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P14=(v) )

Definition at line 439 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P15_GET ( bFM0P_GPIO_PDIR1_P15 )

Definition at line 478 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P15_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P15_INITIN(v) \
                                                            : GPIO1PIN_P15_INITOUT(v) )

Definition at line 482 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P15_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR1_P15=(v).bPullup; \
                                             bFM0P_GPIO_DDR1_P15=0u; \
                                             bFM0P_GPIO_PFR1_P15=0u; \
                                             bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 485 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P15_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR1_P15=(v).bInitVal; \
                                             bFM0P_GPIO_DDR1_P15=1u; \
                                             bFM0P_GPIO_PFR1_P15=0u; \
                                             bFM0P_GPIO_ADE_AN05=0u; }while(0)

Definition at line 491 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P15_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR1_P15=(v) )

Definition at line 480 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P21_GET ( bFM0P_GPIO_PDIR2_P21 )

Definition at line 519 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P21_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P21_INITIN(v) \
                                                            : GPIO1PIN_P21_INITOUT(v) )

Definition at line 523 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P21_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P21=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P21=0u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 526 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P21_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P21=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P21=1u; \
                                             bFM0P_GPIO_PFR2_P21=0u; }while(0)

Definition at line 530 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P21_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P21=(v) )

Definition at line 521 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P22_GET ( bFM0P_GPIO_PDIR2_P22 )

Definition at line 554 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P22_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P22_INITIN(v) \
                                                            : GPIO1PIN_P22_INITOUT(v) )

Definition at line 558 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P22_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P22=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P22=0u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 561 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P22_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P22=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P22=1u; \
                                             bFM0P_GPIO_PFR2_P22=0u; \
                                             bFM0P_GPIO_ADE_AN07=0u; }while(0)

Definition at line 567 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P22_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P22=(v) )

Definition at line 556 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P23_GET ( bFM0P_GPIO_PDIR2_P23 )

Definition at line 595 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P23_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P23_INITIN(v) \
                                                            : GPIO1PIN_P23_INITOUT(v) )

Definition at line 599 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P23_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR2_P23=(v).bPullup; \
                                             bFM0P_GPIO_DDR2_P23=0u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 602 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P23_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR2_P23=(v).bInitVal; \
                                             bFM0P_GPIO_DDR2_P23=1u; \
                                             bFM0P_GPIO_PFR2_P23=0u; \
                                             bFM0P_GPIO_ADE_AN06=0u; }while(0)

Definition at line 608 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P23_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR2_P23=(v) )

Definition at line 597 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P39_GET ( bFM0P_GPIO_PDIR3_P39 )

Definition at line 636 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P39_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P39_INITIN(v) \
                                                            : GPIO1PIN_P39_INITOUT(v) )

Definition at line 640 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P39_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P39=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P39=0u; \
                                             bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 643 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P39_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P39=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P39=1u; \
                                             bFM0P_GPIO_PFR3_P39=0u; }while(0)

Definition at line 647 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P39_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P39=(v) )

Definition at line 638 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3A_GET ( bFM0P_GPIO_PDIR3_P3A )

Definition at line 671 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3A_INITIN(v) \
                                                            : GPIO1PIN_P3A_INITOUT(v) )

Definition at line 675 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3A=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3A=0u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 678 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3A=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3A=1u; \
                                             bFM0P_GPIO_PFR3_P3A=0u; }while(0)

Definition at line 682 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3A=(v) )

Definition at line 673 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3B_GET ( bFM0P_GPIO_PDIR3_P3B )

Definition at line 706 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3B_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3B_INITIN(v) \
                                                            : GPIO1PIN_P3B_INITOUT(v) )

Definition at line 710 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3B_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3B=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3B=0u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 713 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3B_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3B=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3B=1u; \
                                             bFM0P_GPIO_PFR3_P3B=0u; }while(0)

Definition at line 717 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3B_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3B=(v) )

Definition at line 708 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3C_GET ( bFM0P_GPIO_PDIR3_P3C )

Definition at line 741 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3C_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3C_INITIN(v) \
                                                            : GPIO1PIN_P3C_INITOUT(v) )

Definition at line 745 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3C_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3C=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3C=0u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 748 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3C_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3C=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3C=1u; \
                                             bFM0P_GPIO_PFR3_P3C=0u; }while(0)

Definition at line 752 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3C_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3C=(v) )

Definition at line 743 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3D_GET ( bFM0P_GPIO_PDIR3_P3D )

Definition at line 776 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3D_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3D_INITIN(v) \
                                                            : GPIO1PIN_P3D_INITOUT(v) )

Definition at line 780 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3D_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3D=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3D=0u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 783 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3D_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3D=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3D=1u; \
                                             bFM0P_GPIO_PFR3_P3D=0u; }while(0)

Definition at line 787 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3D_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3D=(v) )

Definition at line 778 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3E_GET ( bFM0P_GPIO_PDIR3_P3E )

Definition at line 811 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3E_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3E_INITIN(v) \
                                                            : GPIO1PIN_P3E_INITOUT(v) )

Definition at line 815 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3E_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3E=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3E=0u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 818 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3E_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3E=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3E=1u; \
                                             bFM0P_GPIO_PFR3_P3E=0u; }while(0)

Definition at line 822 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3E_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3E=(v) )

Definition at line 813 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3F_GET ( bFM0P_GPIO_PDIR3_P3F )

Definition at line 846 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3F_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P3F_INITIN(v) \
                                                            : GPIO1PIN_P3F_INITOUT(v) )

Definition at line 850 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3F_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR3_P3F=(v).bPullup; \
                                             bFM0P_GPIO_DDR3_P3F=0u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 853 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3F_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR3_P3F=(v).bInitVal; \
                                             bFM0P_GPIO_DDR3_P3F=1u; \
                                             bFM0P_GPIO_PFR3_P3F=0u; }while(0)

Definition at line 857 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P3F_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR3_P3F=(v) )

Definition at line 848 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P46_GET ( bFM0P_GPIO_PDIR4_P46 )

Definition at line 881 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P46_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P46_INITIN(v) \
                                                            : GPIO1PIN_P46_INITOUT(v) )

Definition at line 885 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P46_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P46=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P46=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 888 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P46_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P46=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P46=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P46=0u; }while(0)

Definition at line 894 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P46_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P46=(v) )

Definition at line 883 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P47_GET ( bFM0P_GPIO_PDIR4_P47 )

Definition at line 924 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P47_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P47_INITIN(v) \
                                                            : GPIO1PIN_P47_INITOUT(v) )

Definition at line 928 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P47_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P47=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P47=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 931 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P47_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P47=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P47=1u; \
                                             bFM0P_GPIO_SPSR_SUBXC0=0u; \
                                             bFM0P_GPIO_SPSR_SUBXC1=0u; \
                                             bFM0P_GPIO_PFR4_P47=0u; }while(0)

Definition at line 937 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P47_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P47=(v) )

Definition at line 926 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P49_GET ( bFM0P_GPIO_PDIR4_P49 )

Definition at line 967 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P49_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P49_INITIN(v) \
                                                            : GPIO1PIN_P49_INITOUT(v) )

Definition at line 971 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P49_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P49=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P49=0u; \
                                             bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 974 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P49_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P49=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P49=1u; \
                                             bFM0P_GPIO_PFR4_P49=0u; }while(0)

Definition at line 978 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P49_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P49=(v) )

Definition at line 969 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P4A_GET ( bFM0P_GPIO_PDIR4_P4A )

Definition at line 1002 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P4A_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P4A_INITIN(v) \
                                                            : GPIO1PIN_P4A_INITOUT(v) )

Definition at line 1006 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P4A_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR4_P4A=(v).bPullup; \
                                             bFM0P_GPIO_DDR4_P4A=0u; \
                                             bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 1009 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P4A_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR4_P4A=(v).bInitVal; \
                                             bFM0P_GPIO_DDR4_P4A=1u; \
                                             bFM0P_GPIO_PFR4_P4A=0u; }while(0)

Definition at line 1013 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P4A_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR4_P4A=(v) )

Definition at line 1004 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P50_GET ( bFM0P_GPIO_PDIR5_P50 )

Definition at line 1037 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P50_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P50_INITIN(v) \
                                                            : GPIO1PIN_P50_INITOUT(v) )

Definition at line 1041 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P50_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P50=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P50=0u; \
                                             bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 1044 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P50_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P50=(v).bInitVal; \
                                             bFM0P_GPIO_DDR5_P50=1u; \
                                             bFM0P_GPIO_PFR5_P50=0u; }while(0)

Definition at line 1048 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P50_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P50=(v) )

Definition at line 1039 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P51_GET ( bFM0P_GPIO_PDIR5_P51 )

Definition at line 1072 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P51_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P51_INITIN(v) \
                                                            : GPIO1PIN_P51_INITOUT(v) )

Definition at line 1076 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P51_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P51=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P51=0u; \
                                             bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 1079 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P51_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P51=(v).bInitVal; \
                                             bFM0P_GPIO_DDR5_P51=1u; \
                                             bFM0P_GPIO_PFR5_P51=0u; }while(0)

Definition at line 1083 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P51_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P51=(v) )

Definition at line 1074 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P52_GET ( bFM0P_GPIO_PDIR5_P52 )

Definition at line 1107 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P52_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P52_INITIN(v) \
                                                            : GPIO1PIN_P52_INITOUT(v) )

Definition at line 1111 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P52_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR5_P52=(v).bPullup; \
                                             bFM0P_GPIO_DDR5_P52=0u; \
                                             bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 1114 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P52_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR5_P52=(v).bInitVal; \
                                             bFM0P_GPIO_DDR5_P52=1u; \
                                             bFM0P_GPIO_PFR5_P52=0u; }while(0)

Definition at line 1118 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P52_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR5_P52=(v) )

Definition at line 1109 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P60_GET ( bFM0P_GPIO_PDIR6_P60 )

Definition at line 1142 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P60_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P60_INITIN(v) \
                                                            : GPIO1PIN_P60_INITOUT(v) )

Definition at line 1146 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P60_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P60=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P60=0u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1149 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P60_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P60=(v).bInitVal; \
                                             bFM0P_GPIO_DDR6_P60=1u; \
                                             bFM0P_GPIO_PFR6_P60=0u; }while(0)

Definition at line 1153 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P60_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P60=(v) )

Definition at line 1144 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P61_GET ( bFM0P_GPIO_PDIR6_P61 )

Definition at line 1177 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P61_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P61_INITIN(v) \
                                                            : GPIO1PIN_P61_INITOUT(v) )

Definition at line 1181 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P61_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR6_P61=(v).bPullup; \
                                             bFM0P_GPIO_DDR6_P61=0u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1184 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P61_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR6_P61=(v).bInitVal; \
                                             bFM0P_GPIO_DDR6_P61=1u; \
                                             bFM0P_GPIO_PFR6_P61=0u; }while(0)

Definition at line 1188 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P61_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR6_P61=(v) )

Definition at line 1179 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P80_GET ( bFM0P_GPIO_PDIR8_P80 )

Definition at line 1212 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P80_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P80_INITIN(v) \
                                                            : GPIO1PIN_P80_INITOUT(v) )

Definition at line 1216 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P80_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P80=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P80=0u; \
                                             bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 1219 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P80_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P80=(v).bInitVal; \
                                             bFM0P_GPIO_DDR8_P80=1u; \
                                             bFM0P_GPIO_PFR8_P80=0u; }while(0)

Definition at line 1223 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P80_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P80=(v) )

Definition at line 1214 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P81_GET ( bFM0P_GPIO_PDIR8_P81 )

Definition at line 1247 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P81_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P81_INITIN(v) \
                                                            : GPIO1PIN_P81_INITOUT(v) )

Definition at line 1251 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P81_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P81=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P81=0u; \
                                             bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 1254 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P81_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P81=(v).bInitVal; \
                                             bFM0P_GPIO_DDR8_P81=1u; \
                                             bFM0P_GPIO_PFR8_P81=0u; }while(0)

Definition at line 1258 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P81_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P81=(v) )

Definition at line 1249 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P82_GET ( bFM0P_GPIO_PDIR8_P82 )

Definition at line 1282 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P82_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_P82_INITIN(v) \
                                                            : GPIO1PIN_P82_INITOUT(v) )

Definition at line 1286 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P82_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCR8_P82=(v).bPullup; \
                                             bFM0P_GPIO_DDR8_P82=0u; \
                                             bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 1289 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P82_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDOR8_P82=(v).bInitVal; \
                                             bFM0P_GPIO_DDR8_P82=1u; \
                                             bFM0P_GPIO_PFR8_P82=0u; }while(0)

Definition at line 1293 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_P82_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDOR8_P82=(v) )

Definition at line 1284 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE0_GET ( bFM0P_GPIO_PDIRE_PE0 )

Definition at line 1317 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE0_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE0_INITIN(v) \
                                                            : GPIO1PIN_PE0_INITOUT(v) )

Definition at line 1321 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE0_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE0=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE0=0u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1324 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE0_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE0=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE0=1u; \
                                             bFM0P_GPIO_PFRE_PE0=0u; }while(0)

Definition at line 1328 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE0_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE0=(v) )

Definition at line 1319 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE2_GET ( bFM0P_GPIO_PDIRE_PE2 )

Definition at line 1352 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE2_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE2_INITIN(v) \
                                                            : GPIO1PIN_PE2_INITOUT(v) )

Definition at line 1356 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE2_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE2=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE2=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1359 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE2_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE2=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE2=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE2=0u; }while(0)

Definition at line 1365 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE2_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE2=(v) )

Definition at line 1354 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE3_GET ( bFM0P_GPIO_PDIRE_PE3 )

Definition at line 1395 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE3_INIT | ( |  | v | ) |

Value:

    ( (0==(v).bOutput) ? GPIO1PIN_PE3_INITIN(v) \
                                                            : GPIO1PIN_PE3_INITOUT(v) )

Definition at line 1399 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE3_INITIN | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PCRE_PE3=(v).bPullup; \
                                             bFM0P_GPIO_DDRE_PE3=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1402 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE3_INITOUT | ( |  | v | ) |

Value:

    do{ bFM0P_GPIO_PDORE_PE3=(v).bInitVal; \
                                             bFM0P_GPIO_DDRE_PE3=1u; \
                                             bFM0P_GPIO_SPSR_MAINXC0=0u; \
                                             bFM0P_GPIO_SPSR_MAINXC1=0u; \
                                             bFM0P_GPIO_PFRE_PE3=0u; }while(0)

Definition at line 1408 of file gpio_s6e1a1xc0a.h.

#define GPIO1PIN_PE3_PUT | ( |  | v | ) | ( bFM0P_GPIO_PDORE_PE3=(v) )

Definition at line 1397 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_1_ADC0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 12u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 2821 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_1_ADC1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 16u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 2825 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_1_ADC2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 20u, 4u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 2829 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_2_ADC0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 12u, 4u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P39 = 1u; }while(0)

Definition at line 2833 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_2_ADC1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 16u, 4u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P39 = 1u; }while(0)

Definition at line 2837 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ADTG_2_ADC2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 20u, 4u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P39 = 1u; }while(0)

Definition at line 2841 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 2845 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 2849 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AIN0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR5_P50 = 1u; }while(0)

Definition at line 2854 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 0u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QAIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 2858 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN00 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN00 = 1 )

Definition at line 3319 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN01 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN01 = 1 )

Definition at line 3322 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN02 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN02 = 1 )

Definition at line 3325 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN03 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN03 = 1 )

Definition at line 3328 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN04 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN04 = 1 )

Definition at line 3331 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN05 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN05 = 1 )

Definition at line 3334 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN06 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN06 = 1 )

Definition at line 3337 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_AN07 | ( |  | dummy | ) | ( bFM0P_GPIO_ADE_AN07 = 1 )

Definition at line 3340 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_BIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 2863 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_BIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 2867 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_BIN0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR5_P51 = 1u; }while(0)

Definition at line 2871 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_BIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 2u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QBIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 2875 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_CROUT_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 1u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 2880 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_DTTI0X_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 16u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P39 = 1u; }while(0)

Definition at line 2884 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_DTTI0X_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 16u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 2888 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_DTTI0X_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 16u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 2892 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_FRCK0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 18u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 2896 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_FRCK0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 18u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR8_P80 = 1u; }while(0)

Definition at line 2900 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_FRCK0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 18u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 2904 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC00_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 20u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 2909 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC00_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 20u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 2913 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC01_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 23u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR5_P50 = 1u; }while(0)

Definition at line 2918 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC01_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 23u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 2922 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC01_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 23u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 2926 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC02_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 26u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 2931 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC02_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 26u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 2936 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC02_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 26u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P14 = 1u; \
                                                     bFM0P_GPIO_ADE_AN04 = 0u; }while(0)

Definition at line 2941 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC03_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 29u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 2946 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IC03_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 29u, 3u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P15 = 1u; \
                                                     bFM0P_GPIO_ADE_AN05 = 0u; }while(0)

Definition at line 2951 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IGTRG0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 13u, 1u, 0x00u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 2956 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_IGTRG0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 13u, 1u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 2960 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT00_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 0u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR5_P50 = 1u; }while(0)

Definition at line 2964 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT00_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 0u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 2968 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT01_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR5_P51 = 1u; }while(0)

Definition at line 2973 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT01_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 2977 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT02_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR5_P52 = 1u; }while(0)

Definition at line 2982 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT02_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 2986 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT02_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFRE_PE0 = 1u; }while(0)

Definition at line 2991 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT03_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 2995 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT03_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 6u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P14 = 1u; \
                                                     bFM0P_GPIO_ADE_AN04 = 0u; }while(0)

Definition at line 2999 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT03_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 3004 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT04_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3008 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT04_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 8u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 3012 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT05_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3017 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT05_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 3021 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT06_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 12u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 3026 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT06_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 3030 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT15_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 30u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 3034 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT15_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 30u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 3038 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_INT15_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR06, 30u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR1_P15 = 1u; \
                                                     bFM0P_GPIO_ADE_AN05 = 0u; }while(0)

Definition at line 3042 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_NMIX | ( |  | dummy | ) |

Value:

    do{ bFM0P_GPIO_EPFR00_NMIS = 1; \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 3047 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTCCO_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 3051 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTCCO_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 3055 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTCCO_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 3060 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO00_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 0u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 3064 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO01_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3068 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO02_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3072 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO03_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 3076 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO04_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 3080 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_RTO05_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR01, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 3084 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 3088 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 8u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 3093 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 14u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 3097 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK1_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 14u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR8_P80 = 1u; }while(0)

Definition at line 3102 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 26u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 3106 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK3_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 26u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR5_P52 = 1u; }while(0)

Definition at line 3110 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCK3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 26u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 3114 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS10_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P14 = 1u; \
                                                     bFM0P_GPIO_ADE_AN04 = 0u; }while(0)

Definition at line 3118 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS10_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 3123 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS11_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 6u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P15 = 1u; \
                                                     bFM0P_GPIO_ADE_AN05 = 0u; }while(0)

Definition at line 3127 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS11_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 3132 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS30_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 12u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3136 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SCS31_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR22, 14u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3140 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 3144 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P14 = 1u; \
                                                     bFM0P_GPIO_ADE_AN04 = 0u; }while(0)

Definition at line 3148 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3153 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P11 = 1u; \
                                                     bFM0P_GPIO_ADE_AN01 = 0u; }while(0)

Definition at line 3157 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN1_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 10u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR8_P82 = 1u; }while(0)

Definition at line 3162 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 22u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 3166 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN3_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 22u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR5_P50 = 1u; }while(0)

Definition at line 3170 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SIN3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 22u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 3174 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 3178 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 6u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P15 = 1u; \
                                                     bFM0P_GPIO_ADE_AN05 = 0u; }while(0)

Definition at line 3183 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3188 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT1_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P12 = 1u; \
                                                     bFM0P_GPIO_ADE_AN02 = 0u; }while(0)

Definition at line 3192 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT1_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 12u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR8_P81 = 1u; }while(0)

Definition at line 3197 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT3_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 24u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 3201 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT3_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 24u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR5_P51 = 1u; }while(0)

Definition at line 3205 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SOT3_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR07, 24u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 3209 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SUBOUT_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR0_P0F = 1u; }while(0)

Definition at line 3213 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SUBOUT_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR1_P13 = 1u; \
                                                     bFM0P_GPIO_ADE_AN03 = 0u; }while(0)

Definition at line 3217 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_SUBOUT_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR00, 6u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 3222 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA0_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 2u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3E = 1u; }while(0)

Definition at line 3226 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA0_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 2u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3A = 1u; }while(0)

Definition at line 3230 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA1_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 8u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 3234 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA1_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 10u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 3238 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA1_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 8u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3242 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA1_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 10u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3B = 1u; }while(0)

Definition at line 3246 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA2_0_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P23 = 1u; \
                                                     bFM0P_GPIO_ADE_AN06 = 0u; }while(0)

Definition at line 3250 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA2_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3255 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA2_2_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 18u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P60 = 1u; }while(0)

Definition at line 3259 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA3_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 24u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 3263 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOA3_1_OUT | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 26u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR3_P3D = 1u; }while(0)

Definition at line 3267 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB0_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 4u, 3u, 0x01u ); \
                                                     bFM0P_GPIO_PFR4_P49 = 1u; }while(0)

Definition at line 3271 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB0_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 4u, 3u, 0x02u ); \
                                                     bFM0P_GPIO_PFR0_P04 = 1u; }while(0)

Definition at line 3275 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB1_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 12u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR4_P4A = 1u; }while(0)

Definition at line 3279 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB1_1_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 12u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P21 = 1u; }while(0)

Definition at line 3283 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB2_0_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 20u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 3287 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_TIOB2_2_IN | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR04, 20u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR6_P61 = 1u; }while(0)

Definition at line 3292 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ZIN0_0 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x01u ); \
                                                     bFM0P_GPIO_PFR3_P3F = 1u; }while(0)

Definition at line 3296 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ZIN0_1 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x02u ); \
                                                     bFM0P_GPIO_PFR2_P22 = 1u; \
                                                     bFM0P_GPIO_ADE_AN07 = 0u; }while(0)

Definition at line 3300 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ZIN0_2 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x03u ); \
                                                     bFM0P_GPIO_PFR5_P52 = 1u; }while(0)

Definition at line 3305 of file gpio_s6e1a1xc0a.h.

#define SetPinFunc_ZIN0_3 | ( |  | dummy | ) |

Value:

    do{ PINRELOC_SET_EPFR( FM0P_GPIO->EPFR09, 4u, 2u, 0x00u ); \
                                                     bFM0P_GPIO_EPFR21_QZIN0S = 1u; \
                                                     bFM0P_GPIO_PFR3_P3C = 1u; }while(0)

Definition at line 3309 of file gpio_s6e1a1xc0a.h.