| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_bt_rt_config Struct Reference
Base Timer (BT)

Structure of Reload timer configuration. More...

`#include <bt.h>`

## Data Fields
en_rt_clock_pres_t | enPres
| Clock prescaler.
en_rt_timer_size_t | enSize
| 16-bit or 32-bit
en_rt_ext_trigger_t | enExtTrig
| External trigger setting.
en_rt_output_polarity_t | enOutputPolarity
| Output polarity setting.
en_rt_mode_t | enMode
| Reload mode or one-shot mode.

## Detailed Description

Structure of Reload timer configuration.

Definition at line 700 of file bt.h.

## Field Documentation

en_rt_ext_trigger_t enExtTrig

External trigger setting.

Definition at line 704 of file bt.h.

Referenced by Bt_Rt_Init().

en_rt_mode_t enMode

Reload mode or one-shot mode.

Definition at line 706 of file bt.h.

Referenced by Bt_Rt_Init().

en_rt_output_polarity_t enOutputPolarity

Output polarity setting.

Definition at line 705 of file bt.h.

Referenced by Bt_Rt_Init().

en_rt_clock_pres_t enPres

Clock prescaler.

Definition at line 702 of file bt.h.

Referenced by Bt_Rt_Init().

en_rt_timer_size_t enSize

16-bit or 32-bit

Definition at line 703 of file bt.h.

Referenced by Bt_Rt_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h