| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_adc_prio Struct Reference
12-Bit Analog Digital Converter (ADC)

Priority Conversion configuration. More...

`#include <adc.h>`

## Data Fields
boolean_t | bPrioExtTrigStartEnable
| TRUE: Triggers Prioritys Conversion on falling edge of external signal.
boolean_t | bPrioTimerStartEnable
| TRUE: Triggers Priority Conversion by Timer.
en_adc_timer_select_t | enPrioTimerTrigger
| See en_adc_timer_select_t for details.
uint8_t | u8PrioFifoDepth
| Depth of the Priority Conversion FIFO 0...3.
uint8_t | u8PrioLevel1AnalogChSel
| Priority Level 1 Analog Channel Selector Ch. 0...7.
uint8_t | u8PrioLevel2AnalogChSel
| Priority Level 2 Analog Channel Selector Ch. 0...31.

## Detailed Description

Priority Conversion configuration.

Definition at line 287 of file adc.h.

## Field Documentation

boolean_t bPrioExtTrigStartEnable

TRUE: Triggers Prioritys Conversion on falling edge of external signal.

Definition at line 289 of file adc.h.

Referenced by Adc_Init().

boolean_t bPrioTimerStartEnable

TRUE: Triggers Priority Conversion by Timer.

Definition at line 290 of file adc.h.

Referenced by Adc_Init().

en_adc_timer_select_t enPrioTimerTrigger

See en_adc_timer_select_t for details.

Definition at line 291 of file adc.h.

Referenced by Adc_Init().

uint8_t u8PrioFifoDepth

Depth of the Priority Conversion FIFO 0...3.

Definition at line 292 of file adc.h.

Referenced by Adc_Init().

uint8_t u8PrioLevel1AnalogChSel

Priority Level 1 Analog Channel Selector Ch. 0...7.

Definition at line 293 of file adc.h.

Referenced by Adc_Init().

uint8_t u8PrioLevel2AnalogChSel

Priority Level 2 Analog Channel Selector Ch. 0...31.

Definition at line 294 of file adc.h.

Referenced by Adc_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/adc/adc.h