| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_lin_int_sel Struct Reference
Multi Function Serial Interface (MFS)

LIN interrupt selection. More...

`#include <mfs.h>`

## Data Fields
boolean_t | bTxInt
| LIN TX interrupt.
boolean_t | bRxInt
| LIN RX interrupt.
boolean_t | bLinBreakInt
| LIN break field interrupt.
boolean_t | bTxIdle
| LIN TX idle interrupt.
boolean_t | bTxFifoInt
| LIN TX FIFO interrupt.

## Detailed Description

LIN interrupt selection.

Definition at line 1000 of file mfs.h.

## Field Documentation

boolean_t bLinBreakInt

LIN break field interrupt.

Definition at line 1004 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), and Mfs_Lin_EnableInt().

boolean_t bRxInt

LIN RX interrupt.

Definition at line 1003 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), and Mfs_Lin_EnableInt().

boolean_t bTxFifoInt

LIN TX FIFO interrupt.

Definition at line 1006 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), and Mfs_Lin_EnableInt().

boolean_t bTxIdle

LIN TX idle interrupt.

Definition at line 1005 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), and Mfs_Lin_EnableInt().

boolean_t bTxInt

LIN TX interrupt.

Definition at line 1002 of file mfs.h.

Referenced by Mfs_Lin_DisableInt(), and Mfs_Lin_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h