| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_i2c_int_sel Struct Reference
Multi Function Serial Interface (MFS)

I2C interrupt selection. More...

`#include <mfs.h>`

## Data Fields
boolean_t | bTxInt
| I2C TX interrupt.
boolean_t | bRxInt
| I2C RX interrupt.
boolean_t | bTxIdle
| I2C TX idle interrupt.
boolean_t | bTxFifoInt
| I2C TX FIFO interrupt.
boolean_t | bTxRxInt
| I2C TX and RX interrupt.
boolean_t | bStopDetectInt
| I2C stop condition interrupt.

## Detailed Description

I2C interrupt selection.

Definition at line 861 of file mfs.h.

## Field Documentation

boolean_t bRxInt

I2C RX interrupt.

Definition at line 864 of file mfs.h.

Referenced by I2cRxData(), I2cStopDetectCallback(), I2cTxRxData(), Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

boolean_t bStopDetectInt

I2C stop condition interrupt.

Definition at line 868 of file mfs.h.

Referenced by I2cRxData(), I2cStopDetectCallback(), I2cTxData(), I2cTxRxData(), Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

boolean_t bTxFifoInt

I2C TX FIFO interrupt.

Definition at line 866 of file mfs.h.

Referenced by Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

boolean_t bTxIdle

I2C TX idle interrupt.

Definition at line 865 of file mfs.h.

Referenced by Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

boolean_t bTxInt

I2C TX interrupt.

Definition at line 863 of file mfs.h.

Referenced by I2cRxData(), I2cStopDetectCallback(), I2cTxCallback(), I2cTxData(), I2cTxRxData(), Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

boolean_t bTxRxInt

I2C TX and RX interrupt.

Definition at line 867 of file mfs.h.

Referenced by I2cRxData(), I2cStopDetectCallback(), I2cTxData(), I2cTxRxData(), Mfs_I2c_DisableInt(), and Mfs_I2c_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h