| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_mfs_fifo_config Struct Reference
Multi Function Serial Interface (MFS)

Mfs FIFO configuration. More...

`#include <mfs.h>`

## Data Fields
en_mfs_fifo_sel_t | enFifoSel
| FIFO selection, see en_mfs_fifo_sel_t for details.
uint8_t | u8ByteCount1
| Transfer data count for FIFO1.
uint8_t | u8ByteCount2
| Transfer data count for FIFO2.

## Detailed Description

Mfs FIFO configuration.

Definition at line 437 of file mfs.h.

## Field Documentation

en_mfs_fifo_sel_t enFifoSel

FIFO selection, see en_mfs_fifo_sel_t for details.

Definition at line 439 of file mfs.h.

Referenced by Mfs_Csio_Init(), Mfs_I2c_Init(), Mfs_Lin_Init(), and Mfs_Uart_Init().

uint8_t u8ByteCount1

Transfer data count for FIFO1.

Definition at line 440 of file mfs.h.

Referenced by Mfs_Csio_Init(), Mfs_I2c_Init(), Mfs_Lin_Init(), and Mfs_Uart_Init().

uint8_t u8ByteCount2

Transfer data count for FIFO2.

Definition at line 441 of file mfs.h.

Referenced by Mfs_Csio_Init(), Mfs_I2c_Init(), Mfs_Lin_Init(), and Mfs_Uart_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h