| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_dma_intern_data Struct Reference
Direct Memory Access (DMA)

Datatype for holding internal data needed for DMA. More...

`#include <dma.h>`

## Data Fields
func_ptr_t | apfnDmaCallback [(4u)]
| Callback pointer array.
func_ptr_arg1_t | apfnDmaErrorCallback [(4u)]
| Error Callback pointer array.

## Detailed Description

Datatype for holding internal data needed for DMA.

Definition at line 214 of file dma.h.

## Field Documentation

func_ptr_t apfnDmaCallback[(4u)]

Callback pointer array.

Definition at line 216 of file dma.h.

Referenced by Dma_DisableInt(), Dma_EnableInt(), and DmaIrqHandler().

func_ptr_arg1_t apfnDmaErrorCallback[(4u)]

Error Callback pointer array.

Definition at line 217 of file dma.h.

Referenced by Dma_DisableInt(), Dma_EnableInt(), and DmaIrqHandler().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/dma/dma.h