| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_mft_ocu_config Struct Reference
Output Compare Unit (OCU)

OCU configure. More...

`#include <mft_ocu.h>`

## Data Fields
en_mft_ocu_frt_t | enFrtConnect
| select the FRT to be connected to OCU
boolean_t | bFm4
| select FM0P mode or FM3-compatible mode
boolean_t | bCmod
| FM3 compatible mode.
uint8_t | u8Mod
| select OCU ch0~ch5 in FM3 compatible
en_ocu_occp_buf_t | enOccpBufMode
| buffer register function of OCCP
en_ocu_ocse_buf_t | enOcseBufMode
| buffer register function of OCSE
en_ocu_rt_out_state_t | enStatePin
| RT output level state.

## Detailed Description

OCU configure.

Definition at line 211 of file mft_ocu.h.

## Field Documentation

boolean_t bCmod

FM3 compatible mode.

Definition at line 215 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

boolean_t bFm4

select FM0P mode or FM3-compatible mode

Definition at line 214 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

en_mft_ocu_frt_t enFrtConnect

select the FRT to be connected to OCU

Definition at line 213 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

en_ocu_occp_buf_t enOccpBufMode

buffer register function of OCCP

Definition at line 217 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

en_ocu_ocse_buf_t enOcseBufMode

buffer register function of OCSE

Definition at line 218 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

en_ocu_rt_out_state_t enStatePin

RT output level state.

Definition at line 219 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

uint8_t u8Mod

select OCU ch0~ch5 in FM3 compatible

Definition at line 216 of file mft_ocu.h.

Referenced by Mft_Ocu_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mft/mft_ocu.h