<map id="G" name="G">
<area shape="rect" id="node2" href="$group___mfs_group.html#ga19aa99d2c86e36d0ef7883339d792176" title="Enable CSIO interrupts." alt="" coords="136,132,269,159"/>
<area shape="rect" id="node14" href="$group___mfs_group.html#ga0f86c7248bdc67e81d03ebc702043478" title="Enable I2C interrupts." alt="" coords="139,385,266,412"/>
<area shape="rect" id="node23" href="$group___mfs_group.html#ga50bccbb67053fbfa6d3b9be8b5cb07ed" title="Enable LIN interrupts." alt="" coords="140,436,265,463"/>
<area shape="rect" id="node24" href="$group___mfs_group.html#ga20659bc423794dfc8739f148e8abfbee" title="Enable UART interrupts." alt="" coords="136,487,269,513"/>
<area shape="rect" id="node3" href="$csio__int__s25fl127s_8c.html#a8d96de1f8acdd5f446026cccd7ee8e0b" title="Read data from S25FL127S." alt="" coords="331,208,418,235"/>
<area shape="rect" id="node6" href="$csio__int__s25fl127s_8c.html#a1080b0f6949d30ea901a3f8225f9787f" title="Read register from S25FL127S." alt="" coords="333,56,416,83"/>
<area shape="rect" id="node11" href="$csio__int__s25fl127s_8c.html#a42260569e48834e4d5bc3bb2a9c3f970" title="Write command only to S25FL127S." alt="" coords="331,107,418,133"/>
<area shape="rect" id="node12" href="$csio__int__s25fl127s_8c.html#aa2ae015adaa95e1c422a5fac316eb1e9" title="Write command and address only to S25FL127S." alt="" coords="318,5,431,32"/>
<area shape="rect" id="node13" href="$csio__int__s25fl127s_8c.html#a3da7a5d796ca9b4041b0f6d46b116b87" title="Write command, address, data to S25FL127S." alt="" coords="331,157,418,184"/>
<area shape="rect" id="node4" href="$csio__int__s25fl127s_8h.html#a9526b5938866a0bd96b1eeb85d716d09" title="Read data from S25FL127S." alt="" coords="509,208,624,235"/>
<area shape="rect" id="node5" href="$csio__int__s25fl127s_8h.html#a0bb140b1ceab26292bb08d17fd9af89d" title="Read ID from S25FL127S." alt="" coords="504,259,629,285"/>
<area shape="rect" id="node7" href="$csio__int__s25fl127s_8h.html#a598e7ad72ae67fa2bc12a359480356d4" title="Sector erase 4KB sector." alt="" coords="483,5,650,32"/>
<area shape="rect" id="node8" href="$csio__int__s25fl127s_8h.html#a95bb1cc75d33448c83cb69e5b4b3886d" title="Chip erase the whole Flash memory." alt="" coords="497,107,637,133"/>
<area shape="rect" id="node9" href="$csio__int__s25fl127s_8h.html#a178746052ef9e5abf9821063ec29da2c" title="Page program S25FL127S." alt="" coords="485,157,648,184"/>
<area shape="rect" id="node10" href="$csio__int__s25fl127s_8h.html#a4f813c900d86faa134d52d4831f4234d" title="Sector erase 64kB or 256kB sector." alt="" coords="489,56,644,83"/>
<area shape="rect" id="node15" href="$i2c__int__at24cxx_8c.html#acdc22353113e27336f95d90c71c1a547" title="Read I2C data." alt="" coords="335,360,414,387"/>
<area shape="rect" id="node18" href="$i2c__int__at24cxx_8c.html#aec4840a29d49b8335f98c801afebeaa5" title="Write I2C data." alt="" coords="335,411,414,437"/>
<area shape="rect" id="node21" href="$i2c__int__at24cxx_8c.html#a6f3d8082e6d0f2a24634e10883ebadfe" title="Perform a dummy write and read at the following." alt="" coords="328,487,421,513"/>
<area shape="rect" id="node16" href="$group___i2c_at24cxx_group.html#ga872adeb2f3933d08622518cc37ba6c28" title="Read the data of current data address of AT24CXX." alt="" coords="481,309,653,336"/>
<area shape="rect" id="node17" href="$group___i2c_at24cxx_group.html#gaf689ffe3a4e1bb250960398d88a882ba" title="Read data bytes following by random read or current address read." alt="" coords="485,360,648,387"/>
<area shape="rect" id="node19" href="$group___i2c_at24cxx_group.html#ga2b547e2af91d16a30b37d34f911f15c4" title="Write byte at a certain address of AT24CXX." alt="" coords="503,411,631,437"/>
<area shape="rect" id="node20" href="$group___i2c_at24cxx_group.html#ga6cd7eaff4e9287364feadd928305f15f" title="Write a page bytes at a page address of AT24CXX." alt="" coords="501,461,633,488"/>
<area shape="rect" id="node22" href="$group___i2c_at24cxx_group.html#ga18bfb67bb388fa8c996b6ac2b3dce006" title="Read a byte data of ramdon data address of AT24CXX." alt="" coords="492,512,641,539"/>
</map>
