<map id="G" name="G">
<area shape="rect" id="node2" href="$i2c__polling__at24cxx_8c.html#ad80ebff2a83ed7dcd8541a7b3113bfc6" title="Read I2C data." alt="" coords="206,31,274,57"/>
<area shape="rect" id="node6" href="$i2c__polling__at24cxx_8c.html#abf0e0cf12ff99a33b2a03dafc4bed27f" title="Generate I2C restart signal and send device address." alt="" coords="200,81,280,108"/>
<area shape="rect" id="node7" href="$i2c__polling__at24cxx_8c.html#a980779b9462a9ef16cb58d3b845dd256" title="Sene I2C data." alt="" coords="193,183,287,209"/>
<area shape="rect" id="node10" href="$i2c__polling__at24cxx_8c.html#a519a7e968f229a923f32be4cfd511109" title="Generate I2C start signal and send device address." alt="" coords="207,132,273,159"/>
<area shape="rect" id="node3" href="$group___i2c_at24cxx_group.html#ga872adeb2f3933d08622518cc37ba6c28" title="Read the data of current data address of AT24CXX." alt="" coords="337,56,509,83"/>
<area shape="rect" id="node4" href="$group___i2c_at24cxx_group.html#ga18bfb67bb388fa8c996b6ac2b3dce006" title="Read a byte data of ramdon data address of AT24CXX." alt="" coords="348,107,497,133"/>
<area shape="rect" id="node5" href="$group___i2c_at24cxx_group.html#gaf689ffe3a4e1bb250960398d88a882ba" title="Read data bytes following by random read or current address read." alt="" coords="341,5,504,32"/>
<area shape="rect" id="node8" href="$group___i2c_at24cxx_group.html#ga2b547e2af91d16a30b37d34f911f15c4" title="Write byte at a certain address of AT24CXX." alt="" coords="359,208,487,235"/>
<area shape="rect" id="node9" href="$group___i2c_at24cxx_group.html#ga6cd7eaff4e9287364feadd928305f15f" title="Write a page bytes at a page address of AT24CXX." alt="" coords="357,157,489,184"/>
</map>
