| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_mfsn Struct Reference
Multi Function Serial Interface (MFS)

MFS common instance structure. More...

`#include <mfs.h>`

## Data Fields
volatile FM0P_MFS_UART_TypeDef * | pstcUartInstance
| Pointer to UART instance.
volatile FM0P_MFS_CSIO_TypeDef * | pstcCsioInstance
| Pointer to CSIO instance.
volatile FM0P_MFS_I2C_TypeDef * | pstcI2cInstance
| Pointer to I2C instance.
volatile FM0P_MFS_LIN_TypeDef * | pstcLinInstance
| Pointer to LIN instance.

## Detailed Description

MFS common instance structure.

Definition at line 1117 of file mfs.h.

## Field Documentation

volatile FM0P_MFS_CSIO_TypeDef* pstcCsioInstance

Pointer to CSIO instance.

Definition at line 1120 of file mfs.h.

volatile FM0P_MFS_I2C_TypeDef* pstcI2cInstance

Pointer to I2C instance.

Definition at line 1121 of file mfs.h.

volatile FM0P_MFS_LIN_TypeDef* pstcLinInstance

Pointer to LIN instance.

Definition at line 1122 of file mfs.h.

volatile FM0P_MFS_UART_TypeDef* pstcUartInstance

Pointer to UART instance.

Definition at line 1119 of file mfs.h.

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/mfs/mfs.h