| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_ppg_igbt_config Struct Reference

structure of PPG IGBT configuration More...

`#include <ppg.h>`

## Data Fields
en_igbt_prohibition_mode_t | enMode
| prohibition mode
en_igbt_filter_width_t | enWidth
| noise filter width
en_igbt_level_t | enTrigInputLevel
| Trigger input level.
en_igbt_level_t | enIgbt0OutputLevel
| IGBT0 output level (PPG0)
en_igbt_level_t | enIgbt1OutputLevel
| IGBT1 output level (PPG4)

## Detailed Description

structure of PPG IGBT configuration

Definition at line 419 of file ppg.h.

## Field Documentation

en_igbt_level_t enIgbt0OutputLevel

IGBT0 output level (PPG0)

Definition at line 424 of file ppg.h.

Referenced by Ppg_InitIgbt().

en_igbt_level_t enIgbt1OutputLevel

IGBT1 output level (PPG4)

Definition at line 425 of file ppg.h.

Referenced by Ppg_InitIgbt().

en_igbt_prohibition_mode_t enMode

prohibition mode

Definition at line 421 of file ppg.h.

Referenced by Ppg_InitIgbt().

en_igbt_level_t enTrigInputLevel

Trigger input level.

Definition at line 423 of file ppg.h.

Referenced by Ppg_InitIgbt().

en_igbt_filter_width_t enWidth

noise filter width

Definition at line 422 of file ppg.h.

Referenced by Ppg_InitIgbt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/ppg/ppg.h