| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
un_dmac_dmacb_t Union Reference
Direct Memory Access (DMA)

## Data Fields
stc_dmac_dmacb0_field_t | stcDMACB
uint32_t | u32DMACB

## Detailed Description

Definition at line 91 of file dma.c.

## Field Documentation

stc_dmac_dmacb0_field_t stcDMACB

Definition at line 93 of file dma.c.

Referenced by Dma_DisableInt(), Dma_EnableInt(), Dma_GetStopCause(), and Dma_Init_Channel().

uint32_t u32DMACB

Definition at line 94 of file dma.c.

Referenced by Dma_DisableInt(), Dma_EnableInt(), Dma_GetStopCause(), and Dma_Init_Channel().

The documentation for this union was generated from the following file:

- C:/pdl_v10/library/driver/dma/dma.c