| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_rtc_timer Struct Reference
Real Time Clock (RTC)

Real Time Clock timer configuration structure. More...

`#include <rtc.h>`

## Data Fields
en_rtc_time_mode_t | enMode
| Timer mode.
uint32_t | u32TimerCycle
| The cycle [uint: second] of timer, after these seconds elapse, timer interrpt will occur.

## Detailed Description

Real Time Clock timer configuration structure.

Definition at line 264 of file rtc.h.

## Field Documentation

en_rtc_time_mode_t enMode

Timer mode.

Definition at line 266 of file rtc.h.

Referenced by Rtc_Init().

uint32_t u32TimerCycle

The cycle [uint: second] of timer, after these seconds elapse, timer interrpt will occur.

Definition at line 267 of file rtc.h.

Referenced by Rtc_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/rtc/rtc.h