| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_bt_intern_data Struct Reference
Base Timer (BT)

BT internal data. More...

`#include <bt.h>`

## Data Fields
func_ptr_t | pfnBit0IntCallback
| Pointer to callback function the interrupt reflected by bit0 of STC.
func_ptr_t | pfnBit1IntCallback
| Pointer to callback function the interrupt reflected by bit1 of STC.
func_ptr_t | pfnBit2IntCallback
| Pointer to callback function the interrupt reflected by bit2 of STC.

## Detailed Description

BT internal data.

Definition at line 846 of file bt.h.

## Field Documentation

func_ptr_t pfnBit0IntCallback

Pointer to callback function the interrupt reflected by bit0 of STC.

Definition at line 848 of file bt.h.

Referenced by Bt_IrqHandler(), Bt_Ppg_DisableInt(), Bt_Ppg_EnableInt(), Bt_Pwc_DisableInt(), Bt_Pwc_EnableInt(), Bt_Pwm_DisableInt(), Bt_Pwm_EnableInt(), Bt_Rt_DisableInt(), and Bt_Rt_EnableInt().

func_ptr_t pfnBit1IntCallback

Pointer to callback function the interrupt reflected by bit1 of STC.

Definition at line 849 of file bt.h.

Referenced by Bt_IrqHandler(), Bt_Pwm_DisableInt(), and Bt_Pwm_EnableInt().

func_ptr_t pfnBit2IntCallback

Pointer to callback function the interrupt reflected by bit2 of STC.

Definition at line 850 of file bt.h.

Referenced by Bt_IrqHandler(), Bt_Ppg_DisableInt(), Bt_Ppg_EnableInt(), Bt_Pwc_DisableInt(), Bt_Pwc_EnableInt(), Bt_Pwm_DisableInt(), Bt_Pwm_EnableInt(), Bt_Rt_DisableInt(), and Bt_Rt_EnableInt().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h