| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_bt_pwc_config Struct Reference
Base Timer (BT)

Structure of PWC timer configuration. More...

`#include <bt.h>`

## Data Fields
en_pwc_clock_pres_t | enPres
| Clock prescaler.
en_pwc_timer_size_t | enSize
| 16-bit or 32-bit
en_pwc_measure_edge_t | enMeasureEdge
| Measure mode setting.
en_pwc_mode_t | enMode
| Continuous mode or one-shot mode.

## Detailed Description

Structure of PWC timer configuration.

Definition at line 800 of file bt.h.

## Field Documentation

en_pwc_measure_edge_t enMeasureEdge

Measure mode setting.

Definition at line 804 of file bt.h.

Referenced by Bt_Pwc_Init().

en_pwc_mode_t enMode

Continuous mode or one-shot mode.

Definition at line 805 of file bt.h.

Referenced by Bt_Pwc_Init().

en_pwc_clock_pres_t enPres

Clock prescaler.

Definition at line 802 of file bt.h.

Referenced by Bt_Pwc_Init().

en_pwc_timer_size_t enSize

16-bit or 32-bit

Definition at line 803 of file bt.h.

Referenced by Bt_Pwc_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/bt/bt.h