| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_swwdg_config Struct Reference
Software Watchdog (SWWDG)

Software and Hardware Watchdog configuration. More...

`#include <swwdg.h>`

## Data Fields
uint32_t | u32LoadValue
| Timer interval.
boolean_t | bResetEnable
| TRUE: Enables SW watchdog reset.
boolean_t | bWinWdgEnable
| TRUE: Enables Window watchdog mode.
boolean_t | bWinWdgResetEnable
uint8_t | u8TimingWindow
| Timing window setting, see description of en_swwdg_timing_window_t.

## Detailed Description

Software and Hardware Watchdog configuration.

Definition at line 146 of file swwdg.h.

## Field Documentation

boolean_t bResetEnable

TRUE: Enables SW watchdog reset.

Definition at line 149 of file swwdg.h.

Referenced by Swwdg_Init().

boolean_t bWinWdgEnable

TRUE: Enables Window watchdog mode.

Definition at line 150 of file swwdg.h.

Referenced by Swwdg_Init().

boolean_t bWinWdgResetEnable

TRUE: Enables reset when reload without timing window was occured. FALSE: Enables interrupt when reload without timing window was occured.

Definition at line 151 of file swwdg.h.

Referenced by Swwdg_Init().

uint32_t u32LoadValue

Timer interval.

Definition at line 148 of file swwdg.h.

Referenced by Swwdg_Init().

uint8_t u8TimingWindow

Timing window setting, see description of en_swwdg_timing_window_t.

Definition at line 153 of file swwdg.h.

Referenced by Swwdg_Init().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/wdg/swwdg.h