| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_reset_result Struct Reference
Reset Factor (RESET)

Datatype for Reset Cause return structure. More...

`#include <reset.h>`

## Data Fields
boolean_t | bPowerOn
| TRUE: Power on reset ocurred.
boolean_t | bInitx
| TRUE: INITX (external) reset ocurred.
boolean_t | bSoftwareWatchdog
| TRUE: Software Watchdog reset ocurred.
boolean_t | bHardwareWatchdog
| TRUE: Hardware Watchdog reset ocurred.
boolean_t | bClockSupervisor
| TRUE: Clock Supervisor reset ocurred.
boolean_t | bAnomalousFrequency
| TRUE: Anomalous Frequency reset ocurred.
boolean_t | bSoftware
| TRUE: Software reset ocurred.

## Detailed Description

Datatype for Reset Cause return structure.

Definition at line 101 of file reset.h.

## Field Documentation

boolean_t bAnomalousFrequency

TRUE: Anomalous Frequency reset ocurred.

Definition at line 108 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bClockSupervisor

TRUE: Clock Supervisor reset ocurred.

Definition at line 107 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bHardwareWatchdog

TRUE: Hardware Watchdog reset ocurred.

Definition at line 106 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bInitx

TRUE: INITX (external) reset ocurred.

Definition at line 104 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bPowerOn

TRUE: Power on reset ocurred.

Definition at line 103 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bSoftware

TRUE: Software reset ocurred.

Definition at line 109 of file reset.h.

Referenced by Reset_GetCause().

boolean_t bSoftwareWatchdog

TRUE: Software Watchdog reset ocurred.

Definition at line 105 of file reset.h.

Referenced by Reset_GetCause().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/reset/reset.h