| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_timer2_gen_ch Struct Reference

Up counter2 stop channels selection. More...

`#include <ppg.h>`

## Data Fields
boolean_t | bPpgCh16
| 1: select Ch.16, 0: not selected
boolean_t | bPpgCh18
| 1: select Ch.18, 0: not selected
boolean_t | bPpgCh20
| 1: select Ch.20, 0: not selected
boolean_t | bPpgCh22
| 1: select Ch.22, 0: not selected

## Detailed Description

Up counter2 stop channels selection.

Definition at line 359 of file ppg.h.

## Field Documentation

boolean_t bPpgCh16

1: select Ch.16, 0: not selected

Definition at line 361 of file ppg.h.

Referenced by Ppg_DisableTimerGen2StartTrig().

boolean_t bPpgCh18

1: select Ch.18, 0: not selected

Definition at line 362 of file ppg.h.

Referenced by Ppg_DisableTimerGen2StartTrig().

boolean_t bPpgCh20

1: select Ch.20, 0: not selected

Definition at line 363 of file ppg.h.

Referenced by Ppg_DisableTimerGen2StartTrig().

boolean_t bPpgCh22

1: select Ch.22, 0: not selected

Definition at line 364 of file ppg.h.

Referenced by Ppg_DisableTimerGen2StartTrig().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/ppg/ppg.h