| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_timer1_gen_ch Struct Reference

Up counter1 stop channels selection. More...

`#include <ppg.h>`

## Data Fields
boolean_t | bPpgCh8
| 1: select Ch.8, 0: not selected
boolean_t | bPpgCh10
| 1: select Ch.10, 0: not selected
boolean_t | bPpgCh12
| 1: select Ch.12, 0: not selected
boolean_t | bPpgCh14
| 1: select Ch.14, 0: not selected

## Detailed Description

Up counter1 stop channels selection.

Definition at line 332 of file ppg.h.

## Field Documentation

boolean_t bPpgCh10

1: select Ch.10, 0: not selected

Definition at line 335 of file ppg.h.

Referenced by Ppg_DisableTimerGen1StartTrig().

boolean_t bPpgCh12

1: select Ch.12, 0: not selected

Definition at line 336 of file ppg.h.

Referenced by Ppg_DisableTimerGen1StartTrig().

boolean_t bPpgCh14

1: select Ch.14, 0: not selected

Definition at line 337 of file ppg.h.

Referenced by Ppg_DisableTimerGen1StartTrig().

boolean_t bPpgCh8

1: select Ch.8, 0: not selected

Definition at line 334 of file ppg.h.

Referenced by Ppg_DisableTimerGen1StartTrig().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/ppg/ppg.h