| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Functions
C:/pdl_v10/library/driver/uid/uid.c File Reference
`#include "uid.h"`
Include dependency graph for uid.c:

Go to the source code of this file.

## Functions
en_result_t | Uid_ReadUniqueId (stc_unique_id_t *pstcUniqueId)
| Read Unique ID registers as is.
uint32_t | Uid_ReadUniqueId0 (void)
| Read Unique ID registers 0 and shifts it by 4 (LSB aligned)
uint32_t | Uid_ReadUniqueId1 (void)
| Read Unique ID registers 1 and masks the upper 19 bits to '0'.
uint64_t | Uid_ReadUniqueId64 (void)
| Read Unique ID registers 0 and 1 and merge it LSB aligned to a 64 bit value.

## Detailed Description

A detailed description is available at Unique ID Module description

History:

- 2014-02-06 1.0 Edison Zhang First version.

Definition in file uid.c.