| PDL for FM0+ Version1.0 Peripheral Driverl Library for FM0+

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
stc_clk_intern_data Struct Reference
Clock Functions (CLK)

Datatype for holding internal data needed for CLK. More...

`#include <clk.h>`

## Data Fields
func_ptr_t | pfnPllStabCb
| PLL stabilization callback function pointer.
func_ptr_t | pfnScoStabCb
| Sub Clock stabilization callback function pointer.
func_ptr_t | pfnMcoStabCb
| Main Clock stabilization callback function pointer.

## Detailed Description

Datatype for holding internal data needed for CLK.

Definition at line 299 of file clk.h.

## Field Documentation

func_ptr_t pfnMcoStabCb

Main Clock stabilization callback function pointer.

Definition at line 303 of file clk.h.

Referenced by Clk_Init(), and Clk_IrqHandler().

func_ptr_t pfnPllStabCb

PLL stabilization callback function pointer.

Definition at line 301 of file clk.h.

Referenced by Clk_Init(), and Clk_IrqHandler().

func_ptr_t pfnScoStabCb

Sub Clock stabilization callback function pointer.

Definition at line 302 of file clk.h.

Referenced by Clk_Init(), and Clk_IrqHandler().

The documentation for this struct was generated from the following file:

- C:/pdl_v10/library/driver/clk/clk.h